--- a/arch/arm/mach-kirkwood/Makefile
+++ b/arch/arm/mach-kirkwood/Makefile
@@ -8,6 +8,7 @@ obj-$(CONFIG_MACH_SHEEVAPLUG)		+= sheeva
 obj-$(CONFIG_MACH_ESATA_SHEEVAPLUG)	+= sheevaplug-setup.o
 obj-$(CONFIG_MACH_GURUPLUG)		+= guruplug-setup.o
 obj-$(CONFIG_MACH_DOCKSTAR)		+= dockstar-setup.o
+obj-$(CONFIG_MACH_ICONNECT)		+= iconnect-setup.o
 obj-$(CONFIG_MACH_TS219)		+= ts219-setup.o tsx1x-common.o
 obj-$(CONFIG_MACH_TS41X)		+= ts41x-setup.o tsx1x-common.o
 obj-$(CONFIG_MACH_OPENRD)		+= openrd-setup.o
--- a/arch/arm/mach-kirkwood/Kconfig
+++ b/arch/arm/mach-kirkwood/Kconfig
@@ -130,6 +130,12 @@ config MACH_T5325
 	  Say 'Y' here if you want your kernel to support the
 	  HP t5325 Thin Client.
 
+config MACH_ICONNECT
+	bool "Iomega iConnect Wireless"
+	help
+	  Say 'Y' here if you want your kernel to support the
+	  Iomega iConnect Wireless.
+
 endmenu
 
 endif
--- a/arch/arm/mach-kirkwood/mpp.h
+++ b/arch/arm/mach-kirkwood/mpp.h
@@ -108,6 +108,7 @@
 #define MPP11_SATA0_ACTn	MPP( 11, 0x5, 0, 1, 0,   1,   1,   1,   1 )
 
 #define MPP12_GPO		MPP( 12, 0x0, 0, 1, 1,   1,   1,   1,   1 )
+#define MPP12_GPIO		MPP( 12, 0x0, 1, 1, 1,   1,   1,   1,   1 )
 #define MPP12_SD_CLK		MPP( 12, 0x1, 0, 1, 1,   1,   1,   1,   1 )
 #define MPP12_AU_SPDIF0		MPP( 12, 0xa, 0, 1, 0,   0,   0,   0,   1 )
 #define MPP12_SPI_MOSI		MPP( 12, 0xb, 0, 1, 0,   0,   0,   0,   1 )
--- /dev/null
+++ b/arch/arm/mach-kirkwood/iconnect-setup.c
@@ -0,0 +1,188 @@
+/*
+ * arch/arm/mach-kirkwood/iconnect-setup.c
+ *
+ * Iomega iConnect Wireless
+ *
+ * This file is licensed under the terms of the GNU General Public
+ * License version 2.  This program is licensed "as is" without any
+ * warranty of any kind, whether express or implied.
+ */
+
+#include <linux/kernel.h>
+#include <linux/init.h>
+#include <linux/platform_device.h>
+#include <linux/irq.h>
+#include <linux/mtd/partitions.h>
+#include <linux/mv643xx_eth.h>
+#include <linux/ethtool.h>
+#include <linux/gpio.h>
+#include <linux/gpio_keys.h>
+#include <linux/input.h>
+#include <linux/leds.h>
+#include <asm/mach-types.h>
+#include <asm/mach/arch.h>
+#include <mach/kirkwood.h>
+#include "common.h"
+#include "mpp.h"
+
+static struct mtd_partition iconnect_nand_parts[] = {
+	{
+		.name = "u-boot",
+		.offset = 0,
+		.size = SZ_1M
+	}, {
+		.name = "uImage",
+		.offset = MTDPART_OFS_NXTBLK,
+		.size = SZ_1M + SZ_2M
+	}, {
+		.name = "rootfs",
+		.offset = MTDPART_OFS_NXTBLK,
+		.size = SZ_32M,
+	}, {
+		.name = "data",
+		.offset = MTDPART_OFS_NXTBLK,
+		.size = MTDPART_SIZ_FULL
+	},
+};
+
+static struct mv643xx_eth_platform_data iconnect_ge00_data = {
+	.phy_addr	= MV643XX_ETH_PHY_ADDR(11),
+};
+
+static struct gpio_led iconnect_led_pins[] = {
+	{
+		.name			= "iconnect:blue:power",
+		.default_trigger	= "default-on",
+		.gpio			= 42,
+	},
+	{
+		.name			= "iconnect:red:power",
+		.gpio			= 43,
+	},
+	{
+		.name			= "iconnect:blue:usb1",
+		.gpio			= 44,
+	},
+	{
+		.name			= "iconnect:blue:usb2",
+		.gpio			= 45,
+	},
+	{
+		.name			= "iconnect:blue:usb3",
+		.gpio			= 46,
+	},
+	{
+		.name			= "iconnect:blue:usb4",
+		.gpio			= 47,
+	},
+	{
+		.name			= "iconnect:blue:otb",
+		.gpio			= 48,
+	},
+};
+
+static struct gpio_led_platform_data iconnect_led_data = {
+	.leds		= iconnect_led_pins,
+	.num_leds	= ARRAY_SIZE(iconnect_led_pins),
+};
+
+static struct platform_device iconnect_leds = {
+	.name	= "leds-gpio",
+	.id	= -1,
+	.dev	= {
+		.platform_data	= &iconnect_led_data,
+	}
+};
+
+#define ICONNECT_GPIO_KEY_RESET		12
+#define ICONNECT_GPIO_KEY_OTB		35
+
+#define ICONNECT_SW_RESET		0x00
+#define ICONNECT_SW_OTB			0x01
+
+static struct gpio_keys_button iconnect_buttons[] = {
+		{
+		.type		= EV_SW,
+		.code		= ICONNECT_SW_RESET,
+		.gpio		= ICONNECT_GPIO_KEY_RESET,
+		.desc		= "Reset Button",
+		.active_low	= 1,
+		.debounce_interval = 100,
+		}, 
+		{
+		.type		= EV_SW,
+		.code		= ICONNECT_SW_OTB,
+		.gpio		= ICONNECT_GPIO_KEY_OTB,
+		.desc		= "OTB Button",
+		.active_low	= 1,
+		.debounce_interval = 100,
+		},
+};
+
+static struct gpio_keys_platform_data iconnect_button_data = {
+	.buttons	= iconnect_buttons,
+	.nbuttons	= ARRAY_SIZE(iconnect_buttons),
+};
+
+static struct platform_device iconnect_button_device = {
+	.name	   = "gpio-keys",
+	.id	     = -1,
+	.num_resources	= 0,
+	.dev	    =	{
+					.platform_data  = &iconnect_button_data,
+					},
+};
+
+static unsigned int iconnect_mpp_config[] __initdata = {
+	MPP12_GPIO, /*Input for reset button*/
+	MPP35_GPIO, /*Input for OTB button*/
+	MPP42_GPIO,
+	MPP43_GPIO,
+	MPP44_GPIO,
+	MPP45_GPIO,
+	MPP46_GPIO,
+	MPP47_GPIO,
+	MPP48_GPIO,
+	0
+};
+
+static void __init iconnect_init(void)
+{
+	u32 dev, rev;
+
+	/*
+	 * Basic setup. Needs to be called early.
+	 */
+	kirkwood_init();
+	kirkwood_mpp_conf(iconnect_mpp_config);
+
+	kirkwood_nand_init(ARRAY_AND_SIZE(iconnect_nand_parts), 25);
+	kirkwood_ehci_init();
+
+	kirkwood_ge00_init(&iconnect_ge00_data);
+	kirkwood_pcie_id(&dev, &rev);
+
+	kirkwood_uart0_init();
+	kirkwood_i2c_init();
+
+	platform_device_register(&iconnect_leds);
+	platform_device_register(&iconnect_button_device);
+}
+
+static int __init iconnect_pci_init(void)
+{
+	if (machine_is_iconnect())
+		kirkwood_pcie_init(KW_PCIE0);
+
+	return 0;
+}
+subsys_initcall(iconnect_pci_init);
+
+
+MACHINE_START(ICONNECT, "Iomega iConnect Wireless")
+	.boot_params	= 0x00000100,
+	.init_machine	= iconnect_init,
+	.map_io		= kirkwood_map_io,
+	.init_irq	= kirkwood_init_irq,
+	.timer		= &kirkwood_timer,
+MACHINE_END
