--- a/net/mac80211/sta_info.h
+++ b/net/mac80211/sta_info.h
@@ -31,7 +31,6 @@
  *	frames.
  * @WLAN_STA_ASSOC_AP: We're associated to that station, it is an AP.
  * @WLAN_STA_WME: Station is a QoS-STA.
- * @WLAN_STA_WDS: Station is one of our WDS peers.
  * @WLAN_STA_CLEAR_PS_FILT: Clear PS filter in hardware (using the
  *	IEEE80211_TX_CTL_CLEAR_PS_FILT control flag) when the next
  *	frame to this station is transmitted.
@@ -54,7 +53,6 @@ enum ieee80211_sta_info_flags {
 	WLAN_STA_SHORT_PREAMBLE	= 1<<4,
 	WLAN_STA_ASSOC_AP	= 1<<5,
 	WLAN_STA_WME		= 1<<6,
-	WLAN_STA_WDS		= 1<<7,
 	WLAN_STA_CLEAR_PS_FILT	= 1<<9,
 	WLAN_STA_MFP		= 1<<10,
 	WLAN_STA_BLOCK_BA	= 1<<11,
--- a/net/mac80211/debugfs_sta.c
+++ b/net/mac80211/debugfs_sta.c
@@ -59,7 +59,7 @@ static ssize_t sta_flags_read(struct fil
 	char buf[100];
 	struct sta_info *sta = file->private_data;
 	u32 staflags = get_sta_flags(sta);
-	int res = scnprintf(buf, sizeof(buf), "%s%s%s%s%s%s%s%s%s",
+	int res = scnprintf(buf, sizeof(buf), "%s%s%s%s%s%s%s%s",
 		staflags & WLAN_STA_AUTH ? "AUTH\n" : "",
 		staflags & WLAN_STA_ASSOC ? "ASSOC\n" : "",
 		staflags & WLAN_STA_PS_STA ? "PS (sta)\n" : "",
@@ -67,7 +67,6 @@ static ssize_t sta_flags_read(struct fil
 		staflags & WLAN_STA_AUTHORIZED ? "AUTHORIZED\n" : "",
 		staflags & WLAN_STA_SHORT_PREAMBLE ? "SHORT PREAMBLE\n" : "",
 		staflags & WLAN_STA_WME ? "WME\n" : "",
-		staflags & WLAN_STA_WDS ? "WDS\n" : "",
 		staflags & WLAN_STA_MFP ? "MFP\n" : "");
 	return simple_read_from_buffer(userbuf, count, ppos, buf, res);
 }
