From 6bbab54ef3cbfc340a3d3ffdcb0aa47bb4c29de9 Mon Sep 17 00:00:00 2001
From: Lars-Peter Clausen <lars@metafoo.de>
Date: Thu, 11 Nov 2010 19:05:40 +0100
Subject: [PATCH 22/23] MIPS: JZ4740: Set nand ecc offsets for the qi_lb60 board

Now that the mtd core supports more then 64 ecc bytes we can use it instead of
some a custom hack in the jz4740 nand driver.
This patches sets the ecc pos fields of the ecc_layout of the qi_lb60 board.

Signed-off-by: Lars-Peter Clausen <lars@metafoo.de>
---
 arch/mips/jz4740/board-qi_lb60.c |    8 ++++----
 1 files changed, 4 insertions(+), 4 deletions(-)

--- a/arch/mips/jz4740/board-qi_lb60.c
+++ b/arch/mips/jz4740/board-qi_lb60.c
@@ -50,14 +50,14 @@ static bool is_avt2;
 
 /* NAND */
 static struct nand_ecclayout qi_lb60_ecclayout_1gb = {
-/*	.eccbytes = 36,
+	.eccbytes = 36,
 	.eccpos = {
 		6,  7,  8,  9,  10, 11, 12, 13,
 		14, 15, 16, 17, 18, 19, 20, 21,
 		22, 23, 24, 25, 26, 27, 28, 29,
 		30, 31, 32, 33, 34, 35, 36, 37,
 		38, 39, 40, 41
-	},*/
+	},
 	.oobfree = {
 		{ .offset = 2, .length = 4 },
 		{ .offset = 42, .length = 22 }
@@ -86,7 +86,7 @@ static struct mtd_partition qi_lb60_part
 };
 
 static struct nand_ecclayout qi_lb60_ecclayout_2gb = {
-/*	.eccbytes = 72,
+	.eccbytes = 72,
 	.eccpos = {
 		12, 13, 14, 15, 16, 17, 18, 19,
 		20, 21, 22, 23, 24, 25, 26, 27,
@@ -97,7 +97,7 @@ static struct nand_ecclayout qi_lb60_ecc
 		60, 61, 62, 63, 64, 65, 66, 67,
 		68, 69, 70, 71, 72, 73, 74, 75,
 		76, 77, 78, 79, 80, 81, 82, 83
-	},*/
+	},
 	.oobfree = {
 		{ .offset = 2, .length = 10 },
 		{ .offset = 84, .length = 44 },
