--- a/drivers/usb/host/ehci-hub.c
+++ b/drivers/usb/host/ehci-hub.c
@@ -883,11 +883,13 @@ static int ehci_hub_control (
 			 * power switching; they're allowed to just limit the
 			 * current.  khubd will turn the power back on.
 			 */
+#ifndef CONFIG_BCM63XX
 			if (HCS_PPC (ehci->hcs_params)){
 				ehci_writel(ehci,
 					temp & ~(PORT_RWC_BITS | PORT_POWER),
 					status_reg);
 			}
+#endif
 		}
 
 		/* whoever resumes must GetPortStatus to complete it!! */
