--- a/drivers/ssb/main.c
+++ b/drivers/ssb/main.c
@@ -384,6 +384,35 @@ static int ssb_device_uevent(struct devi
 			     ssb_dev->id.revision);
 }
 
+#define ssb_config_attr(attrib, field, format_string) \
+static ssize_t \
+attrib##_show(struct device *dev, struct device_attribute *attr, char *buf) \
+{ \
+	return sprintf(buf, format_string, dev_to_ssb_dev(dev)->field); \
+}
+
+ssb_config_attr(core_num, core_index, "%u\n")
+ssb_config_attr(coreid, id.coreid, "0x%04x\n")
+ssb_config_attr(vendor, id.vendor, "0x%04x\n")
+ssb_config_attr(revision, id.revision, "%u\n")
+ssb_config_attr(irq, irq, "%u\n")
+static ssize_t
+name_show(struct device *dev, struct device_attribute *attr, char *buf)
+{
+	return sprintf(buf, "%s\n",
+		       ssb_core_name(dev_to_ssb_dev(dev)->id.coreid));
+}
+
+static struct device_attribute ssb_device_attrs[] = {
+	__ATTR_RO(name),
+	__ATTR_RO(core_num),
+	__ATTR_RO(coreid),
+	__ATTR_RO(vendor),
+	__ATTR_RO(revision),
+	__ATTR_RO(irq),
+	__ATTR_NULL,
+};
+
 static struct bus_type ssb_bustype = {
 	.name		= "ssb",
 	.match		= ssb_bus_match,
@@ -393,6 +422,7 @@ static struct bus_type ssb_bustype = {
 	.suspend	= ssb_device_suspend,
 	.resume		= ssb_device_resume,
 	.uevent		= ssb_device_uevent,
+	.dev_attrs	= ssb_device_attrs,
 };
 
 static void ssb_buses_lock(void)
@@ -1163,10 +1193,10 @@ void ssb_device_enable(struct ssb_device
 }
 EXPORT_SYMBOL(ssb_device_enable);
 
-/* Wait for a bit in a register to get set or unset.
+/* Wait for bitmask in a register to get set or cleared.
  * timeout is in units of ten-microseconds */
-static int ssb_wait_bit(struct ssb_device *dev, u16 reg, u32 bitmask,
-			int timeout, int set)
+static int ssb_wait_bits(struct ssb_device *dev, u16 reg, u32 bitmask,
+			 int timeout, int set)
 {
 	int i;
 	u32 val;
@@ -1174,7 +1204,7 @@ static int ssb_wait_bit(struct ssb_devic
 	for (i = 0; i < timeout; i++) {
 		val = ssb_read32(dev, reg);
 		if (set) {
-			if (val & bitmask)
+			if ((val & bitmask) == bitmask)
 				return 0;
 		} else {
 			if (!(val & bitmask))
@@ -1191,20 +1221,38 @@ static int ssb_wait_bit(struct ssb_devic
 
 void ssb_device_disable(struct ssb_device *dev, u32 core_specific_flags)
 {
-	u32 reject;
+	u32 reject, val;
 
 	if (ssb_read32(dev, SSB_TMSLOW) & SSB_TMSLOW_RESET)
 		return;
 
 	reject = ssb_tmslow_reject_bitmask(dev);
-	ssb_write32(dev, SSB_TMSLOW, reject | SSB_TMSLOW_CLOCK);
-	ssb_wait_bit(dev, SSB_TMSLOW, reject, 1000, 1);
-	ssb_wait_bit(dev, SSB_TMSHIGH, SSB_TMSHIGH_BUSY, 1000, 0);
-	ssb_write32(dev, SSB_TMSLOW,
-		    SSB_TMSLOW_FGC | SSB_TMSLOW_CLOCK |
-		    reject | SSB_TMSLOW_RESET |
-		    core_specific_flags);
-	ssb_flush_tmslow(dev);
+
+	if (ssb_read32(dev, SSB_TMSLOW) & SSB_TMSLOW_CLOCK) {
+		ssb_write32(dev, SSB_TMSLOW, reject | SSB_TMSLOW_CLOCK);
+		ssb_wait_bits(dev, SSB_TMSLOW, reject, 1000, 1);
+		ssb_wait_bits(dev, SSB_TMSHIGH, SSB_TMSHIGH_BUSY, 1000, 0);
+
+		if (ssb_read32(dev, SSB_IDLOW) & SSB_IDLOW_INITIATOR) {
+			val = ssb_read32(dev, SSB_IMSTATE);
+			val |= SSB_IMSTATE_REJECT;
+			ssb_write32(dev, SSB_IMSTATE, val);
+			ssb_wait_bits(dev, SSB_IMSTATE, SSB_IMSTATE_BUSY, 1000,
+				      0);
+		}
+
+		ssb_write32(dev, SSB_TMSLOW,
+			SSB_TMSLOW_FGC | SSB_TMSLOW_CLOCK |
+			reject | SSB_TMSLOW_RESET |
+			core_specific_flags);
+		ssb_flush_tmslow(dev);
+
+		if (ssb_read32(dev, SSB_IDLOW) & SSB_IDLOW_INITIATOR) {
+			val = ssb_read32(dev, SSB_IMSTATE);
+			val &= ~SSB_IMSTATE_REJECT;
+			ssb_write32(dev, SSB_IMSTATE, val);
+		}
+	}
 
 	ssb_write32(dev, SSB_TMSLOW,
 		    reject | SSB_TMSLOW_RESET |
--- a/drivers/ssb/pci.c
+++ b/drivers/ssb/pci.c
@@ -406,6 +406,46 @@ static void sprom_extract_r123(struct ss
 	out->antenna_gain.ghz5.a3 = gain;
 }
 
+/* Revs 4 5 and 8 have partially shared layout */
+static void sprom_extract_r458(struct ssb_sprom *out, const u16 *in)
+{
+	SPEX(txpid2g[0], SSB_SPROM4_TXPID2G01,
+	     SSB_SPROM4_TXPID2G0, SSB_SPROM4_TXPID2G0_SHIFT);
+	SPEX(txpid2g[1], SSB_SPROM4_TXPID2G01,
+	     SSB_SPROM4_TXPID2G1, SSB_SPROM4_TXPID2G1_SHIFT);
+	SPEX(txpid2g[2], SSB_SPROM4_TXPID2G23,
+	     SSB_SPROM4_TXPID2G2, SSB_SPROM4_TXPID2G2_SHIFT);
+	SPEX(txpid2g[3], SSB_SPROM4_TXPID2G23,
+	     SSB_SPROM4_TXPID2G3, SSB_SPROM4_TXPID2G3_SHIFT);
+
+	SPEX(txpid5gl[0], SSB_SPROM4_TXPID5GL01,
+	     SSB_SPROM4_TXPID5GL0, SSB_SPROM4_TXPID5GL0_SHIFT);
+	SPEX(txpid5gl[1], SSB_SPROM4_TXPID5GL01,
+	     SSB_SPROM4_TXPID5GL1, SSB_SPROM4_TXPID5GL1_SHIFT);
+	SPEX(txpid5gl[2], SSB_SPROM4_TXPID5GL23,
+	     SSB_SPROM4_TXPID5GL2, SSB_SPROM4_TXPID5GL2_SHIFT);
+	SPEX(txpid5gl[3], SSB_SPROM4_TXPID5GL23,
+	     SSB_SPROM4_TXPID5GL3, SSB_SPROM4_TXPID5GL3_SHIFT);
+
+	SPEX(txpid5g[0], SSB_SPROM4_TXPID5G01,
+	     SSB_SPROM4_TXPID5G0, SSB_SPROM4_TXPID5G0_SHIFT);
+	SPEX(txpid5g[1], SSB_SPROM4_TXPID5G01,
+	     SSB_SPROM4_TXPID5G1, SSB_SPROM4_TXPID5G1_SHIFT);
+	SPEX(txpid5g[2], SSB_SPROM4_TXPID5G23,
+	     SSB_SPROM4_TXPID5G2, SSB_SPROM4_TXPID5G2_SHIFT);
+	SPEX(txpid5g[3], SSB_SPROM4_TXPID5G23,
+	     SSB_SPROM4_TXPID5G3, SSB_SPROM4_TXPID5G3_SHIFT);
+
+	SPEX(txpid5gh[0], SSB_SPROM4_TXPID5GH01,
+	     SSB_SPROM4_TXPID5GH0, SSB_SPROM4_TXPID5GH0_SHIFT);
+	SPEX(txpid5gh[1], SSB_SPROM4_TXPID5GH01,
+	     SSB_SPROM4_TXPID5GH1, SSB_SPROM4_TXPID5GH1_SHIFT);
+	SPEX(txpid5gh[2], SSB_SPROM4_TXPID5GH23,
+	     SSB_SPROM4_TXPID5GH2, SSB_SPROM4_TXPID5GH2_SHIFT);
+	SPEX(txpid5gh[3], SSB_SPROM4_TXPID5GH23,
+	     SSB_SPROM4_TXPID5GH3, SSB_SPROM4_TXPID5GH3_SHIFT);
+}
+
 static void sprom_extract_r45(struct ssb_sprom *out, const u16 *in)
 {
 	int i;
@@ -428,10 +468,14 @@ static void sprom_extract_r45(struct ssb
 		SPEX(country_code, SSB_SPROM4_CCODE, 0xFFFF, 0);
 		SPEX(boardflags_lo, SSB_SPROM4_BFLLO, 0xFFFF, 0);
 		SPEX(boardflags_hi, SSB_SPROM4_BFLHI, 0xFFFF, 0);
+		SPEX(boardflags2_lo, SSB_SPROM4_BFL2LO, 0xFFFF, 0);
+		SPEX(boardflags2_hi, SSB_SPROM4_BFL2HI, 0xFFFF, 0);
 	} else {
 		SPEX(country_code, SSB_SPROM5_CCODE, 0xFFFF, 0);
 		SPEX(boardflags_lo, SSB_SPROM5_BFLLO, 0xFFFF, 0);
 		SPEX(boardflags_hi, SSB_SPROM5_BFLHI, 0xFFFF, 0);
+		SPEX(boardflags2_lo, SSB_SPROM5_BFL2LO, 0xFFFF, 0);
+		SPEX(boardflags2_hi, SSB_SPROM5_BFL2HI, 0xFFFF, 0);
 	}
 	SPEX(ant_available_a, SSB_SPROM4_ANTAVAIL, SSB_SPROM4_ANTAVAIL_A,
 	     SSB_SPROM4_ANTAVAIL_A_SHIFT);
@@ -471,6 +515,8 @@ static void sprom_extract_r45(struct ssb
 	memcpy(&out->antenna_gain.ghz5, &out->antenna_gain.ghz24,
 	       sizeof(out->antenna_gain.ghz5));
 
+	sprom_extract_r458(out, in);
+
 	/* TODO - get remaining rev 4 stuff needed */
 }
 
@@ -561,6 +607,8 @@ static void sprom_extract_r8(struct ssb_
 	memcpy(&out->antenna_gain.ghz5, &out->antenna_gain.ghz24,
 	       sizeof(out->antenna_gain.ghz5));
 
+	sprom_extract_r458(out, in);
+
 	/* TODO - get remaining rev 8 stuff needed */
 }
 
@@ -573,37 +621,34 @@ static int sprom_extract(struct ssb_bus
 	ssb_dprintk(KERN_DEBUG PFX "SPROM revision %d detected.\n", out->revision);
 	memset(out->et0mac, 0xFF, 6);		/* preset et0 and et1 mac */
 	memset(out->et1mac, 0xFF, 6);
+
 	if ((bus->chip_id & 0xFF00) == 0x4400) {
 		/* Workaround: The BCM44XX chip has a stupid revision
 		 * number stored in the SPROM.
 		 * Always extract r1. */
 		out->revision = 1;
+		ssb_dprintk(KERN_DEBUG PFX "SPROM treated as revision %d\n", out->revision);
+	}
+
+	switch (out->revision) {
+	case 1:
+	case 2:
+	case 3:
 		sprom_extract_r123(out, in);
-	} else if (bus->chip_id == 0x4321) {
-		/* the BCM4328 has a chipid == 0x4321 and a rev 4 SPROM */
-		out->revision = 4;
+		break;
+	case 4:
+	case 5:
 		sprom_extract_r45(out, in);
-	} else {
-		switch (out->revision) {
-		case 1:
-		case 2:
-		case 3:
-			sprom_extract_r123(out, in);
-			break;
-		case 4:
-		case 5:
-			sprom_extract_r45(out, in);
-			break;
-		case 8:
-			sprom_extract_r8(out, in);
-			break;
-		default:
-			ssb_printk(KERN_WARNING PFX "Unsupported SPROM"
-				   "  revision %d detected. Will extract"
-				   " v1\n", out->revision);
-			out->revision = 1;
-			sprom_extract_r123(out, in);
-		}
+		break;
+	case 8:
+		sprom_extract_r8(out, in);
+		break;
+	default:
+		ssb_printk(KERN_WARNING PFX "Unsupported SPROM"
+			   " revision %d detected. Will extract"
+			   " v1\n", out->revision);
+		out->revision = 1;
+		sprom_extract_r123(out, in);
 	}
 
 	if (out->boardflags_lo == 0xFFFF)
@@ -618,7 +663,7 @@ static int ssb_pci_sprom_get(struct ssb_
 			     struct ssb_sprom *sprom)
 {
 	const struct ssb_sprom *fallback;
-	int err = -ENOMEM;
+	int err;
 	u16 *buf;
 
 	if (!ssb_is_sprom_available(bus)) {
@@ -645,7 +690,7 @@ static int ssb_pci_sprom_get(struct ssb_
 
 	buf = kcalloc(SSB_SPROMSIZE_WORDS_R123, sizeof(u16), GFP_KERNEL);
 	if (!buf)
-		goto out;
+		return -ENOMEM;
 	bus->sprom_size = SSB_SPROMSIZE_WORDS_R123;
 	sprom_do_read(bus, buf);
 	err = sprom_check_crc(buf, bus->sprom_size);
@@ -655,7 +700,7 @@ static int ssb_pci_sprom_get(struct ssb_
 		buf = kcalloc(SSB_SPROMSIZE_WORDS_R4, sizeof(u16),
 			      GFP_KERNEL);
 		if (!buf)
-			goto out;
+			return -ENOMEM;
 		bus->sprom_size = SSB_SPROMSIZE_WORDS_R4;
 		sprom_do_read(bus, buf);
 		err = sprom_check_crc(buf, bus->sprom_size);
@@ -677,7 +722,6 @@ static int ssb_pci_sprom_get(struct ssb_
 
 out_free:
 	kfree(buf);
-out:
 	return err;
 }
 
--- a/drivers/ssb/pcihost_wrapper.c
+++ b/drivers/ssb/pcihost_wrapper.c
@@ -59,6 +59,7 @@ static int ssb_pcihost_probe(struct pci_
 	struct ssb_bus *ssb;
 	int err = -ENOMEM;
 	const char *name;
+	u32 val;
 
 	ssb = kzalloc(sizeof(*ssb), GFP_KERNEL);
 	if (!ssb)
@@ -74,6 +75,12 @@ static int ssb_pcihost_probe(struct pci_
 		goto err_pci_disable;
 	pci_set_master(dev);
 
+	/* Disable the RETRY_TIMEOUT register (0x41) to keep
+	 * PCI Tx retries from interfering with C3 CPU state */
+	pci_read_config_dword(dev, 0x40, &val);
+	if ((val & 0x0000ff00) != 0)
+		pci_write_config_dword(dev, 0x40, val & 0xffff00ff);
+
 	err = ssb_bus_pcibus_register(ssb, dev);
 	if (err)
 		goto err_pci_release_regions;
--- a/drivers/ssb/scan.c
+++ b/drivers/ssb/scan.c
@@ -406,10 +406,10 @@ int ssb_bus_scan(struct ssb_bus *bus,
 				/* Ignore PCI cores on PCI-E cards.
 				 * Ignore PCI-E cores on PCI cards. */
 				if (dev->id.coreid == SSB_DEV_PCI) {
-					if (bus->host_pci->is_pcie)
+					if (pci_is_pcie(bus->host_pci))
 						continue;
 				} else {
-					if (!bus->host_pci->is_pcie)
+					if (!pci_is_pcie(bus->host_pci))
 						continue;
 				}
 			}
@@ -421,6 +421,16 @@ int ssb_bus_scan(struct ssb_bus *bus,
 			bus->pcicore.dev = dev;
 #endif /* CONFIG_SSB_DRIVER_PCICORE */
 			break;
+		case SSB_DEV_ETHERNET:
+			if (bus->bustype == SSB_BUSTYPE_PCI) {
+				if (bus->host_pci->vendor == PCI_VENDOR_ID_BROADCOM &&
+				    (bus->host_pci->device & 0xFF00) == 0x4300) {
+					/* This is a dangling ethernet core on a
+					 * wireless device. Ignore it. */
+					continue;
+				}
+			}
+			break;
 		default:
 			break;
 		}
--- a/include/linux/ssb/ssb.h
+++ b/include/linux/ssb/ssb.h
@@ -55,6 +55,10 @@ struct ssb_sprom {
 	u8 tri5gl;		/* 5.2GHz TX isolation */
 	u8 tri5g;		/* 5.3GHz TX isolation */
 	u8 tri5gh;		/* 5.8GHz TX isolation */
+	u8 txpid2g[4];		/* 2GHz TX power index */
+	u8 txpid5gl[4];		/* 4.9 - 5.1GHz TX power index */
+	u8 txpid5g[4];		/* 5.1 - 5.5GHz TX power index */
+	u8 txpid5gh[4];		/* 5.5 - ...GHz TX power index */
 	u8 rxpo2g;		/* 2GHz RX power offset */
 	u8 rxpo5g;		/* 5GHz RX power offset */
 	u8 rssisav2g;		/* 2GHz RSSI params */
--- a/include/linux/ssb/ssb_driver_gige.h
+++ b/include/linux/ssb/ssb_driver_gige.h
@@ -96,16 +96,21 @@ static inline bool ssb_gige_must_flush_p
 	return 0;
 }
 
-extern char * nvram_get(const char *name);
+#ifdef CONFIG_BCM47XX
+#include <asm/mach-bcm47xx/nvram.h>
 /* Get the device MAC address */
 static inline void ssb_gige_get_macaddr(struct pci_dev *pdev, u8 *macaddr)
 {
-#ifdef CONFIG_BCM47XX
-	char *res = nvram_get("et0macaddr");
-	if (res)
-		memcpy(macaddr, res, 6);
-#endif
+	char buf[20];
+	if (nvram_getenv("et0macaddr", buf, sizeof(buf)) < 0)
+		return;
+	nvram_parse_macaddr(buf, macaddr);
 }
+#else
+static inline void ssb_gige_get_macaddr(struct pci_dev *pdev, u8 *macaddr)
+{
+}
+#endif
 
 extern int ssb_gige_pcibios_plat_dev_init(struct ssb_device *sdev,
 					  struct pci_dev *pdev);
--- a/include/linux/ssb/ssb_regs.h
+++ b/include/linux/ssb/ssb_regs.h
@@ -85,6 +85,8 @@
 #define  SSB_IMSTATE_AP_RSV	0x00000030 /* Reserved */
 #define  SSB_IMSTATE_IBE	0x00020000 /* In Band Error */
 #define  SSB_IMSTATE_TO		0x00040000 /* Timeout */
+#define  SSB_IMSTATE_BUSY	0x01800000 /* Busy (Backplane rev >= 2.3 only) */
+#define  SSB_IMSTATE_REJECT	0x02000000 /* Reject (Backplane rev >= 2.3 only) */
 #define SSB_INTVEC		0x0F94     /* SB Interrupt Mask */
 #define  SSB_INTVEC_PCI		0x00000001 /* Enable interrupts for PCI */
 #define  SSB_INTVEC_ENET0	0x00000002 /* Enable interrupts for enet 0 */
@@ -267,6 +269,8 @@
 /* SPROM Revision 4 */
 #define SSB_SPROM4_BFLLO		0x0044	/* Boardflags (low 16 bits) */
 #define SSB_SPROM4_BFLHI		0x0046  /* Board Flags Hi */
+#define SSB_SPROM4_BFL2LO		0x0048	/* Board flags 2 (low 16 bits) */
+#define SSB_SPROM4_BFL2HI		0x004A	/* Board flags 2 Hi */
 #define SSB_SPROM4_IL0MAC		0x004C	/* 6 byte MAC address for a/b/g/n */
 #define SSB_SPROM4_CCODE		0x0052	/* Country Code (2 bytes) */
 #define SSB_SPROM4_GPIOA		0x0056	/* Gen. Purpose IO # 0 and 1 */
@@ -298,6 +302,46 @@
 #define  SSB_SPROM4_AGAIN2_SHIFT	0
 #define  SSB_SPROM4_AGAIN3		0xFF00	/* Antenna 3 */
 #define  SSB_SPROM4_AGAIN3_SHIFT	8
+#define SSB_SPROM4_TXPID2G01		0x0062 	/* TX Power Index 2GHz */
+#define  SSB_SPROM4_TXPID2G0		0x00FF
+#define  SSB_SPROM4_TXPID2G0_SHIFT	0
+#define  SSB_SPROM4_TXPID2G1		0xFF00
+#define  SSB_SPROM4_TXPID2G1_SHIFT	8
+#define SSB_SPROM4_TXPID2G23		0x0064 	/* TX Power Index 2GHz */
+#define  SSB_SPROM4_TXPID2G2		0x00FF
+#define  SSB_SPROM4_TXPID2G2_SHIFT	0
+#define  SSB_SPROM4_TXPID2G3		0xFF00
+#define  SSB_SPROM4_TXPID2G3_SHIFT	8
+#define SSB_SPROM4_TXPID5G01		0x0066 	/* TX Power Index 5GHz middle subband */
+#define  SSB_SPROM4_TXPID5G0		0x00FF
+#define  SSB_SPROM4_TXPID5G0_SHIFT	0
+#define  SSB_SPROM4_TXPID5G1		0xFF00
+#define  SSB_SPROM4_TXPID5G1_SHIFT	8
+#define SSB_SPROM4_TXPID5G23		0x0068 	/* TX Power Index 5GHz middle subband */
+#define  SSB_SPROM4_TXPID5G2		0x00FF
+#define  SSB_SPROM4_TXPID5G2_SHIFT	0
+#define  SSB_SPROM4_TXPID5G3		0xFF00
+#define  SSB_SPROM4_TXPID5G3_SHIFT	8
+#define SSB_SPROM4_TXPID5GL01		0x006A 	/* TX Power Index 5GHz low subband */
+#define  SSB_SPROM4_TXPID5GL0		0x00FF
+#define  SSB_SPROM4_TXPID5GL0_SHIFT	0
+#define  SSB_SPROM4_TXPID5GL1		0xFF00
+#define  SSB_SPROM4_TXPID5GL1_SHIFT	8
+#define SSB_SPROM4_TXPID5GL23		0x006C 	/* TX Power Index 5GHz low subband */
+#define  SSB_SPROM4_TXPID5GL2		0x00FF
+#define  SSB_SPROM4_TXPID5GL2_SHIFT	0
+#define  SSB_SPROM4_TXPID5GL3		0xFF00
+#define  SSB_SPROM4_TXPID5GL3_SHIFT	8
+#define SSB_SPROM4_TXPID5GH01		0x006E 	/* TX Power Index 5GHz high subband */
+#define  SSB_SPROM4_TXPID5GH0		0x00FF
+#define  SSB_SPROM4_TXPID5GH0_SHIFT	0
+#define  SSB_SPROM4_TXPID5GH1		0xFF00
+#define  SSB_SPROM4_TXPID5GH1_SHIFT	8
+#define SSB_SPROM4_TXPID5GH23		0x0070 	/* TX Power Index 5GHz high subband */
+#define  SSB_SPROM4_TXPID5GH2		0x00FF
+#define  SSB_SPROM4_TXPID5GH2_SHIFT	0
+#define  SSB_SPROM4_TXPID5GH3		0xFF00
+#define  SSB_SPROM4_TXPID5GH3_SHIFT	8
 #define SSB_SPROM4_MAXP_BG		0x0080  /* Max Power BG in path 1 */
 #define  SSB_SPROM4_MAXP_BG_MASK	0x00FF  /* Mask for Max Power BG */
 #define  SSB_SPROM4_ITSSI_BG		0xFF00	/* Mask for path 1 itssi_bg */
@@ -317,6 +361,8 @@
 #define SSB_SPROM5_CCODE		0x0044	/* Country Code (2 bytes) */
 #define SSB_SPROM5_BFLLO		0x004A	/* Boardflags (low 16 bits) */
 #define SSB_SPROM5_BFLHI		0x004C  /* Board Flags Hi */
+#define SSB_SPROM5_BFL2LO		0x004E	/* Board flags 2 (low 16 bits) */
+#define SSB_SPROM5_BFL2HI		0x0050	/* Board flags 2 Hi */
 #define SSB_SPROM5_IL0MAC		0x0052	/* 6 byte MAC address for a/b/g/n */
 #define SSB_SPROM5_GPIOA		0x0076	/* Gen. Purpose IO # 0 and 1 */
 #define  SSB_SPROM5_GPIOA_P0		0x00FF	/* Pin 0 */
