--- a/drivers/net/wireless/ath/ath9k/debug.c
+++ b/drivers/net/wireless/ath/ath9k/debug.c
@@ -548,6 +548,7 @@ static ssize_t read_file_xmit(struct fil
 
 	PR("MPDUs Queued:    ", queued);
 	PR("MPDUs Completed: ", completed);
+	PR("MPDUs XRetried:  ", xretries);
 	PR("Aggregates:      ", a_aggr);
 	PR("AMPDUs Queued HW:", a_queued_hw);
 	PR("AMPDUs Queued SW:", a_queued_sw);
@@ -803,7 +804,10 @@ void ath_debug_stat_tx(struct ath_softc 
 		else
 			TX_STAT_INC(qnum, a_completed);
 	} else {
-		TX_STAT_INC(qnum, completed);
+		if (bf_isxretried(bf))
+			TX_STAT_INC(qnum, xretries);
+		else
+			TX_STAT_INC(qnum, completed);
 	}
 
 	if (ts->ts_status & ATH9K_TXERR_FIFO)
--- a/drivers/net/wireless/ath/ath9k/debug.h
+++ b/drivers/net/wireless/ath/ath9k/debug.h
@@ -116,6 +116,7 @@ struct ath_tx_stats {
 	u32 tx_bytes_all;
 	u32 queued;
 	u32 completed;
+	u32 xretries;
 	u32 a_aggr;
 	u32 a_queued_hw;
 	u32 a_queued_sw;
