From 5cd5a44b94b451ecaf593bb49919cfbb51ccb622 Mon Sep 17 00:00:00 2001
From: Lars-Peter Clausen <lars@metafoo.de>
Date: Sat, 17 Jul 2010 11:12:20 +0000
Subject: [PATCH] MIPS: JZ4740: Add PWM support

Add support for the PWM part of the timer unit on a JZ4740 SoC.

Signed-off-by: Lars-Peter Clausen <lars@metafoo.de>
Cc: linux-mips@linux-mips.org
Cc: linux-kernel@vger.kernel.org
Patchwork: https://patchwork.linux-mips.org/patch/1468/
Signed-off-by: Ralf Baechle <ralf@linux-mips.org>
---
 arch/mips/jz4740/pwm.c |  177 ++++++++++++++++++++++++++++++++++++++++++++++++
 1 files changed, 177 insertions(+), 0 deletions(-)
 create mode 100644 arch/mips/jz4740/pwm.c

--- /dev/null
+++ b/arch/mips/jz4740/pwm.c
@@ -0,0 +1,177 @@
+/*
+ *  Copyright (C) 2010, Lars-Peter Clausen <lars@metafoo.de>
+ *  JZ4740 platform PWM support
+ *
+ *  This program is free software; you can redistribute it and/or modify it
+ *  under  the terms of the GNU General  Public License as published by the
+ *  Free Software Foundation;  either version 2 of the License, or (at your
+ *  option) any later version.
+ *
+ *  You should have received a copy of the GNU General Public License along
+ *  with this program; if not, write to the Free Software Foundation, Inc.,
+ *  675 Mass Ave, Cambridge, MA 02139, USA.
+ *
+ */
+
+#include <linux/kernel.h>
+
+#include <linux/clk.h>
+#include <linux/err.h>
+#include <linux/pwm.h>
+#include <linux/gpio.h>
+
+#include <asm/mach-jz4740/gpio.h>
+#include "timer.h"
+
+static struct clk *jz4740_pwm_clk;
+
+DEFINE_MUTEX(jz4740_pwm_mutex);
+
+struct pwm_device {
+	unsigned int id;
+	unsigned int gpio;
+	bool used;
+};
+
+static struct pwm_device jz4740_pwm_list[] = {
+	{ 2, JZ_GPIO_PWM2, false },
+	{ 3, JZ_GPIO_PWM3, false },
+	{ 4, JZ_GPIO_PWM4, false },
+	{ 5, JZ_GPIO_PWM5, false },
+	{ 6, JZ_GPIO_PWM6, false },
+	{ 7, JZ_GPIO_PWM7, false },
+};
+
+struct pwm_device *pwm_request(int id, const char *label)
+{
+	int ret = 0;
+	struct pwm_device *pwm;
+
+	if (id < 2 || id > 7 || !jz4740_pwm_clk)
+		return ERR_PTR(-ENODEV);
+
+	mutex_lock(&jz4740_pwm_mutex);
+
+	pwm = &jz4740_pwm_list[id - 2];
+	if (pwm->used)
+		ret = -EBUSY;
+	else
+		pwm->used = true;
+
+	mutex_unlock(&jz4740_pwm_mutex);
+
+	if (ret)
+		return ERR_PTR(ret);
+
+	ret = gpio_request(pwm->gpio, label);
+
+	if (ret) {
+		printk(KERN_ERR "Failed to request pwm gpio: %d\n", ret);
+		pwm->used = false;
+		return ERR_PTR(ret);
+	}
+
+	jz_gpio_set_function(pwm->gpio, JZ_GPIO_FUNC_PWM);
+
+	jz4740_timer_start(id);
+
+	return pwm;
+}
+
+void pwm_free(struct pwm_device *pwm)
+{
+	pwm_disable(pwm);
+	jz4740_timer_set_ctrl(pwm->id, 0);
+
+	jz_gpio_set_function(pwm->gpio, JZ_GPIO_FUNC_NONE);
+	gpio_free(pwm->gpio);
+
+	jz4740_timer_stop(pwm->id);
+
+	pwm->used = false;
+}
+
+int pwm_config(struct pwm_device *pwm, int duty_ns, int period_ns)
+{
+	unsigned long long tmp;
+	unsigned long period, duty;
+	unsigned int prescaler = 0;
+	unsigned int id = pwm->id;
+	uint16_t ctrl;
+	bool is_enabled;
+
+	if (duty_ns < 0 || duty_ns > period_ns)
+		return -EINVAL;
+
+	tmp = (unsigned long long)clk_get_rate(jz4740_pwm_clk) * period_ns;
+	do_div(tmp, 1000000000);
+	period = tmp;
+
+	while (period > 0xffff && prescaler < 6) {
+		period >>= 2;
+		++prescaler;
+	}
+
+	if (prescaler == 6)
+		return -EINVAL;
+
+	tmp = (unsigned long long)period * duty_ns;
+	do_div(tmp, period_ns);
+	duty = period - tmp;
+
+	if (duty >= period)
+		duty = period - 1;
+
+	is_enabled = jz4740_timer_is_enabled(id);
+	if (is_enabled)
+		pwm_disable(pwm);
+
+	jz4740_timer_set_count(id, 0);
+	jz4740_timer_set_duty(id, duty);
+	jz4740_timer_set_period(id, period);
+
+	ctrl = JZ_TIMER_CTRL_PRESCALER(prescaler) | JZ_TIMER_CTRL_SRC_EXT |
+		JZ_TIMER_CTRL_PWM_ABBRUPT_SHUTDOWN;
+
+	jz4740_timer_set_ctrl(id, ctrl);
+
+	if (is_enabled)
+		pwm_enable(pwm);
+
+	return 0;
+}
+
+int pwm_enable(struct pwm_device *pwm)
+{
+	uint32_t ctrl = jz4740_timer_get_ctrl(pwm->id);
+
+	ctrl |= JZ_TIMER_CTRL_PWM_ENABLE;
+	jz4740_timer_set_ctrl(pwm->id, ctrl);
+	jz4740_timer_enable(pwm->id);
+
+	return 0;
+}
+
+void pwm_disable(struct pwm_device *pwm)
+{
+	uint32_t ctrl = jz4740_timer_get_ctrl(pwm->id);
+
+	ctrl &= ~JZ_TIMER_CTRL_PWM_ENABLE;
+	jz4740_timer_disable(pwm->id);
+	jz4740_timer_set_ctrl(pwm->id, ctrl);
+}
+
+static int __init jz4740_pwm_init(void)
+{
+	int ret = 0;
+
+	jz4740_pwm_clk = clk_get(NULL, "ext");
+
+	if (IS_ERR(jz4740_pwm_clk)) {
+		ret = PTR_ERR(jz4740_pwm_clk);
+		jz4740_pwm_clk = NULL;
+	}
+
+	return ret;
+}
+subsys_initcall(jz4740_pwm_init);
