From eb15b4f5046dbb1a530ec3e6134b1b68753e1f31 Mon Sep 17 00:00:00 2001
From: Lars-Peter Clausen <lars@metafoo.de>
Date: Sat, 24 Apr 2010 17:24:26 +0200
Subject: [PATCH] Add qi_lb60 board support

---
 arch/mips/include/asm/mach-jz4740/board-qi_lb60.h |   51 +++
 arch/mips/jz4740/Kconfig                          |    4 +
 arch/mips/jz4740/Makefile                         |    2 +
 arch/mips/jz4740/board-qi_lb60.c                  |  486 +++++++++++++++++++++
 4 files changed, 543 insertions(+), 0 deletions(-)
 create mode 100644 arch/mips/include/asm/mach-jz4740/board-qi_lb60.h
 create mode 100644 arch/mips/jz4740/board-qi_lb60.c

diff --git a/arch/mips/include/asm/mach-jz4740/board-qi_lb60.h b/arch/mips/include/asm/mach-jz4740/board-qi_lb60.h
new file mode 100644
index 0000000..cfbf073
--- /dev/null
+++ b/arch/mips/include/asm/mach-jz4740/board-qi_lb60.h
@@ -0,0 +1,51 @@
+/*
+ * Copyright (c) 2009 Qi Hardware Inc.,
+ * Author: Xiangfu Liu <xiangfu@qi-hardware.com>
+ *
+ * This program is free software: you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation, either version 3 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program.  If not, see <http://www.gnu.org/licenses/>.
+ */
+
+#ifndef __ASM_JZ4740_QI_LB60_H__
+#define __ASM_JZ4740_QI_LB60_H__
+
+#include <linux/gpio.h>
+
+/*
+ * GPIO
+ */
+#define GPIO_DC_DETE_N          JZ_GPIO_PORTC(26)
+#define GPIO_CHARG_STAT_N       JZ_GPIO_PORTC(27)
+#define GPIO_LED_EN             JZ_GPIO_PORTC(28)
+#define GPIO_LCD_CS             JZ_GPIO_PORTC(21)
+#define GPIO_DISP_OFF_N         JZ_GPIO_PORTD(21)
+#define GPIO_PWM                JZ_GPIO_PORTD(27)
+#define GPIO_WAKEUP_N           JZ_GPIO_PORTD(29)
+
+#define GPIO_AMP_EN             JZ_GPIO_PORTD(4)
+
+#define GPIO_SD_CD_N            JZ_GPIO_PORTD(0)
+#define GPIO_SD_VCC_EN_N        JZ_GPIO_PORTD(2)
+
+#define GPIO_USB_DETE           JZ_GPIO_PORTD(28)
+#define GPIO_BUZZ_PWM           JZ_GPIO_PORTD(27)
+#define GPIO_UDC_HOTPLUG        GPIO_USB_DETE
+
+#define GPIO_AUDIO_POP          JZ_GPIO_PORTB(29)
+#define GPIO_COB_TEST           JZ_GPIO_PORTB(30)
+
+#define GPIO_KEYOUT_BASE        JZ_GPIO_PORTC(10)
+#define GPIO_KEYIN_BASE         JZ_GPIO_PORTD(18)
+#define GPIO_KEYIN_8            JZ_GPIO_PORTD(26)
+
+#endif /* __ASM_JZ4740_QI_LB60_H__ */
diff --git a/arch/mips/jz4740/Kconfig b/arch/mips/jz4740/Kconfig
index b959769..a255c1a 100644
--- a/arch/mips/jz4740/Kconfig
+++ b/arch/mips/jz4740/Kconfig
@@ -3,6 +3,10 @@ choice
 	depends on MACH_JZ
 	default JZ4740_QI_LB60
 
+config JZ4740_QI_LB60
+	bool "Qi Hardware Ben NanoNote"
+	select SOC_JZ4740
+
 endchoice
 
 config HAVE_PWM
diff --git a/arch/mips/jz4740/Makefile b/arch/mips/jz4740/Makefile
index 398ee91..dd27b49 100644
--- a/arch/mips/jz4740/Makefile
+++ b/arch/mips/jz4740/Makefile
@@ -11,6 +11,8 @@ obj-$(CONFIG_DEBUG_FS) += clock-debugfs.o
 
 # board specific support
 
+obj-$(CONFIG_JZ4740_QI_LB60)	+= board-qi_lb60.o
+
 # PM support
 
 obj-$(CONFIG_PM) += pm.o
diff --git a/arch/mips/jz4740/board-qi_lb60.c b/arch/mips/jz4740/board-qi_lb60.c
new file mode 100644
index 0000000..b3cc308
--- /dev/null
+++ b/arch/mips/jz4740/board-qi_lb60.c
@@ -0,0 +1,486 @@
+/*
+ * linux/arch/mips/jz4740/board-qi_lb60.c
+ *
+ * QI_LB60 setup routines.
+ *
+ * Copyright (c) 2009 Qi Hardware inc.,
+ * Author: Xiangfu Liu <xiangfu@qi-hardware.com>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 or later
+ * as published by the Free Software Foundation.
+ */
+
+#include <linux/kernel.h>
+#include <linux/init.h>
+#include <linux/gpio.h>
+
+#include <asm/mach-jz4740/board-qi_lb60.h>
+#include <asm/mach-jz4740/platform.h>
+
+#include <linux/input.h>
+#include <linux/gpio_keys.h>
+#include <linux/mtd/jz4740_nand.h>
+#include <linux/jz4740_fb.h>
+#include <linux/input/matrix_keypad.h>
+#include <linux/mtd/jz4740_nand.h>
+#include <linux/spi/spi.h>
+#include <linux/spi/spi_gpio.h>
+#include <linux/power_supply.h>
+#include <linux/power/jz4740-battery.h>
+#include <linux/power/gpio-charger.h>
+#include <linux/mmc/jz4740_mmc.h>
+
+#include <linux/regulator/fixed.h>
+#include <linux/regulator/machine.h>
+
+#include <linux/leds_pwm.h>
+
+#include "clock.h"
+
+static bool is_avt2;
+
+/* NAND */
+static struct nand_ecclayout qi_lb60_ecclayout_1gb = {
+	.eccbytes = 36,
+	.eccpos = {
+		6,  7,  8,  9,  10, 11, 12, 13,
+		14, 15, 16, 17, 18, 19, 20, 21,
+		22, 23, 24, 25, 26, 27, 28, 29,
+		30, 31, 32, 33, 34, 35, 36, 37,
+		38, 39, 40, 41},
+	.oobfree = {
+		{.offset = 2,
+		 .length = 4},
+		{.offset = 42,
+		 .length = 22}}
+};
+
+static struct mtd_partition qi_lb60_partitions_1gb[] = {
+	{ .name = "NAND BOOT partition",
+	  .offset = 0 * 0x100000,
+	  .size = 4 * 0x100000,
+ 	},
+	{ .name = "NAND KERNEL partition",
+	  .offset = 4 * 0x100000,
+	  .size = 4 * 0x100000,
+ 	},
+	{ .name = "NAND ROOTFS partition",
+	  .offset = 8 * 0x100000,
+	  .size = (504 + 512) * 0x100000,
+ 	},
+};
+
+static struct nand_ecclayout qi_lb60_ecclayout_2gb = {
+	.eccbytes = 72,
+	.eccpos = {
+		12, 13, 14, 15, 16, 17, 18, 19,
+		20, 21, 22, 23, 24, 25, 26, 27,
+		28, 29, 30, 31, 32, 33, 34, 35,
+		36, 37, 38, 39, 40, 41, 42, 43,
+		44, 45, 46, 47, 48, 49, 50, 51,
+		52, 53, 54, 55, 56, 57, 58, 59,
+		60, 61, 62, 63, 64, 65, 66, 67,
+		68, 69, 70, 71, 72, 73, 74, 75,
+		76, 77, 78, 79, 80, 81, 82, 83},
+	.oobfree = {
+ 		{ .offset = 2, .length = 10},
+		{ .offset = 84, .length = 44},
+	},
+};
+
+static struct mtd_partition qi_lb60_partitions_2gb[] = {
+	{ .name = "NAND BOOT partition",
+	  .offset = 0 * 0x100000,
+	  .size = 4 * 0x100000,
+ 	},
+	{ .name = "NAND KERNEL partition",
+	  .offset = 4 * 0x100000,
+	  .size = 4 * 0x100000,
+ 	},
+	{ .name = "NAND ROOTFS partition",
+	  .offset = 8 * 0x100000,
+	  .size = (504 + 512 + 1024) * 0x100000,
+ 	},
+};
+
+static void qi_lb60_nand_ident(struct platform_device *pdev,
+		struct nand_chip *chip, struct mtd_partition **partitions,
+		int *num_partitions)
+{
+	if (chip->page_shift == 12) {
+		chip->ecc.layout = &qi_lb60_ecclayout_2gb;
+		*partitions = qi_lb60_partitions_2gb;
+		*num_partitions = ARRAY_SIZE(qi_lb60_partitions_2gb);
+	} else {
+		chip->ecc.layout = &qi_lb60_ecclayout_1gb;
+		*partitions = qi_lb60_partitions_1gb;
+		*num_partitions = ARRAY_SIZE(qi_lb60_partitions_1gb);
+	}
+}
+
+static struct jz_nand_platform_data qi_lb60_nand_pdata = {
+	.ident_callback = qi_lb60_nand_ident,
+	.busy_gpio = 94,
+};
+
+/* Keyboard*/
+
+/* #define KEEP_UART_ALIVE
+ * don't define this. the keyboard and keyboard both work
+ */
+
+#define KEY_QI_QI	KEY_F13
+#define KEY_QI_UPRED	KEY_RIGHTALT
+#define KEY_QI_VOLUP	KEY_VOLUMEUP
+#define KEY_QI_VOLDOWN	KEY_VOLUMEDOWN
+#define KEY_QI_FN	KEY_LEFTCTRL
+
+static const uint32_t qi_lb60_keymap[] = {
+	KEY(0, 0, KEY_F1),	/* S2 */
+	KEY(0, 1, KEY_F2),	/* S3 */
+	KEY(0, 2, KEY_F3),	/* S4 */
+	KEY(0, 3, KEY_F4),	/* S5 */
+	KEY(0, 4, KEY_F5),	/* S6 */
+	KEY(0, 5, KEY_F6),	/* S7 */
+	KEY(0, 6, KEY_F7),	/* S8 */
+
+	KEY(1, 0, KEY_Q),	/* S10 */
+	KEY(1, 1, KEY_W),	/* S11 */
+	KEY(1, 2, KEY_E),	/* S12 */
+	KEY(1, 3, KEY_R),	/* S13 */
+	KEY(1, 4, KEY_T),	/* S14 */
+	KEY(1, 5, KEY_Y),	/* S15 */
+	KEY(1, 6, KEY_U),	/* S16 */
+	KEY(1, 7, KEY_I),	/* S17 */
+	KEY(2, 0, KEY_A),	/* S18 */
+	KEY(2, 1, KEY_S),	/* S19 */
+	KEY(2, 2, KEY_D),	/* S20 */
+	KEY(2, 3, KEY_F),	/* S21 */
+	KEY(2, 4, KEY_G),	/* S22 */
+	KEY(2, 5, KEY_H),	/* S23 */
+	KEY(2, 6, KEY_J),	/* S24 */
+	KEY(2, 7, KEY_K),	/* S25 */
+	KEY(3, 0, KEY_ESC),	/* S26 */
+	KEY(3, 1, KEY_Z),	/* S27 */
+	KEY(3, 2, KEY_X),	/* S28 */
+	KEY(3, 3, KEY_C),	/* S29 */
+	KEY(3, 4, KEY_V),	/* S30 */
+	KEY(3, 5, KEY_B),	/* S31 */
+	KEY(3, 6, KEY_N),	/* S32 */
+	KEY(3, 7, KEY_M),	/* S33 */
+	KEY(4, 0, KEY_TAB),	/* S34 */
+	KEY(4, 1, KEY_CAPSLOCK),	/* S35 */
+	KEY(4, 2, KEY_BACKSLASH),	/* S36 */
+	KEY(4, 3, KEY_APOSTROPHE),	/* S37 */
+	KEY(4, 4, KEY_COMMA),	/* S38 */
+	KEY(4, 5, KEY_DOT),	/* S39 */
+	KEY(4, 6, KEY_SLASH),	/* S40 */
+	KEY(4, 7, KEY_UP),	/* S41 */
+	KEY(5, 0, KEY_O),	/* S42 */
+	KEY(5, 1, KEY_L),	/* S43 */
+	KEY(5, 2, KEY_EQUAL),	/* S44 */
+	KEY(5, 3, KEY_QI_UPRED),	/* S45 */
+	KEY(5, 4, KEY_SPACE),	/* S46 */
+	KEY(5, 5, KEY_QI_QI),	/* S47 */
+	KEY(5, 6, KEY_RIGHTCTRL),	/* S48 */
+	KEY(5, 7, KEY_LEFT),	/* S49 */
+	KEY(6, 0, KEY_F8),	/* S50 */
+	KEY(6, 1, KEY_P),	/* S51 */
+	KEY(6, 2, KEY_BACKSPACE),/* S52 */
+	KEY(6, 3, KEY_ENTER),	/* S53 */
+	KEY(6, 4, KEY_QI_VOLUP),	/* S54 */
+	KEY(6, 5, KEY_QI_VOLDOWN),	/* S55 */
+	KEY(6, 6, KEY_DOWN),	/* S56 */
+	KEY(6, 7, KEY_RIGHT),	/* S57 */
+
+#ifndef KEEP_UART_ALIVE
+	KEY(7, 0, KEY_LEFTSHIFT),	/* S58 */
+	KEY(7, 1, KEY_LEFTALT),	/* S59 */
+	KEY(7, 2, KEY_QI_FN),	/* S60 */
+#endif
+};
+
+static const struct matrix_keymap_data qi_lb60_keymap_data = {
+	.keymap		= qi_lb60_keymap,
+	.keymap_size	= ARRAY_SIZE(qi_lb60_keymap),
+};
+
+static const unsigned int qi_lb60_keypad_cols[] = {
+	74, 75, 76, 77, 78, 79, 80, 81,
+};
+
+static const unsigned int qi_lb60_keypad_rows[] = {
+	114, 115, 116, 117, 118, 119, 120,
+#ifndef KEEP_UART_ALIVE
+	122,
+#endif
+};
+
+static struct matrix_keypad_platform_data qi_lb60_pdata = {
+	.keymap_data = &qi_lb60_keymap_data,
+	.col_gpios	= qi_lb60_keypad_cols,
+	.row_gpios	= qi_lb60_keypad_rows,
+	.num_col_gpios	= ARRAY_SIZE(qi_lb60_keypad_cols),
+	.num_row_gpios	= ARRAY_SIZE(qi_lb60_keypad_rows),
+	.col_scan_delay_us	= 10,
+	.debounce_ms		= 10,
+	.wakeup			= 1,
+	.active_low		= 1,
+};
+
+static struct platform_device qi_lb60_keypad = {
+	.name		= "matrix-keypad",
+	.id		= -1,
+	.dev		= {
+		.platform_data = &qi_lb60_pdata,
+	},
+};
+
+/* Display */
+static struct fb_videomode qi_lb60_video_modes[] = {
+	{
+		.name = "320x240",
+		.xres = 320,
+		.yres = 240,
+		.refresh = 30,
+		.left_margin = 140,
+		.right_margin = 273,
+		.upper_margin = 20,
+		.lower_margin = 2,
+		.hsync_len = 1,
+		.vsync_len = 1,
+		.sync = 0,
+		.vmode = FB_VMODE_NONINTERLACED,
+	},
+};
+
+static struct jz4740_fb_platform_data qi_lb60_fb_pdata = {
+	.width		= 60,
+	.height		= 45,
+	.num_modes	= ARRAY_SIZE(qi_lb60_video_modes),
+	.modes		= qi_lb60_video_modes,
+	.bpp		= 24,
+	.lcd_type	= JZ_LCD_TYPE_8BIT_SERIAL,
+	.pixclk_falling_edge = 1,
+};
+
+
+struct spi_gpio_platform_data spigpio_platform_data = {
+	.sck = JZ_GPIO_PORTC(23),
+	.mosi = JZ_GPIO_PORTC(22),
+	.miso = -1,
+	.num_chipselect = 1,
+};
+
+static struct platform_device spigpio_device = {
+	.name = "spi_gpio",
+	.id   = 1,
+	.dev = {
+		.platform_data = &spigpio_platform_data,
+	},
+};
+
+static struct spi_board_info qi_lb60_spi_board_info[] = {
+	{
+		.modalias = "gpm940b0",
+		.controller_data = (void *)JZ_GPIO_PORTC(21),
+		.chip_select = 0,
+		.bus_num = 1,
+		.max_speed_hz = 30 * 1000,
+		.mode = SPI_3WIRE,
+	},
+};
+
+/* Battery */
+static struct jz_battery_platform_data qi_lb60_battery_pdata = {
+	.gpio_charge = GPIO_CHARG_STAT_N,
+	.gpio_charge_active_low = 1,
+	.info = {
+		.name = "battery",
+		.technology = POWER_SUPPLY_TECHNOLOGY_LIPO,
+		.voltage_max_design = 4200000,
+		.voltage_min_design = 3600000,
+	},
+};
+
+static char *qi_lb60_batteries[] = {
+	"battery",
+};
+
+static struct gpio_charger_platform_data qi_lb60_charger_pdata = {
+	.name = "USB",
+	.type = POWER_SUPPLY_TYPE_USB,
+	.gpio = GPIO_USB_DETE,
+	.gpio_active_low = 1,
+	.batteries = qi_lb60_batteries,
+	.num_batteries = ARRAY_SIZE(qi_lb60_batteries),
+};
+
+static struct platform_device qi_lb60_charger_device = {
+	.name = "gpio-charger",
+	.dev = {
+		.platform_data = &qi_lb60_charger_pdata,
+	},
+};
+
+/* GPIO Key: power */
+static struct gpio_keys_button qi_lb60_gpio_keys_buttons[] = {
+	[0] = {
+		.code		= KEY_POWER,
+		.gpio		= GPIO_WAKEUP_N,
+		.active_low	= 1,
+		.desc		= "Power",
+		.wakeup		= 1,
+	},
+};
+
+static struct gpio_keys_platform_data qi_lb60_gpio_keys_data = {
+	.nbuttons = ARRAY_SIZE(qi_lb60_gpio_keys_buttons),
+	.buttons = qi_lb60_gpio_keys_buttons,
+};
+
+static struct platform_device qi_lb60_gpio_keys = {
+	.name =	"gpio-keys",
+	.id =	-1,
+	.dev = {
+		.platform_data = &qi_lb60_gpio_keys_data,
+	}
+};
+
+static struct jz4740_mmc_platform_data qi_lb60_mmc_pdata = {
+	.gpio_card_detect	= JZ_GPIO_PORTD(0),
+	.gpio_read_only		= -1,
+	.gpio_power		= JZ_GPIO_PORTD(2),
+	.power_active_low	= 1,
+};
+
+static struct regulator_consumer_supply avt2_usb_regulator_consumer =
+	REGULATOR_SUPPLY("vbus", "jz4740-ohci");
+
+static struct regulator_init_data avt2_usb_regulator_init_data = {
+	.num_consumer_supplies = 1,
+	.consumer_supplies = &avt2_usb_regulator_consumer,
+	.constraints = {
+		.name = "USB power",
+		.min_uV = 5000000,
+		.max_uV = 5000000,
+		.valid_modes_mask = REGULATOR_MODE_NORMAL,
+		.valid_ops_mask = REGULATOR_CHANGE_STATUS,
+	},
+};
+
+static struct fixed_voltage_config avt2_usb_regulator_data = {
+	.supply_name = "USB power",
+	.microvolts = 5000000,
+	.gpio = JZ_GPIO_PORTB(17),
+	.init_data = &avt2_usb_regulator_init_data,
+};
+
+static struct platform_device avt2_usb_regulator_device = {
+	.name = "reg-fixed-voltage",
+	.id = -1,
+	.dev = {
+		.platform_data = &avt2_usb_regulator_data,
+	}
+};
+
+static struct led_pwm qi_lb60_pizo_led = {
+	.name = "nanonote::pizo",
+	.pwm_id = 4,
+	.max_brightness = 255,
+	.pwm_period_ns = 1000000,
+};
+
+static struct led_pwm_platform_data qi_lb60_pizo_data = {
+	.num_leds = 1,
+	.leds = &qi_lb60_pizo_led,
+};
+
+static struct platform_device qi_lb60_pizo_device = {
+	.name = "leds_pwm",
+	.id = -1,
+	.dev = {
+		.platform_data = &qi_lb60_pizo_data,
+	}
+};
+
+static struct platform_device *jz_platform_devices[] __initdata = {
+	&jz4740_usb_gdt_device,
+	&jz4740_mmc_device,
+	&jz4740_nand_device,
+	&qi_lb60_keypad,
+	&spigpio_device,
+	&jz4740_framebuffer_device,
+	&jz4740_i2s_device,
+	&jz4740_codec_device,
+	&jz4740_rtc_device,
+	&jz4740_adc_device,
+	&jz4740_battery_device,
+	&qi_lb60_gpio_keys,
+	&qi_lb60_charger_device,
+	&qi_lb60_pizo_device,
+};
+
+static void __init board_gpio_setup(void)
+{
+	/* We only need to enable/disable pullup here for pins used in generic
+	 * drivers. Everything else is done by the drivers themselfs. */
+	jz_gpio_disable_pullup(GPIO_SD_VCC_EN_N);
+	jz_gpio_disable_pullup(GPIO_SD_CD_N);
+}
+
+static int __init qi_lb60_init_platform_devices(void)
+{
+	jz4740_framebuffer_device.dev.platform_data = &qi_lb60_fb_pdata;
+	jz4740_nand_device.dev.platform_data = &qi_lb60_nand_pdata;
+	jz4740_battery_device.dev.platform_data = &qi_lb60_battery_pdata;
+	jz4740_mmc_device.dev.platform_data = &qi_lb60_mmc_pdata;
+
+	spi_register_board_info(qi_lb60_spi_board_info,
+				ARRAY_SIZE(qi_lb60_spi_board_info));
+
+	if (is_avt2) {
+		platform_device_register(&avt2_usb_regulator_device);
+		platform_device_register(&jz4740_usb_ohci_device);
+	}
+
+	return platform_add_devices(jz_platform_devices,
+					ARRAY_SIZE(jz_platform_devices));
+
+}
+
+struct jz4740_clock_board_data jz4740_clock_bdata = {
+	.ext_rate = 12000000,
+	.rtc_rate = 32768,
+};
+
+extern int jz_gpiolib_init(void);
+
+static __init int board_avt2(char *str)
+{
+	qi_lb60_mmc_pdata.card_detect_active_low = 1;
+	qi_lb60_mmc_pdata.power_active_low	= 1;
+	is_avt2 = true;
+
+	return 1;
+}
+
+__setup("avt2", board_avt2);
+
+static int __init qi_lb60_board_setup(void)
+{
+	printk(KERN_INFO "Qi Hardware JZ4740 QI_LB60 setup\n");
+	if (jz_gpiolib_init())
+		panic("Failed to initalize jz gpio\n");
+
+	jz4740_clock_init();
+	board_gpio_setup();
+
+	if (qi_lb60_init_platform_devices())
+		panic("Failed to initalize platform devices\n");
+
+	return 0;
+}
+
+arch_initcall(qi_lb60_board_setup);
-- 
1.5.6.5

