From ae6e941c5d58262c0a09c355ae384b7109977053 Mon Sep 17 00:00:00 2001
From: Lars-Peter Clausen <lars@metafoo.de>
Date: Mon, 12 Jul 2010 03:48:08 +0200
Subject: [PATCH] mfd: Add JZ4740 ADC driver

This patch adds a MFD driver for the JZ4740 ADC unit. The driver is used to
demultiplex IRQs and synchronize access to shared registers between the
battery, hwmon and (future) touchscreen driver.

Signed-off-by: Lars-Peter Clausen <lars@metafoo.de>
Signed-off-by: Samuel Ortiz <sameo@linux.intel.com>
---
 drivers/mfd/Kconfig        |    8 +
 drivers/mfd/Makefile       |    1 +
 drivers/mfd/jz4740-adc.c   |  394 ++++++++++++++++++++++++++++++++++++++++++++
 include/linux/jz4740-adc.h |   32 ++++
 4 files changed, 435 insertions(+), 0 deletions(-)
 create mode 100644 drivers/mfd/jz4740-adc.c
 create mode 100644 include/linux/jz4740-adc.h

--- a/drivers/mfd/Kconfig
+++ b/drivers/mfd/Kconfig
@@ -482,6 +482,14 @@ config MFD_JANZ_CMODIO
 	  host many different types of MODULbus daughterboards, including
 	  CAN and GPIO controllers.
 
+config MFD_JZ4740_ADC
+	tristate "Support for the JZ4740 SoC ADC core"
+	select MFD_CORE
+	depends on MACH_JZ4740
+	help
+	  Say yes here if you want support for the ADC unit in the JZ4740 SoC.
+	  This driver is necessary for jz4740-battery and jz4740-hwmon driver.
+
 endif # MFD_SUPPORT
 
 menu "Multimedia Capabilities Port drivers"
--- a/drivers/mfd/Makefile
+++ b/drivers/mfd/Makefile
@@ -71,3 +71,4 @@ obj-$(CONFIG_PMIC_ADP5520)	+= adp5520.o
 obj-$(CONFIG_LPC_SCH)		+= lpc_sch.o
 obj-$(CONFIG_MFD_RDC321X)	+= rdc321x-southbridge.o
 obj-$(CONFIG_MFD_JANZ_CMODIO)	+= janz-cmodio.o
+obj-$(CONFIG_MFD_JZ4740_ADC)	+= jz4740-adc.o
--- /dev/null
+++ b/drivers/mfd/jz4740-adc.c
@@ -0,0 +1,394 @@
+/*
+ * Copyright (C) 2009-2010, Lars-Peter Clausen <lars@metafoo.de>
+ * JZ4740 SoC ADC driver
+ *
+ * This program is free software; you can redistribute it and/or modify it
+ * under  the terms of the GNU General  Public License as published by the
+ * Free Software Foundation;  either version 2 of the License, or (at your
+ * option) any later version.
+ *
+ * You should have received a copy of the GNU General Public License along
+ * with this program; if not, write to the Free Software Foundation, Inc.,
+ * 675 Mass Ave, Cambridge, MA 02139, USA.
+ *
+ * This driver synchronizes access to the JZ4740 ADC core between the
+ * JZ4740 battery and hwmon drivers.
+ */
+
+#include <linux/err.h>
+#include <linux/irq.h>
+#include <linux/interrupt.h>
+#include <linux/kernel.h>
+#include <linux/module.h>
+#include <linux/platform_device.h>
+#include <linux/slab.h>
+#include <linux/spinlock.h>
+
+#include <linux/clk.h>
+#include <linux/mfd/core.h>
+
+#include <linux/jz4740-adc.h>
+
+
+#define JZ_REG_ADC_ENABLE	0x00
+#define JZ_REG_ADC_CFG		0x04
+#define JZ_REG_ADC_CTRL		0x08
+#define JZ_REG_ADC_STATUS	0x0c
+
+#define JZ_REG_ADC_TOUCHSCREEN_BASE	0x10
+#define JZ_REG_ADC_BATTERY_BASE	0x1c
+#define JZ_REG_ADC_HWMON_BASE	0x20
+
+#define JZ_ADC_ENABLE_TOUCH	BIT(2)
+#define JZ_ADC_ENABLE_BATTERY	BIT(1)
+#define JZ_ADC_ENABLE_ADCIN	BIT(0)
+
+enum {
+	JZ_ADC_IRQ_ADCIN = 0,
+	JZ_ADC_IRQ_BATTERY,
+	JZ_ADC_IRQ_TOUCH,
+	JZ_ADC_IRQ_PENUP,
+	JZ_ADC_IRQ_PENDOWN,
+};
+
+struct jz4740_adc {
+	struct resource *mem;
+	void __iomem *base;
+
+	int irq;
+	int irq_base;
+
+	struct clk *clk;
+	atomic_t clk_ref;
+
+	spinlock_t lock;
+};
+
+static inline void jz4740_adc_irq_set_masked(struct jz4740_adc *adc, int irq,
+	bool masked)
+{
+	unsigned long flags;
+	uint8_t val;
+
+	irq -= adc->irq_base;
+
+	spin_lock_irqsave(&adc->lock, flags);
+
+	val = readb(adc->base + JZ_REG_ADC_CTRL);
+	if (masked)
+		val |= BIT(irq);
+	else
+		val &= ~BIT(irq);
+	writeb(val, adc->base + JZ_REG_ADC_CTRL);
+
+	spin_unlock_irqrestore(&adc->lock, flags);
+}
+
+static void jz4740_adc_irq_mask(unsigned int irq)
+{
+	struct jz4740_adc *adc = get_irq_chip_data(irq);
+	jz4740_adc_irq_set_masked(adc, irq, true);
+}
+
+static void jz4740_adc_irq_unmask(unsigned int irq)
+{
+	struct jz4740_adc *adc = get_irq_chip_data(irq);
+	jz4740_adc_irq_set_masked(adc, irq, false);
+}
+
+static void jz4740_adc_irq_ack(unsigned int irq)
+{
+	struct jz4740_adc *adc = get_irq_chip_data(irq);
+
+	irq -= adc->irq_base;
+	writeb(BIT(irq), adc->base + JZ_REG_ADC_STATUS);
+}
+
+static struct irq_chip jz4740_adc_irq_chip = {
+	.name = "jz4740-adc",
+	.mask = jz4740_adc_irq_mask,
+	.unmask = jz4740_adc_irq_unmask,
+	.ack = jz4740_adc_irq_ack,
+};
+
+static void jz4740_adc_irq_demux(unsigned int irq, struct irq_desc *desc)
+{
+	struct jz4740_adc *adc = get_irq_desc_data(desc);
+	uint8_t status;
+	unsigned int i;
+
+	status = readb(adc->base + JZ_REG_ADC_STATUS);
+
+	for (i = 0; i < 5; ++i) {
+		if (status & BIT(i))
+			generic_handle_irq(adc->irq_base + i);
+	}
+}
+
+
+/* Refcounting for the ADC clock is done in here instead of in the clock
+ * framework, because it is the only clock which is shared between multiple
+ * devices and thus is the only clock which needs refcounting */
+static inline void jz4740_adc_clk_enable(struct jz4740_adc *adc)
+{
+	if (atomic_inc_return(&adc->clk_ref) == 1)
+		clk_enable(adc->clk);
+}
+
+static inline void jz4740_adc_clk_disable(struct jz4740_adc *adc)
+{
+	if (atomic_dec_return(&adc->clk_ref) == 0)
+		clk_disable(adc->clk);
+}
+
+static inline void jz4740_adc_set_enabled(struct jz4740_adc *adc, int engine,
+	bool enabled)
+{
+	unsigned long flags;
+	uint8_t val;
+
+	spin_lock_irqsave(&adc->lock, flags);
+
+	val = readb(adc->base + JZ_REG_ADC_ENABLE);
+	if (enabled)
+		val |= BIT(engine);
+	else
+		val &= BIT(engine);
+	writeb(val, adc->base + JZ_REG_ADC_ENABLE);
+
+	spin_unlock_irqrestore(&adc->lock, flags);
+}
+
+static int jz4740_adc_cell_enable(struct platform_device *pdev)
+{
+	struct jz4740_adc *adc = dev_get_drvdata(pdev->dev.parent);
+
+	jz4740_adc_clk_enable(adc);
+	jz4740_adc_set_enabled(adc, pdev->id, true);
+
+	return 0;
+}
+
+static int jz4740_adc_cell_disable(struct platform_device *pdev)
+{
+	struct jz4740_adc *adc = dev_get_drvdata(pdev->dev.parent);
+
+	jz4740_adc_set_enabled(adc, pdev->id, false);
+	jz4740_adc_clk_disable(adc);
+
+	return 0;
+}
+
+int jz4740_adc_set_config(struct device *dev, uint32_t mask, uint32_t val)
+{
+	struct jz4740_adc *adc = dev_get_drvdata(dev);
+	unsigned long flags;
+	uint32_t cfg;
+
+	if (!adc)
+		return -ENODEV;
+
+	spin_lock_irqsave(&adc->lock, flags);
+
+	cfg = readl(adc->base + JZ_REG_ADC_CFG);
+
+	cfg &= ~mask;
+	cfg |= val;
+
+	writel(cfg, adc->base + JZ_REG_ADC_CFG);
+
+	spin_unlock_irqrestore(&adc->lock, flags);
+
+	return 0;
+}
+EXPORT_SYMBOL_GPL(jz4740_adc_set_config);
+
+static struct resource jz4740_hwmon_resources[] = {
+	{
+		.start = JZ_ADC_IRQ_ADCIN,
+		.flags = IORESOURCE_IRQ,
+	},
+	{
+		.start	= JZ_REG_ADC_HWMON_BASE,
+		.end	= JZ_REG_ADC_HWMON_BASE + 3,
+		.flags	= IORESOURCE_MEM,
+	},
+};
+
+static struct resource jz4740_battery_resources[] = {
+	{
+		.start = JZ_ADC_IRQ_BATTERY,
+		.flags = IORESOURCE_IRQ,
+	},
+	{
+		.start	= JZ_REG_ADC_BATTERY_BASE,
+		.end	= JZ_REG_ADC_BATTERY_BASE + 3,
+		.flags	= IORESOURCE_MEM,
+	},
+};
+
+const struct mfd_cell jz4740_adc_cells[] = {
+	{
+		.id = 0,
+		.name = "jz4740-hwmon",
+		.num_resources = ARRAY_SIZE(jz4740_hwmon_resources),
+		.resources = jz4740_hwmon_resources,
+		.platform_data = (void *)&jz4740_adc_cells[0],
+		.data_size = sizeof(struct mfd_cell),
+
+		.enable = jz4740_adc_cell_enable,
+		.disable = jz4740_adc_cell_disable,
+	},
+	{
+		.id = 1,
+		.name = "jz4740-battery",
+		.num_resources = ARRAY_SIZE(jz4740_battery_resources),
+		.resources = jz4740_battery_resources,
+		.platform_data = (void *)&jz4740_adc_cells[1],
+		.data_size = sizeof(struct mfd_cell),
+
+		.enable = jz4740_adc_cell_enable,
+		.disable = jz4740_adc_cell_disable,
+	},
+};
+
+static int __devinit jz4740_adc_probe(struct platform_device *pdev)
+{
+	int ret;
+	struct jz4740_adc *adc;
+	struct resource *mem_base;
+	int irq;
+
+	adc = kmalloc(sizeof(*adc), GFP_KERNEL);
+	if (!adc) {
+		dev_err(&pdev->dev, "Failed to allocate driver structure\n");
+		return -ENOMEM;
+	}
+
+	adc->irq = platform_get_irq(pdev, 0);
+	if (adc->irq < 0) {
+		ret = adc->irq;
+		dev_err(&pdev->dev, "Failed to get platform irq: %d\n", ret);
+		goto err_free;
+	}
+
+	adc->irq_base = platform_get_irq(pdev, 1);
+	if (adc->irq_base < 0) {
+		ret = adc->irq_base;
+		dev_err(&pdev->dev, "Failed to get irq base: %d\n", ret);
+		goto err_free;
+	}
+
+	mem_base = platform_get_resource(pdev, IORESOURCE_MEM, 0);
+	if (!mem_base) {
+		ret = -ENOENT;
+		dev_err(&pdev->dev, "Failed to get platform mmio resource\n");
+		goto err_free;
+	}
+
+	/* Only request the shared registers for the MFD driver */
+	adc->mem = request_mem_region(mem_base->start, JZ_REG_ADC_STATUS,
+					pdev->name);
+	if (!adc->mem) {
+		ret = -EBUSY;
+		dev_err(&pdev->dev, "Failed to request mmio memory region\n");
+		goto err_free;
+	}
+
+	adc->base = ioremap_nocache(adc->mem->start, resource_size(adc->mem));
+	if (!adc->base) {
+		ret = -EBUSY;
+		dev_err(&pdev->dev, "Failed to ioremap mmio memory\n");
+		goto err_release_mem_region;
+	}
+
+	adc->clk = clk_get(&pdev->dev, "adc");
+	if (IS_ERR(adc->clk)) {
+		ret = PTR_ERR(adc->clk);
+		dev_err(&pdev->dev, "Failed to get clock: %d\n", ret);
+		goto err_iounmap;
+	}
+
+	spin_lock_init(&adc->lock);
+	atomic_set(&adc->clk_ref, 0);
+
+	platform_set_drvdata(pdev, adc);
+
+	for (irq = adc->irq_base; irq < adc->irq_base + 5; ++irq) {
+		set_irq_chip_data(irq, adc);
+		set_irq_chip_and_handler(irq, &jz4740_adc_irq_chip,
+		    handle_level_irq);
+	}
+
+	set_irq_data(adc->irq, adc);
+	set_irq_chained_handler(adc->irq, jz4740_adc_irq_demux);
+
+	writeb(0x00, adc->base + JZ_REG_ADC_ENABLE);
+	writeb(0xff, adc->base + JZ_REG_ADC_CTRL);
+
+	ret = mfd_add_devices(&pdev->dev, 0, jz4740_adc_cells,
+		ARRAY_SIZE(jz4740_adc_cells), mem_base, adc->irq_base);
+	if (ret < 0)
+		goto err_clk_put;
+
+	return 0;
+
+err_clk_put:
+	clk_put(adc->clk);
+err_iounmap:
+	platform_set_drvdata(pdev, NULL);
+	iounmap(adc->base);
+err_release_mem_region:
+	release_mem_region(adc->mem->start, resource_size(adc->mem));
+err_free:
+	kfree(adc);
+
+	return ret;
+}
+
+static int __devexit jz4740_adc_remove(struct platform_device *pdev)
+{
+	struct jz4740_adc *adc = platform_get_drvdata(pdev);
+
+	mfd_remove_devices(&pdev->dev);
+
+	set_irq_data(adc->irq, NULL);
+	set_irq_chained_handler(adc->irq, NULL);
+
+	iounmap(adc->base);
+	release_mem_region(adc->mem->start, resource_size(adc->mem));
+
+	clk_put(adc->clk);
+
+	platform_set_drvdata(pdev, NULL);
+
+	kfree(adc);
+
+	return 0;
+}
+
+struct platform_driver jz4740_adc_driver = {
+	.probe	= jz4740_adc_probe,
+	.remove = __devexit_p(jz4740_adc_remove),
+	.driver = {
+		.name = "jz4740-adc",
+		.owner = THIS_MODULE,
+	},
+};
+
+static int __init jz4740_adc_init(void)
+{
+	return platform_driver_register(&jz4740_adc_driver);
+}
+module_init(jz4740_adc_init);
+
+static void __exit jz4740_adc_exit(void)
+{
+	platform_driver_unregister(&jz4740_adc_driver);
+}
+module_exit(jz4740_adc_exit);
+
+MODULE_DESCRIPTION("JZ4740 SoC ADC driver");
+MODULE_AUTHOR("Lars-Peter Clausen <lars@metafoo.de>");
+MODULE_LICENSE("GPL");
+MODULE_ALIAS("platform:jz4740-adc");
--- /dev/null
+++ b/include/linux/jz4740-adc.h
@@ -0,0 +1,32 @@
+
+#ifndef __LINUX_JZ4740_ADC
+#define __LINUX_JZ4740_ADC
+
+#include <linux/device.h>
+
+/*
+ * jz4740_adc_set_config - Configure a JZ4740 adc device
+ * @dev: Pointer to a jz4740-adc device
+ * @mask: Mask for the config value to be set
+ * @val: Value to be set
+ *
+ * This function can be used by the JZ4740 ADC mfd cells to configure their
+ * options in the shared config register.
+*/
+int jz4740_adc_set_config(struct device *dev, uint32_t mask, uint32_t val);
+
+#define JZ_ADC_CONFIG_SPZZ		BIT(31)
+#define JZ_ADC_CONFIG_EX_IN		BIT(30)
+#define JZ_ADC_CONFIG_DNUM_MASK		(0x7 << 16)
+#define JZ_ADC_CONFIG_DMA_ENABLE	BIT(15)
+#define JZ_ADC_CONFIG_XYZ_MASK		(0x2 << 13)
+#define JZ_ADC_CONFIG_SAMPLE_NUM_MASK	(0x7 << 10)
+#define JZ_ADC_CONFIG_CLKDIV_MASK	(0xf << 5)
+#define JZ_ADC_CONFIG_BAT_MB		BIT(4)
+
+#define JZ_ADC_CONFIG_DNUM(dnum)	((dnum) << 16)
+#define JZ_ADC_CONFIG_XYZ_OFFSET(dnum)	((xyz) << 13)
+#define JZ_ADC_CONFIG_SAMPLE_NUM(x)	((x) << 10)
+#define JZ_ADC_CONFIG_CLKDIV(div)	((div) << 5)
+
+#endif
