--- a/src/drivers/nl80211_copy.h
+++ b/src/drivers/nl80211_copy.h
@@ -709,6 +709,9 @@ enum nl80211_commands {
  *	NL80211_CMD_AUTHENTICATE, NL80211_CMD_DEAUTHENTICATE,
  *	NL80211_CMD_DISASSOCIATE.
  *
+ * @NL80211_ATTR_AP_ISOLATE: (AP mode) Do not forward traffic between stations
+ *	connected to this BSS.
+ *
  * @NL80211_ATTR_MAX: highest attribute number currently defined
  * @__NL80211_ATTR_AFTER_LAST: internal use
  */
@@ -864,6 +867,8 @@ enum nl80211_attrs {
 
 	NL80211_ATTR_LOCAL_STATE_CHANGE,
 
+	NL80211_ATTR_AP_ISOLATE,
+
 	/* add attributes here, update the policy in nl80211.c */
 
 	__NL80211_ATTR_AFTER_LAST,
