From 53b1d94ccca6a06e86460344f7c38949d53374b6 Mon Sep 17 00:00:00 2001
From: Lars-Peter Clausen <lars@metafoo.de>
Date: Sat, 24 Apr 2010 12:36:15 +0200
Subject: [PATCH] Add qi_lb60 SoC sound board driver

---
 sound/soc/jz4740/Kconfig   |    8 ++
 sound/soc/jz4740/Makefile  |    4 +
 sound/soc/jz4740/qi_lb60.c |  182 ++++++++++++++++++++++++++++++++++++++++++++
 3 files changed, 194 insertions(+), 0 deletions(-)
 create mode 100644 sound/soc/jz4740/qi_lb60.c

diff --git a/sound/soc/jz4740/Kconfig b/sound/soc/jz4740/Kconfig
index 39df949..e546c30 100644
--- a/sound/soc/jz4740/Kconfig
+++ b/sound/soc/jz4740/Kconfig
@@ -11,3 +11,11 @@ config SND_JZ4740_SOC_I2S
 	tristate "SoC Audio (I2S protocol) for Ingenic jz4740 chip"
 	help
 	  Say Y if you want to use I2S protocol and I2S codec on Ingenic Jz4740 QI_LB60 board.
+
+config SND_JZ4740_SOC_QI_LB60
+	tristate "SoC Audio support for Qi Hardware Ben Nanonote"
+	depends on SND_JZ4740_SOC && JZ4740_QI_LB60
+	select SND_JZ4740_SOC_I2S
+    select SND_SOC_JZCODEC
+	help
+	  Say Y if you want to add support for SoC audio of internal codec on Ingenic Jz4740 QI_LB60 board.
diff --git a/sound/soc/jz4740/Makefile b/sound/soc/jz4740/Makefile
index 1be8d19..be873c1 100644
--- a/sound/soc/jz4740/Makefile
+++ b/sound/soc/jz4740/Makefile
@@ -7,3 +7,7 @@ snd-soc-jz4740-i2s-objs := jz4740-i2s.o
 obj-$(CONFIG_SND_JZ4740_SOC) += snd-soc-jz4740.o
 obj-$(CONFIG_SND_JZ4740_SOC_I2S) += snd-soc-jz4740-i2s.o
 
+# Jz4740 Machine Support
+snd-soc-qi-lb60-objs := qi_lb60.o
+
+obj-$(CONFIG_SND_JZ4740_SOC_QI_LB60) += snd-soc-qi-lb60.o
diff --git a/sound/soc/jz4740/qi_lb60.c b/sound/soc/jz4740/qi_lb60.c
new file mode 100644
index 0000000..a2ce3cf
--- /dev/null
+++ b/sound/soc/jz4740/qi_lb60.c
@@ -0,0 +1,182 @@
+/*
+ * Copyright (C) 2009, Lars-Peter Clausen <lars@metafoo.de>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ *
+ *  You should have received a copy of the  GNU General Public License along
+ *  with this program; if not, write  to the Free Software Foundation, Inc.,
+ *  675 Mass Ave, Cambridge, MA 02139, USA.
+ *
+ */
+
+#include <linux/module.h>
+#include <linux/moduleparam.h>
+#include <linux/timer.h>
+#include <linux/interrupt.h>
+#include <linux/platform_device.h>
+#include <sound/core.h>
+#include <sound/pcm.h>
+#include <sound/soc.h>
+#include <sound/soc-dapm.h>
+#include <linux/gpio.h>
+
+#include "../codecs/jzcodec.h"
+#include "jz4740-pcm.h"
+#include "jz4740-i2s.h"
+
+
+#define QI_LB60_SND_GPIO JZ_GPIO_PORTB(29)
+#define QI_LB60_AMP_GPIO JZ_GPIO_PORTD(4)
+
+static int qi_lb60_spk_event(struct snd_soc_dapm_widget *widget,
+			     struct snd_kcontrol *ctrl, int event)
+{
+	int on = 0;
+	if (event & SND_SOC_DAPM_POST_PMU)
+		on = 1;
+	else if (event & SND_SOC_DAPM_PRE_PMD)
+		on = 0;
+
+	gpio_set_value(QI_LB60_SND_GPIO, on);
+	gpio_set_value(QI_LB60_AMP_GPIO, on);
+
+	return 0;
+}
+
+static const struct snd_soc_dapm_widget qi_lb60_widgets[] = {
+	SND_SOC_DAPM_SPK("Speaker", qi_lb60_spk_event),
+	SND_SOC_DAPM_MIC("Mic", NULL),
+};
+
+static const struct snd_soc_dapm_route qi_lb60_routes[] = {
+	{"Mic", NULL, "MIC"},
+	{"Speaker", NULL, "LOUT"},
+	{"Speaker", NULL, "ROUT"},
+};
+
+#define QI_LB60_DAIFMT (SND_SOC_DAIFMT_I2S | \
+			SND_SOC_DAIFMT_NB_NF | \
+			SND_SOC_DAIFMT_CBM_CFM)
+
+static int qi_lb60_codec_init(struct snd_soc_codec *codec)
+{
+	int ret;
+	struct snd_soc_dai *cpu_dai = codec->socdev->card->dai_link->cpu_dai;
+	struct snd_soc_dai *codec_dai = codec->socdev->card->dai_link->codec_dai;
+
+	snd_soc_dapm_nc_pin(codec, "LIN");
+	snd_soc_dapm_nc_pin(codec, "RIN");
+
+	ret = snd_soc_dai_set_fmt(codec_dai, QI_LB60_DAIFMT);
+	if (ret < 0) {
+		dev_err(codec->dev, "Failed to set codec dai format: %d\n", ret);
+		return ret;
+	}
+
+	ret = snd_soc_dai_set_fmt(cpu_dai, QI_LB60_DAIFMT);
+	if (ret < 0) {
+		dev_err(codec->dev, "Failed to set cpu dai format: %d\n", ret);
+		return ret;
+	}
+
+	ret = snd_soc_dai_set_sysclk(codec_dai, JZCODEC_SYSCLK, 111,
+		SND_SOC_CLOCK_IN);
+	if (ret < 0) {
+		dev_err(codec->dev, "Failed to set codec dai sysclk: %d\n", ret);
+		return ret;
+	}
+
+	snd_soc_dapm_new_controls(codec, qi_lb60_widgets, ARRAY_SIZE(qi_lb60_widgets));
+
+	snd_soc_dapm_add_routes(codec, qi_lb60_routes, ARRAY_SIZE(qi_lb60_routes));
+
+	snd_soc_dapm_sync(codec);
+
+	return 0;
+}
+
+static struct snd_soc_dai_link qi_lb60_dai = {
+	.name = "jz-codec",
+	.stream_name = "JZCODEC",
+	.cpu_dai = &jz4740_i2s_dai,
+	.codec_dai = &jz_codec_dai,
+	.init = qi_lb60_codec_init,
+};
+
+static struct snd_soc_card qi_lb60 = {
+	.name = "QI LB60",
+	.dai_link = &qi_lb60_dai,
+	.num_links = 1,
+	.platform = &jz4740_soc_platform,
+};
+
+static struct snd_soc_device qi_lb60_snd_devdata = {
+	.card = &qi_lb60,
+	.codec_dev = &soc_codec_dev_jzcodec,
+};
+
+static struct platform_device *qi_lb60_snd_device;
+
+static int __init qi_lb60_init(void)
+{
+	int ret;
+
+	qi_lb60_snd_device = platform_device_alloc("soc-audio", -1);
+
+	if (!qi_lb60_snd_device)
+		return -ENOMEM;
+
+
+	ret = gpio_request(QI_LB60_SND_GPIO, "SND");
+	if (ret) {
+		pr_err("qi_lb60 snd: Failed to request SND GPIO(%d): %d\n",
+				QI_LB60_SND_GPIO, ret);
+		goto err_device_put;
+	}
+
+	ret = gpio_request(QI_LB60_AMP_GPIO, "AMP");
+	if (ret) {
+		pr_err("qi_lb60 snd: Failed to request AMP GPIO(%d): %d\n",
+				QI_LB60_AMP_GPIO, ret);
+		goto err_gpio_free_snd;
+	}
+
+	gpio_direction_output(JZ_GPIO_PORTB(29), 0);
+	gpio_direction_output(JZ_GPIO_PORTD(4), 0);
+
+	platform_set_drvdata(qi_lb60_snd_device, &qi_lb60_snd_devdata);
+	qi_lb60_snd_devdata.dev = &qi_lb60_snd_device->dev;
+	ret = platform_device_add(qi_lb60_snd_device);
+	if (ret) {
+		pr_err("qi_lb60 snd: Failed to add snd soc device: %d\n", ret);
+		goto err_unset_pdata;
+	}
+
+	 return 0;
+
+err_unset_pdata:
+	platform_set_drvdata(qi_lb60_snd_device, NULL);
+/*err_gpio_free_amp:*/
+	gpio_free(QI_LB60_AMP_GPIO);
+err_gpio_free_snd:
+	gpio_free(QI_LB60_SND_GPIO);
+err_device_put:
+	platform_device_put(qi_lb60_snd_device);
+
+	return ret;
+}
+module_init(qi_lb60_init);
+
+static void __exit qi_lb60_exit(void)
+{
+	gpio_free(QI_LB60_AMP_GPIO);
+	gpio_free(QI_LB60_SND_GPIO);
+	platform_device_unregister(qi_lb60_snd_device);
+}
+module_exit(qi_lb60_exit);
+
+MODULE_AUTHOR("Lars-Peter Clausen <lars@metafoo.de>");
+MODULE_DESCRIPTION("ALSA SoC QI LB60 Audio support");
+MODULE_LICENSE("GPL v2");
-- 
1.5.6.5

