--- a/drivers/power/Kconfig
+++ b/drivers/power/Kconfig
@@ -88,4 +88,16 @@ config CHARGER_PCF50633
 	help
 	 Say Y to include support for NXP PCF50633 Main Battery Charger.
 
+config BATTERY_BQ27000_HDQ
+	tristate "BQ27000 HDQ battery monitor driver"
+	help
+	  Say Y to enable support for the battery on the Neo Freerunner
+
+config HDQ_GPIO_BITBANG
+	bool "Generic gpio based HDQ bitbang"
+	help
+	  Say Y to enable supoort for generic gpio based HDQ bitbang driver.
+	  This can not be built as a module.
+
 endif # POWER_SUPPLY
+
--- a/drivers/power/Makefile
+++ b/drivers/power/Makefile
@@ -25,4 +25,7 @@ obj-$(CONFIG_BATTERY_TOSA)	+= tosa_batte
 obj-$(CONFIG_BATTERY_WM97XX)	+= wm97xx_battery.o
 obj-$(CONFIG_BATTERY_BQ27x00)	+= bq27x00_battery.o
 obj-$(CONFIG_BATTERY_DA9030)	+= da9030_battery.o
-obj-$(CONFIG_CHARGER_PCF50633)	+= pcf50633-charger.o
\ No newline at end of file
+obj-$(CONFIG_CHARGER_PCF50633)	+= pcf50633-charger.o
+obj-$(CONFIG_BATTERY_BQ27000_HDQ)	+= bq27000_battery.o
+
+obj-$(CONFIG_HDQ_GPIO_BITBANG)  += hdq.o
