--- a/drivers/serial/Kconfig
+++ b/drivers/serial/Kconfig
@@ -1383,6 +1383,14 @@ config SERIAL_OF_PLATFORM_NWPSERIAL_CONS
 	help
 	  Support for Console on the NWP serial ports.
 
+config SERIAL_IFXMIPS
+	bool "IFXMips serial driver"
+	depends on IFXMIPS
+	select SERIAL_CORE
+	select SERIAL_CORE_CONSOLE
+	help
+	  Driver for the ifxmipss built in ASC hardware
+
 config SERIAL_QE
 	tristate "Freescale QUICC Engine serial port support"
 	depends on QUICC_ENGINE
--- a/drivers/serial/Makefile
+++ b/drivers/serial/Makefile
@@ -82,3 +82,4 @@ obj-$(CONFIG_KGDB_SERIAL_CONSOLE) += kgd
 obj-$(CONFIG_SERIAL_QE) += ucc_uart.o
 obj-$(CONFIG_SERIAL_TIMBERDALE)	+= timbuart.o
 obj-$(CONFIG_SERIAL_GRLIB_GAISLER_APBUART) += apbuart.o
+obj-$(CONFIG_SERIAL_IFXMIPS) += ifxmips.o
--- a/drivers/net/Kconfig
+++ b/drivers/net/Kconfig
@@ -343,6 +343,12 @@ config MACB
 
 source "drivers/net/arm/Kconfig"
 
+config IFXMIPS_MII0
+	tristate "Infineon IFXMips eth0 driver"
+	depends on IFXMIPS
+	help
+	  Support for the MII0 inside the IFXMips SOC
+
 config AX88796
 	tristate "ASIX AX88796 NE2000 clone support"
 	depends on ARM || MIPS || SUPERH
--- a/drivers/net/Makefile
+++ b/drivers/net/Makefile
@@ -247,6 +247,7 @@ pasemi_mac_driver-objs := pasemi_mac.o p
 obj-$(CONFIG_MLX4_CORE) += mlx4/
 obj-$(CONFIG_ENC28J60) += enc28j60.o
 obj-$(CONFIG_ETHOC) += ethoc.o
+obj-$(CONFIG_IFXMIPS_MII0) += ifxmips.o
 
 obj-$(CONFIG_XTENSA_XT2000_SONIC) += xtsonic.o
 
--- a/drivers/mtd/maps/Kconfig
+++ b/drivers/mtd/maps/Kconfig
@@ -257,6 +257,12 @@ config MTD_ALCHEMY
 	help
 	  Flash memory access on AMD Alchemy Pb/Db/RDK Reference Boards
 
+config MTD_IFXMIPS
+	tristate "IFXMIPS MTD support"
+	depends on IFXMIPS
+	help
+	  Flash memory access on AMD Alchemy Pb/Db/RDK Reference Boards
+
 config MTD_DILNETPC
 	tristate "CFI Flash device mapped on DIL/Net PC"
 	depends on X86 && MTD_CONCAT && MTD_PARTITIONS && MTD_CFI_INTELEXT && BROKEN
--- a/drivers/mtd/maps/Makefile
+++ b/drivers/mtd/maps/Makefile
@@ -61,3 +61,4 @@ obj-$(CONFIG_MTD_BFIN_ASYNC)	+= bfin-asy
 obj-$(CONFIG_MTD_RBTX4939)	+= rbtx4939-flash.o
 obj-$(CONFIG_MTD_VMU)		+= vmu-flash.o
 obj-$(CONFIG_MTD_GPIO_ADDR)	+= gpio-addr-flash.o
+obj-$(CONFIG_MTD_IFXMIPS)  += ifxmips.o
--- a/drivers/watchdog/Kconfig
+++ b/drivers/watchdog/Kconfig
@@ -840,6 +840,12 @@ config TXX9_WDT
 	help
 	  Hardware driver for the built-in watchdog timer on TXx9 MIPS SoCs.
 
+config IFXMIPS_WDT
+	bool "IFXMips watchdog"
+	depends on IFXMIPS
+	help
+	  Hardware driver for the IFXMIPS Watchdog Timer.
+
 # PARISC Architecture
 
 # POWERPC Architecture
--- a/drivers/watchdog/Makefile
+++ b/drivers/watchdog/Makefile
@@ -112,6 +112,7 @@ obj-$(CONFIG_PNX833X_WDT) += pnx833x_wdt
 obj-$(CONFIG_SIBYTE_WDOG) += sb_wdog.o
 obj-$(CONFIG_AR7_WDT) += ar7_wdt.o
 obj-$(CONFIG_TXX9_WDT) += txx9wdt.o
+obj-$(CONFIG_IFXMIPS_WDT) += ifxmips.o
 
 # PARISC Architecture
 
--- a/drivers/leds/Kconfig
+++ b/drivers/leds/Kconfig
@@ -269,6 +269,12 @@ config LEDS_ADP5520
 	  To compile this driver as a module, choose M here: the module will
 	  be called leds-adp5520.
 
+config LEDS_IFXMIPS
+	tristate "LED Support for IFXMIPS  LEDs"
+	depends on LEDS_CLASS && IFXMIPS
+	help
+	  This option enables support for the CM-X270 LEDs.
+
 comment "LED Triggers"
 
 config LEDS_TRIGGERS
--- a/drivers/leds/Makefile
+++ b/drivers/leds/Makefile
@@ -33,6 +33,7 @@ obj-$(CONFIG_LEDS_REGULATOR)		+= leds-re
 obj-$(CONFIG_LEDS_INTEL_SS4200)		+= leds-ss4200.o
 obj-$(CONFIG_LEDS_LT3593)		+= leds-lt3593.o
 obj-$(CONFIG_LEDS_ADP5520)		+= leds-adp5520.o
+obj-$(CONFIG_LEDS_IFXMIPS)		+= leds-ifxmips.o
 
 # LED SPI Drivers
 obj-$(CONFIG_LEDS_DAC124S085)		+= leds-dac124s085.o
