--- a/drivers/net/r6040.c
+++ b/drivers/net/r6040.c
@@ -45,6 +45,7 @@
 #include <linux/io.h>
 #include <linux/irq.h>
 #include <linux/uaccess.h>
+#include <linux/phy.h>
 
 #include <asm/processor.h>
 
@@ -180,7 +181,6 @@ struct r6040_descriptor {
 
 struct r6040_private {
 	spinlock_t lock;		/* driver lock */
-	struct timer_list timer;
 	struct pci_dev *pdev;
 	struct r6040_descriptor *rx_insert_ptr;
 	struct r6040_descriptor *rx_remove_ptr;
@@ -190,13 +190,15 @@ struct r6040_private {
 	struct r6040_descriptor *tx_ring;
 	dma_addr_t rx_ring_dma;
 	dma_addr_t tx_ring_dma;
-	u16	tx_free_desc, phy_addr, phy_mode;
+	u16	tx_free_desc, phy_addr;
 	u16	mcr0, mcr1;
-	u16	switch_sig;
 	struct net_device *dev;
-	struct mii_if_info mii_if;
+	struct mii_bus *mii_bus;
 	struct napi_struct napi;
 	void __iomem *base;
+	struct phy_device *phydev;
+	int old_link;
+	int old_duplex;
 };
 
 static char version[] __devinitdata = KERN_INFO DRV_NAME
@@ -239,20 +241,29 @@ static void r6040_phy_write(void __iomem
 	}
 }
 
-static int r6040_mdio_read(struct net_device *dev, int mii_id, int reg)
+static int r6040_mdiobus_read(struct mii_bus *bus, int phy_addr, int reg)
 {
+	struct net_device *dev = bus->priv;
 	struct r6040_private *lp = netdev_priv(dev);
 	void __iomem *ioaddr = lp->base;
 
-	return (r6040_phy_read(ioaddr, lp->phy_addr, reg));
+	return r6040_phy_read(ioaddr, phy_addr, reg);
 }
 
-static void r6040_mdio_write(struct net_device *dev, int mii_id, int reg, int val)
+static int r6040_mdiobus_write(struct mii_bus *bus, int phy_addr, int reg, u16 value)
 {
+	struct net_device *dev = bus->priv;
 	struct r6040_private *lp = netdev_priv(dev);
 	void __iomem *ioaddr = lp->base;
 
-	r6040_phy_write(ioaddr, lp->phy_addr, reg, val);
+	r6040_phy_write(ioaddr, phy_addr, reg, value);
+
+	return 0;
+}
+
+static int r6040_mdiobus_reset(struct mii_bus *bus)
+{
+	return 0;
 }
 
 static void r6040_free_txbufs(struct net_device *dev)
@@ -409,10 +420,9 @@ static void r6040_tx_timeout(struct net_
 	void __iomem *ioaddr = priv->base;
 
 	printk(KERN_WARNING "%s: transmit timed out, int enable %4.4x "
-		"status %4.4x, PHY status %4.4x\n",
+		"status %4.4x\n",
 		dev->name, ioread16(ioaddr + MIER),
-		ioread16(ioaddr + MISR),
-		r6040_mdio_read(dev, priv->mii_if.phy_id, MII_BMSR));
+		ioread16(ioaddr + MISR));
 
 	dev->stats.tx_errors++;
 
@@ -464,9 +474,6 @@ static int r6040_close(struct net_device
 	struct r6040_private *lp = netdev_priv(dev);
 	struct pci_dev *pdev = lp->pdev;
 
-	/* deleted timer */
-	del_timer_sync(&lp->timer);
-
 	spin_lock_irq(&lp->lock);
 	napi_disable(&lp->napi);
 	netif_stop_queue(dev);
@@ -496,64 +503,14 @@ static int r6040_close(struct net_device
 	return 0;
 }
 
-/* Status of PHY CHIP */
-static int r6040_phy_mode_chk(struct net_device *dev)
-{
-	struct r6040_private *lp = netdev_priv(dev);
-	void __iomem *ioaddr = lp->base;
-	int phy_dat;
-
-	/* PHY Link Status Check */
-	phy_dat = r6040_phy_read(ioaddr, lp->phy_addr, 1);
-	if (!(phy_dat & 0x4))
-		phy_dat = 0x8000;	/* Link Failed, full duplex */
-
-	/* PHY Chip Auto-Negotiation Status */
-	phy_dat = r6040_phy_read(ioaddr, lp->phy_addr, 1);
-	if (phy_dat & 0x0020) {
-		/* Auto Negotiation Mode */
-		phy_dat = r6040_phy_read(ioaddr, lp->phy_addr, 5);
-		phy_dat &= r6040_phy_read(ioaddr, lp->phy_addr, 4);
-		if (phy_dat & 0x140)
-			/* Force full duplex */
-			phy_dat = 0x8000;
-		else
-			phy_dat = 0;
-	} else {
-		/* Force Mode */
-		phy_dat = r6040_phy_read(ioaddr, lp->phy_addr, 0);
-		if (phy_dat & 0x100)
-			phy_dat = 0x8000;
-		else
-			phy_dat = 0x0000;
-	}
-
-	return phy_dat;
-};
-
-static void r6040_set_carrier(struct mii_if_info *mii)
-{
-	if (r6040_phy_mode_chk(mii->dev)) {
-		/* autoneg is off: Link is always assumed to be up */
-		if (!netif_carrier_ok(mii->dev))
-			netif_carrier_on(mii->dev);
-	} else
-		r6040_phy_mode_chk(mii->dev);
-}
-
 static int r6040_ioctl(struct net_device *dev, struct ifreq *rq, int cmd)
 {
 	struct r6040_private *lp = netdev_priv(dev);
-	struct mii_ioctl_data *data = if_mii(rq);
-	int rc;
 
-	if (!netif_running(dev))
+	if (!lp->phydev)
 		return -EINVAL;
-	spin_lock_irq(&lp->lock);
-	rc = generic_mii_ioctl(&lp->mii_if, data, cmd, NULL);
-	spin_unlock_irq(&lp->lock);
-	r6040_set_carrier(&lp->mii_if);
-	return rc;
+
+	return phy_mii_ioctl(lp->phydev, if_mii(rq), cmd);
 }
 
 static int r6040_rx(struct net_device *dev, int limit)
@@ -752,26 +709,6 @@ static int r6040_up(struct net_device *d
 	if (ret)
 		return ret;
 
-	/* Read the PHY ID */
-	lp->switch_sig = r6040_phy_read(ioaddr, 0, 2);
-
-	if (lp->switch_sig  == ICPLUS_PHY_ID) {
-		r6040_phy_write(ioaddr, 29, 31, 0x175C); /* Enable registers */
-		lp->phy_mode = 0x8000;
-	} else {
-		/* PHY Mode Check */
-		r6040_phy_write(ioaddr, lp->phy_addr, 4, PHY_CAP);
-		r6040_phy_write(ioaddr, lp->phy_addr, 0, PHY_MODE);
-
-		if (PHY_MODE == 0x3100)
-			lp->phy_mode = r6040_phy_mode_chk(dev);
-		else
-			lp->phy_mode = (PHY_MODE & 0x0100) ? 0x8000:0x0;
-	}
-
-	/* Set duplex mode */
-	lp->mcr0 |= lp->phy_mode;
-
 	/* improve performance (by RDC guys) */
 	r6040_phy_write(ioaddr, 30, 17, (r6040_phy_read(ioaddr, 30, 17) | 0x4000));
 	r6040_phy_write(ioaddr, 30, 17, ~((~r6040_phy_read(ioaddr, 30, 17)) | 0x2000));
@@ -784,35 +721,6 @@ static int r6040_up(struct net_device *d
 	return 0;
 }
 
-/*
-  A periodic timer routine
-	Polling PHY Chip Link Status
-*/
-static void r6040_timer(unsigned long data)
-{
-	struct net_device *dev = (struct net_device *)data;
-	struct r6040_private *lp = netdev_priv(dev);
-	void __iomem *ioaddr = lp->base;
-	u16 phy_mode;
-
-	/* Polling PHY Chip Status */
-	if (PHY_MODE == 0x3100)
-		phy_mode = r6040_phy_mode_chk(dev);
-	else
-		phy_mode = (PHY_MODE & 0x0100) ? 0x8000:0x0;
-
-	if (phy_mode != lp->phy_mode) {
-		lp->phy_mode = phy_mode;
-		lp->mcr0 = (lp->mcr0 & 0x7fff) | phy_mode;
-		iowrite16(lp->mcr0, ioaddr);
-	}
-
-	/* Timer active again */
-	mod_timer(&lp->timer, round_jiffies(jiffies + HZ));
-
-	/* Check media */
-	mii_check_media(&lp->mii_if, 1, 1);
-}
 
 /* Read/set MAC address routines */
 static void r6040_mac_address(struct net_device *dev)
@@ -874,10 +782,6 @@ static int r6040_open(struct net_device 
 	napi_enable(&lp->napi);
 	netif_start_queue(dev);
 
-	/* set and active a timer process */
-	setup_timer(&lp->timer, r6040_timer, (unsigned long) dev);
-	if (lp->switch_sig != ICPLUS_PHY_ID)
-		mod_timer(&lp->timer, jiffies + HZ);
 	return 0;
 }
 
@@ -1020,40 +924,22 @@ static void netdev_get_drvinfo(struct ne
 static int netdev_get_settings(struct net_device *dev, struct ethtool_cmd *cmd)
 {
 	struct r6040_private *rp = netdev_priv(dev);
-	int rc;
-
-	spin_lock_irq(&rp->lock);
-	rc = mii_ethtool_gset(&rp->mii_if, cmd);
-	spin_unlock_irq(&rp->lock);
 
-	return rc;
+	return  phy_ethtool_gset(rp->phydev, cmd);
 }
 
 static int netdev_set_settings(struct net_device *dev, struct ethtool_cmd *cmd)
 {
 	struct r6040_private *rp = netdev_priv(dev);
-	int rc;
-
-	spin_lock_irq(&rp->lock);
-	rc = mii_ethtool_sset(&rp->mii_if, cmd);
-	spin_unlock_irq(&rp->lock);
-	r6040_set_carrier(&rp->mii_if);
-
-	return rc;
-}
-
-static u32 netdev_get_link(struct net_device *dev)
-{
-	struct r6040_private *rp = netdev_priv(dev);
 
-	return mii_link_ok(&rp->mii_if);
+	return phy_ethtool_sset(rp->phydev, cmd);
 }
 
 static const struct ethtool_ops netdev_ethtool_ops = {
 	.get_drvinfo		= netdev_get_drvinfo,
 	.get_settings		= netdev_get_settings,
 	.set_settings		= netdev_set_settings,
-	.get_link		= netdev_get_link,
+	.get_link		= ethtool_op_get_link,
 };
 
 static const struct net_device_ops r6040_netdev_ops = {
@@ -1072,6 +958,86 @@ static const struct net_device_ops r6040
 #endif
 };
 
+static void r6040_adjust_link(struct net_device *dev)
+{
+	struct r6040_private *lp = netdev_priv(dev);
+	struct phy_device *phydev = lp->phydev;
+	int status_changed = 0;
+	void __iomem *ioaddr = lp->base;
+
+	BUG_ON (!phydev);
+
+	if (lp->old_link != phydev->link) {
+		status_changed = 1;
+		lp->old_link = phydev->link;
+	}
+
+	/* reflect duplex change */
+	if (phydev->link && (lp->old_duplex != phydev->duplex)) {
+		lp->mcr0 |= (phydev->duplex == DUPLEX_FULL ? 0x8000 : 0);
+		iowrite16(lp->mcr0, ioaddr);
+
+		status_changed = 1;
+		lp->old_duplex = phydev->duplex;
+	}
+
+	if (status_changed) {
+		pr_info("%s: link %s", dev->name, phydev->link ?
+			"UP" : "DOWN");
+		if (phydev->link)
+			pr_cont(" - %d/%s", phydev->speed,
+                               DUPLEX_FULL == phydev->duplex ? "full" : "half");
+		pr_cont("\n");
+	}
+}
+
+static int r6040_mii_probe(struct net_device *dev)
+{
+	struct r6040_private *lp = netdev_priv(dev);
+	struct phy_device *phydev = NULL;
+	int phy_addr;
+
+	for (phy_addr = 0; phy_addr < PHY_MAX_ADDR; phy_addr++) {
+		if (lp->mii_bus->phy_map[phy_addr]) {
+			phydev = lp->mii_bus->phy_map[phy_addr];
+			break;
+		}
+	}
+
+	if (!phydev) {
+		printk(KERN_ERR DRV_NAME "no PHY found\n");
+		return -ENODEV;
+	}
+
+	phydev = phy_connect(dev, dev_name(&phydev->dev), &r6040_adjust_link,
+				0, PHY_INTERFACE_MODE_MII);
+
+	if (IS_ERR(phydev)) {
+		printk(KERN_ERR DRV_NAME "could not attach to PHY\n");
+		return PTR_ERR(phydev);
+	}
+
+	/* mask with MAC supported features */
+	phydev->supported &= (SUPPORTED_10baseT_Half
+				| SUPPORTED_10baseT_Full
+				| SUPPORTED_100baseT_Half
+				| SUPPORTED_100baseT_Full
+				| SUPPORTED_Autoneg
+				| SUPPORTED_MII
+				| SUPPORTED_TP);
+
+	phydev->advertising = phydev->supported;
+	lp->phydev = phydev;
+	lp->old_link = 0;
+	lp->old_duplex = -1;
+
+        printk(KERN_INFO "%s: attached PHY driver [%s] "
+               "(mii_bus:phy_addr=%s)\n", dev->name,
+               phydev->drv->name, dev_name(&phydev->dev));
+
+	return 0;
+}
+
 static int __devinit r6040_init_one(struct pci_dev *pdev,
 					 const struct pci_device_id *ent)
 {
@@ -1082,6 +1048,7 @@ static int __devinit r6040_init_one(stru
 	static int card_idx = -1;
 	int bar = 0;
 	u16 *adrp;
+	int i;
 
 	printk("%s\n", version);
 
@@ -1169,7 +1136,6 @@ static int __devinit r6040_init_one(stru
 	/* Init RDC private data */
 	lp->mcr0 = 0x1002;
 	lp->phy_addr = phy_table[card_idx];
-	lp->switch_sig = 0;
 
 	/* The RDC-specific entries in the device structure. */
 	dev->netdev_ops = &r6040_netdev_ops;
@@ -1177,28 +1143,61 @@ static int __devinit r6040_init_one(stru
 	dev->watchdog_timeo = TX_TIMEOUT;
 
 	netif_napi_add(dev, &lp->napi, r6040_poll, 64);
-	lp->mii_if.dev = dev;
-	lp->mii_if.mdio_read = r6040_mdio_read;
-	lp->mii_if.mdio_write = r6040_mdio_write;
-	lp->mii_if.phy_id = lp->phy_addr;
-	lp->mii_if.phy_id_mask = 0x1f;
-	lp->mii_if.reg_num_mask = 0x1f;
+
+	lp->mii_bus = mdiobus_alloc();
+	if (!lp->mii_bus) {
+		printk(KERN_ERR DRV_NAME ": mdiobus_alloc failed\n");
+		goto err_out_unmap;
+	}
+
+	lp->mii_bus->priv = dev;
+	lp->mii_bus->read = r6040_mdiobus_read;
+	lp->mii_bus->write = r6040_mdiobus_write;
+	lp->mii_bus->reset = r6040_mdiobus_reset;
+	lp->mii_bus->name = "r6040_eth_mii";
+	snprintf(lp->mii_bus->id, MII_BUS_ID_SIZE, "%x", card_idx);
+	lp->mii_bus->irq = kmalloc(sizeof(int)*PHY_MAX_ADDR, GFP_KERNEL);
+	if (!lp->mii_bus->irq) {
+		printk(KERN_ERR DRV_NAME ": allocation failed\n");
+		goto err_out_mdio;
+	}
+
+	for (i = 0; i < PHY_MAX_ADDR; i++)
+		lp->mii_bus->irq[i] = PHY_POLL;
+
+	err = mdiobus_register(lp->mii_bus);
+	if (err) {
+		printk(KERN_ERR DRV_NAME ": failed to register MII bus\n");
+		goto err_out_mdio_irq;
+	}
+
+	err = r6040_mii_probe(dev);
+	if (err) {
+		printk(KERN_ERR DRV_NAME ": failed to probe MII bus\n");
+		goto err_out_mdio_unregister;
+	}
 
 	/* Check the vendor ID on the PHY, if 0xffff assume none attached */
 	if (r6040_phy_read(ioaddr, lp->phy_addr, 2) == 0xffff) {
 		printk(KERN_ERR DRV_NAME ": Failed to detect an attached PHY\n");
 		err = -ENODEV;
-		goto err_out_unmap;
+		goto err_out_mdio_unregister;
 	}
 
 	/* Register net device. After this dev->name assign */
 	err = register_netdev(dev);
 	if (err) {
 		printk(KERN_ERR DRV_NAME ": Failed to register net device\n");
-		goto err_out_unmap;
+		goto err_out_mdio_unregister;
 	}
 	return 0;
 
+err_out_mdio_unregister:
+	mdiobus_unregister(lp->mii_bus);
+err_out_mdio_irq:
+	kfree(lp->mii_bus->irq);
+err_out_mdio:
+	mdiobus_free(lp->mii_bus);
 err_out_unmap:
 	pci_iounmap(pdev, ioaddr);
 err_out_free_res:
@@ -1212,8 +1211,12 @@ err_out:
 static void __devexit r6040_remove_one(struct pci_dev *pdev)
 {
 	struct net_device *dev = pci_get_drvdata(pdev);
+	struct r6040_private *lp = netdev_priv(dev);
 
 	unregister_netdev(dev);
+	mdiobus_unregister(lp->mii_bus);
+	kfree(lp->mii_bus->irq);
+	mdiobus_free(lp->mii_bus);
 	pci_release_regions(pdev);
 	free_netdev(dev);
 	pci_disable_device(pdev);
