---
 arch/arm/mach-omap1/board-nokia770.c |   16 +
 arch/arm/mach-omap2/Kconfig          |   10 +
 arch/arm/mach-omap2/Makefile         |    2 
 arch/arm/mach-omap2/board-n8x0-lcd.c |  127 +++++++++++++
 arch/arm/mach-omap2/board-n8x0-usb.c |  175 +++++++++++++++++++
 arch/arm/mach-omap2/board-n8x0.c     |  319 +++++++++++++++++++++++++----------
 arch/arm/mach-omap2/control.c        |    2 
 arch/arm/mach-omap2/serial.c         |    8 
 8 files changed, 569 insertions(+), 90 deletions(-)

--- linux-2.6.35.3.orig/arch/arm/mach-omap1/board-nokia770.c
+++ linux-2.6.35.3/arch/arm/mach-omap1/board-nokia770.c
@@ -37,6 +37,7 @@
 #include <plat/lcd_mipid.h>
 #include <plat/mmc.h>
 #include <plat/clock.h>
+#include <plat/cbus.h>
 
 #define ADS7846_PENDOWN_GPIO	15
 
@@ -96,8 +97,23 @@ static struct platform_device nokia770_k
 	.resource	= nokia770_kp_resources,
 };
 
+static struct cbus_host_platform_data nokia770_cbus_data = {
+	.clk_gpio	= OMAP_MPUIO(11),
+	.dat_gpio	= OMAP_MPUIO(10),
+	.sel_gpio	= OMAP_MPUIO(9),
+};
+
+static struct platform_device nokia770_cbus_device = {
+	.name		= "cbus",
+	.id		= -1,
+	.dev		= {
+		.platform_data = &nokia770_cbus_data,
+	},
+};
+
 static struct platform_device *nokia770_devices[] __initdata = {
 	&nokia770_kp_device,
+	&nokia770_cbus_device,
 };
 
 static void mipid_shutdown(struct mipid_platform_data *pdata)
--- linux-2.6.35.3.orig/arch/arm/mach-omap2/board-n8x0.c
+++ linux-2.6.35.3/arch/arm/mach-omap2/board-n8x0.c
@@ -18,8 +18,12 @@
 #include <linux/io.h>
 #include <linux/stddef.h>
 #include <linux/i2c.h>
+#include <linux/platform_device.h>
 #include <linux/spi/spi.h>
+#include <linux/spi/tsc2005.h>
+#include <linux/input.h>
 #include <linux/usb/musb.h>
+#include <linux/i2c/lm8323.h>
 
 #include <asm/mach/arch.h>
 #include <asm/mach-types.h>
@@ -32,114 +36,156 @@
 #include <plat/onenand.h>
 #include <plat/mmc.h>
 #include <plat/serial.h>
+#include <plat/cbus.h>
 
-static int slot1_cover_open;
-static int slot2_cover_open;
-static struct device *mmc_device;
+#define	RX51_TSC2005_RESET_GPIO	94
+#define	RX51_TSC2005_IRQ_GPIO	106
+#define OMAP_TAG_NOKIA_BT	0x4e01
+
+static s16 rx44_keymap[LM8323_KEYMAP_SIZE] = {
+	[0x01] = KEY_Q,
+	[0x02] = KEY_K,
+	[0x03] = KEY_O,
+	[0x04] = KEY_P,
+	[0x05] = KEY_BACKSPACE,
+	[0x06] = KEY_A,
+	[0x07] = KEY_S,
+	[0x08] = KEY_D,
+	[0x09] = KEY_F,
+	[0x0a] = KEY_G,
+	[0x0b] = KEY_H,
+	[0x0c] = KEY_J,
+
+	[0x11] = KEY_W,
+	[0x12] = KEY_F4,
+	[0x13] = KEY_L,
+	[0x14] = KEY_APOSTROPHE,
+	[0x16] = KEY_Z,
+	[0x17] = KEY_X,
+	[0x18] = KEY_C,
+	[0x19] = KEY_V,
+	[0x1a] = KEY_B,
+	[0x1b] = KEY_N,
+	[0x1c] = KEY_LEFTSHIFT, /* Actually, this is both shift keys */
+	[0x1f] = KEY_F7,
+
+	[0x21] = KEY_E,
+	[0x22] = KEY_SEMICOLON,
+	[0x23] = KEY_MINUS,
+	[0x24] = KEY_EQUAL,
+	[0x2b] = KEY_FN,
+	[0x2c] = KEY_M,
+	[0x2f] = KEY_F8,
+
+	[0x31] = KEY_R,
+	[0x32] = KEY_RIGHTCTRL,
+	[0x34] = KEY_SPACE,
+	[0x35] = KEY_COMMA,
+	[0x37] = KEY_UP,
+	[0x3c] = KEY_COMPOSE,
+	[0x3f] = KEY_F6,
+
+	[0x41] = KEY_T,
+	[0x44] = KEY_DOT,
+	[0x46] = KEY_RIGHT,
+	[0x4f] = KEY_F5,
+	[0x51] = KEY_Y,
+	[0x53] = KEY_DOWN,
+	[0x55] = KEY_ENTER,
+	[0x5f] = KEY_ESC,
 
-#define TUSB6010_ASYNC_CS	1
-#define TUSB6010_SYNC_CS	4
-#define TUSB6010_GPIO_INT	58
-#define TUSB6010_GPIO_ENABLE	0
-#define TUSB6010_DMACHAN	0x3f
+	[0x61] = KEY_U,
+	[0x64] = KEY_LEFT,
 
-#if defined(CONFIG_USB_TUSB6010) || \
-	defined(CONFIG_USB_TUSB6010_MODULE)
-/*
- * Enable or disable power to TUSB6010. When enabling, turn on 3.3 V and
- * 1.5 V voltage regulators of PM companion chip. Companion chip will then
- * provide then PGOOD signal to TUSB6010 which will release it from reset.
- */
-static int tusb_set_power(int state)
-{
-	int i, retval = 0;
+	[0x71] = KEY_I,
+	[0x75] = KEY_KPENTER,
+};
 
-	if (state) {
-		gpio_set_value(TUSB6010_GPIO_ENABLE, 1);
-		msleep(1);
+static struct lm8323_platform_data lm8323_pdata = {
+	.repeat		= 0, /* Repeat is handled in userspace for now. */
+	.keymap		= rx44_keymap,
+	.size_x		= 8,
+	.size_y		= 12,
+	.debounce_time	= 12,
+	.active_time	= 500,
+
+	.name		= "Internal keyboard",
+	.pwm_names[0] 	= "n810::keyboard",
+	.pwm_names[1] 	= "n810::cover",
+	//.pwm1_name	= "n810::keyboard",
+	//.pwm2_name	= "n810::cover",
+};
 
-		/* Wait until TUSB6010 pulls INT pin down */
-		i = 100;
-		while (i && gpio_get_value(TUSB6010_GPIO_INT)) {
-			msleep(1);
-			i--;
-		}
+struct omap_bluetooth_config {
+	u8    chip_type;
+	u8    bt_wakeup_gpio;
+	u8    host_wakeup_gpio;
+	u8    reset_gpio;
+	u8    bt_uart;
+	u8    bd_addr[6];
+	u8    bt_sysclk;
+};
 
-		if (!i) {
-			printk(KERN_ERR "tusb: powerup failed\n");
-			retval = -ENODEV;
-		}
-	} else {
-		gpio_set_value(TUSB6010_GPIO_ENABLE, 0);
-		msleep(10);
-	}
+static struct platform_device n8x0_bt_device = {
+	.name           = "hci_h4p",
+	.id             = -1,
+	.num_resources  = 0,
+};
+
+void __init n8x0_bt_init(void)
+{
+	const struct omap_bluetooth_config *bt_config;
 
-	return retval;
+	bt_config = (void *) omap_get_config(OMAP_TAG_NOKIA_BT,
+					     struct omap_bluetooth_config);
+	n8x0_bt_device.dev.platform_data = (void *) bt_config;
+	if (platform_device_register(&n8x0_bt_device) < 0)
+		BUG();
 }
 
-static struct musb_hdrc_config musb_config = {
-	.multipoint	= 1,
-	.dyn_fifo	= 1,
-	.num_eps	= 16,
-	.ram_bits	= 12,
+static struct omap2_mcspi_device_config mipid_mcspi_config = {
+	.turbo_mode	= 0,
+	.single_channel	= 1,
 };
 
-static struct musb_hdrc_platform_data tusb_data = {
-#if defined(CONFIG_USB_MUSB_OTG)
-	.mode		= MUSB_OTG,
-#elif defined(CONFIG_USB_MUSB_PERIPHERAL)
-	.mode		= MUSB_PERIPHERAL,
-#else /* defined(CONFIG_USB_MUSB_HOST) */
-	.mode		= MUSB_HOST,
-#endif
-	.set_power	= tusb_set_power,
-	.min_power	= 25,	/* x2 = 50 mA drawn from VBUS as peripheral */
-	.power		= 100,	/* Max 100 mA VBUS for host mode */
-	.config		= &musb_config,
-};
-
-static void __init n8x0_usb_init(void)
-{
-	int ret = 0;
-	static char	announce[] __initdata = KERN_INFO "TUSB 6010\n";
-
-	/* PM companion chip power control pin */
-	ret = gpio_request(TUSB6010_GPIO_ENABLE, "TUSB6010 enable");
-	if (ret != 0) {
-		printk(KERN_ERR "Could not get TUSB power GPIO%i\n",
-		       TUSB6010_GPIO_ENABLE);
-		return;
-	}
-	gpio_direction_output(TUSB6010_GPIO_ENABLE, 0);
-
-	tusb_set_power(0);
+static int slot1_cover_open;
+static int slot2_cover_open;
+static struct device *mmc_device;
 
-	ret = tusb6010_setup_interface(&tusb_data, TUSB6010_REFCLK_19, 2,
-					TUSB6010_ASYNC_CS, TUSB6010_SYNC_CS,
-					TUSB6010_GPIO_INT, TUSB6010_DMACHAN);
-	if (ret != 0)
-		goto err;
 
-	printk(announce);
+static struct omap2_mcspi_device_config p54spi_mcspi_config = {
+	.turbo_mode	= 0,
+	.single_channel = 1,
+};
 
-	return;
+#ifdef CONFIG_MACH_NOKIA_N8X0_LCD
+extern struct mipid_platform_data n8x0_mipid_platform_data;
+#endif
 
-err:
-	gpio_free(TUSB6010_GPIO_ENABLE);
+#ifdef CONFIG_TOUCHSCREEN_TSC2005
+static struct tsc2005_platform_data tsc2005_config;
+static void rx51_tsc2005_set_reset(bool enable)
+{
+	gpio_set_value(RX51_TSC2005_RESET_GPIO, enable);
 }
-#else
-
-static void __init n8x0_usb_init(void) {}
-
-#endif /*CONFIG_USB_TUSB6010 */
 
-
-static struct omap2_mcspi_device_config p54spi_mcspi_config = {
+static struct omap2_mcspi_device_config tsc2005_mcspi_config = {
 	.turbo_mode	= 0,
 	.single_channel = 1,
 };
+#endif
 
 static struct spi_board_info n800_spi_board_info[] __initdata = {
+#ifdef CONFIG_MACH_NOKIA_N8X0_LCD
+	{
+		.modalias	= "lcd_mipid",
+		.bus_num	= 1,
+		.chip_select	= 1,
+		.max_speed_hz	= 4000000,
+		.controller_data= &mipid_mcspi_config,
+		.platform_data	= &n8x0_mipid_platform_data,
+	},
+#endif
 	{
 		.modalias	= "p54spi",
 		.bus_num	= 2,
@@ -147,6 +193,68 @@ static struct spi_board_info n800_spi_bo
 		.max_speed_hz   = 48000000,
 		.controller_data = &p54spi_mcspi_config,
 	},
+	{
+		.modalias	 = "tsc2005",
+		.bus_num	 = 1,
+		.chip_select	 = 0,
+		.irq		 = OMAP_GPIO_IRQ(RX51_TSC2005_IRQ_GPIO),
+		.max_speed_hz    = 6000000,
+		.controller_data = &tsc2005_mcspi_config,
+		.platform_data   = &tsc2005_config,
+	},
+};
+
+static void __init tsc2005_set_config(void)
+{
+	const struct omap_lcd_config *conf;
+
+	conf = omap_get_config(OMAP_TAG_LCD, struct omap_lcd_config);
+	if (conf != NULL) {
+#ifdef CONFIG_TOUCHSCREEN_TSC2005
+		if (strcmp(conf->panel_name, "lph8923") == 0) {
+			tsc2005_config.ts_x_plate_ohm = 180;
+			tsc2005_config.ts_hw_avg = 0;
+			tsc2005_config.ts_ignore_last = 0;
+			tsc2005_config.ts_touch_pressure = 1500;
+			tsc2005_config.ts_stab_time = 100;
+			tsc2005_config.ts_pressure_max = 2048;
+			tsc2005_config.ts_pressure_fudge = 2;
+			tsc2005_config.ts_x_max = 4096;
+			tsc2005_config.ts_x_fudge = 4;
+			tsc2005_config.ts_y_max = 4096;
+			tsc2005_config.ts_y_fudge = 7;
+			tsc2005_config.set_reset = rx51_tsc2005_set_reset;
+		} else if (strcmp(conf->panel_name, "ls041y3") == 0) {
+			tsc2005_config.ts_x_plate_ohm = 280;
+			tsc2005_config.ts_hw_avg = 0;
+			tsc2005_config.ts_ignore_last = 0;
+			tsc2005_config.ts_touch_pressure = 1500;
+			tsc2005_config.ts_stab_time = 1000;
+			tsc2005_config.ts_pressure_max = 2048;
+			tsc2005_config.ts_pressure_fudge = 2;
+			tsc2005_config.ts_x_max = 4096;
+			tsc2005_config.ts_x_fudge = 4;
+			tsc2005_config.ts_y_max = 4096;
+			tsc2005_config.ts_y_fudge = 7;
+			tsc2005_config.set_reset = rx51_tsc2005_set_reset;
+		} else {
+			printk(KERN_ERR "Unknown panel type, set default "
+			       "touchscreen configuration\n");
+			tsc2005_config.ts_x_plate_ohm = 200;
+			tsc2005_config.ts_stab_time = 100;
+		}
+#endif
+	}
+}
+
+static struct i2c_board_info __initdata_or_module n8x0_i2c_board_info_2[] = {};
+
+static struct i2c_board_info __initdata_or_module n810_i2c_board_info_2[] = {
+	{
+		I2C_BOARD_INFO("lm8323", 0x45),
+		.irq		= OMAP_GPIO_IRQ(109),
+		.platform_data	= &lm8323_pdata,
+	},
 };
 
 #if defined(CONFIG_MTD_ONENAND_OMAP2) || \
@@ -181,6 +289,20 @@ static struct mtd_partition onenand_part
 	},
 };
 
+static struct cbus_host_platform_data n8x0_cbus_data = {
+	.clk_gpio	= 66,
+	.dat_gpio	= 65,
+	.sel_gpio	= 64,
+};
+
+static struct platform_device n8x0_cbus_device = {
+	.name		= "cbus",
+	.id		= -1,
+	.dev		= {
+		.platform_data = &n8x0_cbus_data,
+	},
+};
+
 static struct omap_onenand_platform_data board_onenand_data = {
 	.cs		= 0,
 	.gpio_irq	= 26,
@@ -649,14 +771,39 @@ static void __init n8x0_init_irq(void)
 	omap_gpio_init();
 }
 
+#ifdef CONFIG_MACH_NOKIA_N8X0_LCD
+extern void n8x0_mipid_init(void);
+extern void n8x0_blizzard_init(void);
+#else
+#define n8x0_mipid_init() 0
+#define n8x0_blizzard_init() 0
+#endif
+
+extern void n8x0_usb_init(void);
+
 static void __init n8x0_init_machine(void)
 {
+	platform_device_register(&n8x0_cbus_device);
+
+	n8x0_bt_init();
+
 	/* FIXME: add n810 spi devices */
+	tsc2005_set_config();
 	spi_register_board_info(n800_spi_board_info,
 				ARRAY_SIZE(n800_spi_board_info));
 
 	omap_serial_init();
 	n8x0_menelaus_init();
+
+	omap_register_i2c_bus(2, 400, n8x0_i2c_board_info_2,
+			      ARRAY_SIZE(n8x0_i2c_board_info_2));
+
+	i2c_register_board_info(2, n810_i2c_board_info_2,
+				ARRAY_SIZE(n810_i2c_board_info_2));
+
+	n8x0_mipid_init();
+	n8x0_blizzard_init();
+
 	n8x0_onenand_init();
 	n8x0_mmc_init();
 	n8x0_usb_init();
--- /dev/null
+++ linux-2.6.35.3/arch/arm/mach-omap2/board-n8x0-lcd.c
@@ -0,0 +1,127 @@
+/*
+ * linux/arch/arm/mach-omap2/board-n8x0.c
+ *
+ * Copyright (C) 2005-2009 Nokia Corporation
+ * Author: Juha Yrjola <juha.yrjola@nokia.com>
+ *
+ * Modified from mach-omap2/board-generic.c
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+
+#include <linux/clk.h>
+#include <linux/delay.h>
+#include <linux/gpio.h>
+#include <linux/omapfb.h>
+
+#include <plat/lcd_mipid.h>
+#include <plat/blizzard.h>
+
+#include <../drivers/cbus/tahvo.h>
+
+#define N8X0_BLIZZARD_POWERDOWN_GPIO	15
+
+// MIPID LCD Panel
+
+static void mipid_shutdown(struct mipid_platform_data *pdata)
+{
+	if (pdata->nreset_gpio != -1) {
+		pr_info("shutdown LCD\n");
+		gpio_set_value(pdata->nreset_gpio, 0);
+		msleep(120);
+	}
+}
+
+struct mipid_platform_data n8x0_mipid_platform_data = {
+	.shutdown = mipid_shutdown,
+};
+
+void __init n8x0_mipid_init(void)
+{
+	const struct omap_lcd_config *conf;
+
+	conf = omap_get_config(OMAP_TAG_LCD, struct omap_lcd_config);
+	if (conf != NULL) {
+		n8x0_mipid_platform_data.nreset_gpio = conf->nreset_gpio;
+		n8x0_mipid_platform_data.data_lines = conf->data_lines;
+		printk(KERN_INFO "N8x0 MIPID config loaded");
+	}
+	else
+		printk(KERN_INFO "N8x0 MIPID config not provided");
+}
+
+
+// Epson Blizzard LCD Controller
+
+static struct {
+	struct clk *sys_ck;
+} blizzard;
+
+static int blizzard_get_clocks(void)
+{
+	blizzard.sys_ck = clk_get(0, "osc_ck");
+	if (IS_ERR(blizzard.sys_ck)) {
+		printk(KERN_ERR "can't get Blizzard clock\n");
+		return PTR_ERR(blizzard.sys_ck);
+	}
+	return 0;
+}
+
+static unsigned long blizzard_get_clock_rate(struct device *dev)
+{
+	return clk_get_rate(blizzard.sys_ck);
+}
+
+static void blizzard_enable_clocks(int enable)
+{
+	if (enable)
+		clk_enable(blizzard.sys_ck);
+	else
+		clk_disable(blizzard.sys_ck);
+}
+
+static void blizzard_power_up(struct device *dev)
+{
+	/* Vcore to 1.475V */
+	tahvo_set_clear_reg_bits(0x07, 0, 0xf);
+	msleep(10);
+
+	blizzard_enable_clocks(1);
+	gpio_set_value(N8X0_BLIZZARD_POWERDOWN_GPIO, 1);
+}
+
+static void blizzard_power_down(struct device *dev)
+{
+	gpio_set_value(N8X0_BLIZZARD_POWERDOWN_GPIO, 0);
+	blizzard_enable_clocks(0);
+
+	/* Vcore to 1.005V */
+	tahvo_set_clear_reg_bits(0x07, 0xf, 0);
+}
+
+static struct blizzard_platform_data n8x0_blizzard_data = {
+	.power_up	= blizzard_power_up,
+	.power_down	= blizzard_power_down,
+	.get_clock_rate	= blizzard_get_clock_rate,
+	.te_connected	= 1,
+};
+
+void __init n8x0_blizzard_init(void)
+{
+	int r;
+
+	r = gpio_request(N8X0_BLIZZARD_POWERDOWN_GPIO, "Blizzard pd");
+	if (r < 0)
+	{
+		printk(KERN_ERR "Can't get N8x0 Blizzard powerdown GPIO %d\n", N8X0_BLIZZARD_POWERDOWN_GPIO);
+		return;
+	}
+	gpio_direction_output(N8X0_BLIZZARD_POWERDOWN_GPIO, 1);
+
+	blizzard_get_clocks();
+	omapfb_set_ctrl_platform_data(&n8x0_blizzard_data);
+
+	printk(KERN_INFO "N8x0 Blizzard initialized");
+}
--- /dev/null
+++ linux-2.6.35.3/arch/arm/mach-omap2/board-n8x0-usb.c
@@ -0,0 +1,175 @@
+/*
+ * linux/arch/arm/mach-omap2/board-n8x0-usb.c
+ *
+ * Copyright (C) 2006 Nokia Corporation
+ * Author: Juha Yrjola
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+
+#include <linux/types.h>
+#include <linux/delay.h>
+#include <linux/platform_device.h>
+#include <linux/clk.h>
+#include <linux/err.h>
+#include <linux/gpio.h>
+#include <linux/usb/musb.h>
+
+#include <plat/gpmc.h>
+
+#define TUSB_ASYNC_CS		1
+#define TUSB_SYNC_CS		4
+#define GPIO_TUSB_INT		58
+#define GPIO_TUSB_ENABLE	0
+
+static int tusb_set_power(int state);
+static int tusb_set_clock(struct clk *osc_ck, int state);
+
+#if	defined(CONFIG_USB_MUSB_OTG)
+#	define BOARD_MODE	MUSB_OTG
+#elif	defined(CONFIG_USB_MUSB_PERIPHERAL)
+#	define BOARD_MODE	MUSB_PERIPHERAL
+#else	/* defined(CONFIG_USB_MUSB_HOST) */
+#	define BOARD_MODE	MUSB_HOST
+#endif
+
+static struct musb_hdrc_eps_bits musb_eps[] = {
+	{	"ep1_tx", 5,	},
+	{	"ep1_rx", 5,	},
+	{	"ep2_tx", 5,	},
+	{	"ep2_rx", 5,	},
+	{	"ep3_tx", 3,	},
+	{	"ep3_rx", 3,	},
+	{	"ep4_tx", 3,	},
+	{	"ep4_rx", 3,	},
+	{	"ep5_tx", 2,	},
+	{	"ep5_rx", 2,	},
+	{	"ep6_tx", 2,	},
+	{	"ep6_rx", 2,	},
+	{	"ep7_tx", 2,	},
+	{	"ep7_rx", 2,	},
+	{	"ep8_tx", 2,	},
+	{	"ep8_rx", 2,	},
+	{	"ep9_tx", 2,	},
+	{	"ep9_rx", 2,	},
+	{	"ep10_tx", 2,	},
+	{	"ep10_rx", 2,	},
+	{	"ep11_tx", 2,	},
+	{	"ep11_rx", 2,	},
+	{	"ep12_tx", 2,	},
+	{	"ep12_rx", 2,	},
+	{	"ep13_tx", 2,	},
+	{	"ep13_rx", 2,	},
+	{	"ep14_tx", 2,	},
+	{	"ep14_rx", 2,	},
+	{	"ep15_tx", 2,	},
+	{	"ep15_rx", 2,	},
+};
+
+static struct musb_hdrc_config musb_config = {
+	.multipoint	= 1,
+	.dyn_fifo	= 1,
+	.soft_con	= 1,
+	.dma		= 1,
+	.num_eps	= 16,
+	.dma_channels	= 7,
+	.ram_bits	= 12,
+	.eps_bits	= musb_eps,
+};
+
+static struct musb_hdrc_platform_data tusb_data = {
+	.mode		= BOARD_MODE,
+	.set_power	= tusb_set_power,
+	.set_clock	= tusb_set_clock,
+	.min_power	= 25,	/* x2 = 50 mA drawn from VBUS as peripheral */
+	.power		= 100,	/* Max 100 mA VBUS for host mode */
+	.clock		= "osc_ck",
+	.config		= &musb_config,
+};
+
+/*
+ * Enable or disable power to TUSB6010. When enabling, turn on 3.3 V and
+ * 1.5 V voltage regulators of PM companion chip. Companion chip will then
+ * provide then PGOOD signal to TUSB6010 which will release it from reset.
+ */
+static int tusb_set_power(int state)
+{
+	int i, retval = 0;
+
+	if (state) {
+		gpio_set_value(GPIO_TUSB_ENABLE, 1);
+		msleep(1);
+
+		/* Wait until TUSB6010 pulls INT pin down */
+		i = 100;
+		while (i && gpio_get_value(GPIO_TUSB_INT)) {
+			msleep(1);
+			i--;
+		}
+
+		if (!i) {
+			printk(KERN_ERR "tusb: powerup failed\n");
+			retval = -ENODEV;
+		}
+	} else {
+		gpio_set_value(GPIO_TUSB_ENABLE, 0);
+		msleep(10);
+	}
+
+	return retval;
+}
+
+static int		osc_ck_on;
+
+static int tusb_set_clock(struct clk *osc_ck, int state)
+{
+	if (state) {
+		if (osc_ck_on > 0)
+			return -ENODEV;
+
+		//omap2_block_sleep();
+		clk_enable(osc_ck);
+		osc_ck_on = 1;
+	} else {
+		if (osc_ck_on == 0)
+			return -ENODEV;
+
+		clk_disable(osc_ck);
+		osc_ck_on = 0;
+		//omap2_allow_sleep();
+	}
+
+	return 0;
+}
+
+void __init n8x0_usb_init(void)
+{
+	int ret = 0;
+	static char	announce[] __initdata = KERN_INFO "TUSB 6010\n";
+
+	/* PM companion chip power control pin */
+	ret = gpio_request(GPIO_TUSB_ENABLE, "TUSB6010 enable");
+	if (ret != 0) {
+		printk(KERN_ERR "Could not get TUSB power GPIO%i\n",
+		       GPIO_TUSB_ENABLE);
+		return;
+	}
+	gpio_direction_output(GPIO_TUSB_ENABLE, 0);
+
+	tusb_set_power(0);
+
+	ret = tusb6010_setup_interface(&tusb_data, TUSB6010_REFCLK_19, 2,
+					TUSB_ASYNC_CS, TUSB_SYNC_CS,
+					GPIO_TUSB_INT, 0x3f);
+	if (ret != 0)
+		goto err;
+
+	printk(announce);
+
+	return;
+
+err:
+	gpio_free(GPIO_TUSB_ENABLE);
+}
--- linux-2.6.35.3.orig/arch/arm/mach-omap2/control.c
+++ linux-2.6.35.3/arch/arm/mach-omap2/control.c
@@ -162,6 +162,7 @@ u16 omap_ctrl_readw(u16 offset)
 	return __raw_readw(OMAP_CTRL_REGADDR(offset));
 }
 
+EXPORT_SYMBOL_GPL(omap_ctrl_readl);
 u32 omap_ctrl_readl(u16 offset)
 {
 	return __raw_readl(OMAP_CTRL_REGADDR(offset));
@@ -177,6 +178,7 @@ void omap_ctrl_writew(u16 val, u16 offse
 	__raw_writew(val, OMAP_CTRL_REGADDR(offset));
 }
 
+EXPORT_SYMBOL_GPL(omap_ctrl_writel);
 void omap_ctrl_writel(u32 val, u16 offset)
 {
 	__raw_writel(val, OMAP_CTRL_REGADDR(offset));
--- linux-2.6.35.3.orig/arch/arm/mach-omap2/Kconfig
+++ linux-2.6.35.3/arch/arm/mach-omap2/Kconfig
@@ -116,6 +116,16 @@ config MACH_NOKIA_N8X0
 	select MACH_NOKIA_N810
 	select MACH_NOKIA_N810_WIMAX
 
+config MACH_NOKIA_N8X0_LCD
+	bool
+	depends on MACH_NOKIA_N8X0 && FB_OMAP_LCDC_BLIZZARD && FB_OMAP_LCD_MIPID
+	default y
+
+config MACH_NOKIA_N8X0_USB
+	bool
+	depends on MACH_NOKIA_N8X0 && MACH_OMAP2_TUSB6010
+	default y
+
 config MACH_NOKIA_RX51
 	bool "Nokia RX-51 board"
 	depends on ARCH_OMAP3
--- linux-2.6.35.3.orig/arch/arm/mach-omap2/Makefile
+++ linux-2.6.35.3/arch/arm/mach-omap2/Makefile
@@ -116,6 +116,8 @@ obj-$(CONFIG_MACH_OMAP_3430SDP)		+= boar
 					   hsmmc.o \
 					   board-sdp-flash.o
 obj-$(CONFIG_MACH_NOKIA_N8X0)		+= board-n8x0.o
+obj-$(CONFIG_MACH_NOKIA_N8X0_LCD)	+= board-n8x0-lcd.o
+obj-$(CONFIG_MACH_NOKIA_N8X0_USB)	+= board-n8x0-usb.o
 obj-$(CONFIG_MACH_NOKIA_RX51)		+= board-rx51.o \
 					   board-rx51-sdram.o \
 					   board-rx51-peripherals.o \
--- linux-2.6.35.3.orig/arch/arm/mach-omap2/serial.c
+++ linux-2.6.35.3/arch/arm/mach-omap2/serial.c
@@ -495,10 +495,10 @@ static void omap_uart_idle_init(struct o
 		uart->padconf = 0;
 	}
 
-	p->irqflags |= IRQF_SHARED;
+/*	p->irqflags |= IRQF_SHARED;
 	ret = request_irq(p->irq, omap_uart_interrupt, IRQF_SHARED,
 			  "serial idle", (void *)uart);
-	WARN_ON(ret);
+	WARN_ON(ret); */
 }
 
 void omap_uart_enable_irqs(int enable)
@@ -506,13 +506,13 @@ void omap_uart_enable_irqs(int enable)
 	int ret;
 	struct omap_uart_state *uart;
 
-	list_for_each_entry(uart, &uart_list, node) {
+/*	list_for_each_entry(uart, &uart_list, node) {
 		if (enable)
 			ret = request_irq(uart->p->irq, omap_uart_interrupt,
 				IRQF_SHARED, "serial idle", (void *)uart);
 		else
 			free_irq(uart->p->irq, (void *)uart);
-	}
+	} */
 }
 
 static ssize_t sleep_timeout_show(struct device *dev,
