# Device Usage Statistics Report

### Device Usage Page (usage_statistics_webtalk.html)

This HTML page displays the device usage statistics that will be sent to Xilinx.

Software Version and Target Device
Product Version: | ISE:12.2 (WebPack) - M.63c | Target Family: | Spartan3E
OS Platform: | LIN64 | Target Device: | xc3s500e
Project ID (random number) | c2aacd1c16a742efb7b16ebde1b15f3a.be534f09916d4e59b80fec647873aecc.1 | Target Package: | vq100
Registration ID | 0_0_674 | Target Speed: | -4
Date Generated | 2010-10-31T20:57:09 | Tool Flow | CommandLine

User Environment
OS Name | unknown | OS Release | unknown
CPU Name | Intel(R) Core(TM)2 Duo CPU T6670 @ 2.20GHz | CPU Speed | 2201.000 MHz

Device Usage Statistics
Macro Statistics | Miscellaneous Statistics | Net Statistics | Site Usage

MiscellaneousStatistics

- AGG_BONDED_IO=34
- AGG_IO=34
- AGG_SLICE=118
- NUM_4_INPUT_LUT=140
- NUM_BONDED_IBUF=22
- NUM_BONDED_IOB=12
- NUM_BUFGMUX=1
- NUM_CYMUX=74
- NUM_IOB_FF=27
- NUM_LUT_RT=28
- NUM_RAMB16=4
- NUM_SLICEL=118
- NUM_SLICE_FF=131
- NUM_XOR=48

NetStatistics

- NumNets_Active=311
- NumNets_Gnd=1
- NumNets_Vcc=1
- NumNodesOfType_Active_BRAMADDR=44
- NumNodesOfType_Active_BRAMDUMMY=70
- NumNodesOfType_Active_CLKPIN=99
- NumNodesOfType_Active_CNTRLPIN=71
- NumNodesOfType_Active_DOUBLE=712
- NumNodesOfType_Active_DUMMY=359
- NumNodesOfType_Active_DUMMYBANK=56
- NumNodesOfType_Active_DUMMYESC=4
- NumNodesOfType_Active_GLOBAL=42
- NumNodesOfType_Active_HFULLHEX=15
- NumNodesOfType_Active_HUNIHEX=93
- NumNodesOfType_Active_INPUT=590
- NumNodesOfType_Active_IOBOUTPUT=31
- NumNodesOfType_Active_OMUX=273
- NumNodesOfType_Active_OUTPUT=218
- NumNodesOfType_Active_PREBXBY=207
- NumNodesOfType_Active_VFULLHEX=41
- NumNodesOfType_Active_VLONG=3
- NumNodesOfType_Active_VUNIHEX=74
- NumNodesOfType_Gnd_BRAMADDR=22
- NumNodesOfType_Gnd_BRAMDUMMY=12
- NumNodesOfType_Gnd_DOUBLE=21
- NumNodesOfType_Gnd_DUMMYBANK=4
- NumNodesOfType_Gnd_INPUT=38
- NumNodesOfType_Gnd_OMUX=14
- NumNodesOfType_Gnd_OUTPUT=7
- NumNodesOfType_Gnd_PREBXBY=5
- NumNodesOfType_Vcc_BRAMDUMMY=4
- NumNodesOfType_Vcc_CNTRLPIN=1
- NumNodesOfType_Vcc_INPUT=9
- NumNodesOfType_Vcc_PREBXBY=5
- NumNodesOfType_Vcc_VCCOUT=8

SiteStatistics

- IBUF-DIFFM=8
- IBUF-DIFFMI=2
- IBUF-DIFFS=9
- IBUF-DIFFSI=1
- IBUF-IOB=1
- IOB-DIFFM=8
- IOB-DIFFS=4
- SLICEL-SLICEM=41

SiteSummary

- BUFGMUX=1
- BUFGMUX_GCLKMUX=1
- BUFGMUX_GCLK_BUFFER=1
- IBUF=22
- IBUF_IFD_DELAY=19
- IBUF_IFF1=19
- IBUF_INBUF=22
- IBUF_PAD=22
- IOB=12
- IOB_IFD_DELAY=8
- IOB_IFF1=8
- IOB_INBUF=8
- IOB_OUTBUF=12
- IOB_PAD=12
- RAMB16=4
- RAMB16_RAMB16=4
- RAMB16_RAMB16A=4
- RAMB16_RAMB16B=2
- SLICEL=118
- SLICEL_C1VDD=4
- SLICEL_CYMUXF=40
- SLICEL_CYMUXG=34
- SLICEL_F=76
- SLICEL_F5MUX=10
- SLICEL_FFX=65
- SLICEL_FFY=66
- SLICEL_G=64
- SLICEL_GNDF=12
- SLICEL_GNDG=12
- SLICEL_XORF=24
- SLICEL_XORG=24

Configuration Data

BUFGMUX

- S=[S_INV:1] [S:0]

BUFGMUX_GCLKMUX

- DISABLE_ATTR=[LOW:1]
- S=[S_INV:1] [S:0]

IBUF

- ICLK1=[ICLK1_INV:15] [ICLK1:4]

IBUF_IFF1

- CK=[CK:4] [CK_INV:15]
- IFF1_INIT_ATTR=[INIT0:19]
- LATCH_OR_FF=[FF:19]

IBUF_INBUF

- IFD_DELAY_VALUE=[DLY3:19]

IBUF_PAD

- IOATTRBOX=[LVCMOS25:22]

IOB

- ICLK1=[ICLK1_INV:8] [ICLK1:0]
- O1=[O1_INV:4] [O1:8]
- T1=[T1_INV:0] [T1:8]

IOB_IFF1

- CK=[CK:0] [CK_INV:8]
- IFF1_INIT_ATTR=[INIT0:8]
- LATCH_OR_FF=[FF:8]

IOB_INBUF

- IFD_DELAY_VALUE=[DLY3:8]

IOB_OUTBUF

- IN=[IN_INV:4] [IN:8]
- TRI=[TRI_INV:0] [TRI:8]

IOB_PAD

- DRIVEATTRBOX=[12:12]
- IOATTRBOX=[LVCMOS25:12]
- SLEW=[SLOW:12]

RAMB16

- CLKA=[CLKA_INV:4] [CLKA:0]
- CLKB=[CLKB_INV:2] [CLKB:0]
- ENA=[ENA_INV:0] [ENA:4]
- ENB=[ENB_INV:0] [ENB:2]
- SSRA=[SSRA_INV:0] [SSRA:4]
- SSRB=[SSRB_INV:0] [SSRB:2]
- WEA=[WEA:4] [WEA_INV:0]
- WEB=[WEB:2] [WEB_INV:0]

RAMB16_RAMB16A

- CLKA=[CLKA_INV:4] [CLKA:0]
- ENA=[ENA_INV:0] [ENA:4]
- PORTA_ATTR=[2048X9:4]
- SSRA=[SSRA_INV:0] [SSRA:4]
- WEA=[WEA:4] [WEA_INV:0]
- WRITEMODEA=[WRITE_FIRST:4]

RAMB16_RAMB16B

- CLKB=[CLKB_INV:2] [CLKB:0]
- ENB=[ENB_INV:0] [ENB:2]
- PORTB_ATTR=[2048X9:2]
- SSRB=[SSRB_INV:0] [SSRB:2]
- WEB=[WEB:2] [WEB_INV:0]
- WRITEMODEB=[WRITE_FIRST:2]

SLICEL

- BX=[BX_INV:0] [BX:60]
- BY=[BY:41] [BY_INV:0]
- CE=[CE:25] [CE_INV:0]
- CIN=[CIN_INV:0] [CIN:30]
- CLK=[CLK:49] [CLK_INV:17]
- SR=[SR:17] [SR_INV:21]

SLICEL_CYMUXF

- 0=[0:40] [0_INV:0]
- 1=[1_INV:0] [1:40]

SLICEL_CYMUXG

- 0=[0:34] [0_INV:0]

SLICEL_F5MUX

- S0=[S0:10] [S0_INV:0]

SLICEL_FFX

- CE=[CE:24] [CE_INV:0]
- CK=[CK:49] [CK_INV:16]
- D=[D:65] [D_INV:0]
- FFX_INIT_ATTR=[INIT0:65]
- FFX_SR_ATTR=[SRLOW:65]
- LATCH_OR_FF=[FF:65]
- SR=[SR:16] [SR_INV:21]
- SYNC_ATTR=[ASYNC:28] [SYNC:37]

SLICEL_FFY

- CE=[CE:25] [CE_INV:0]
- CK=[CK:49] [CK_INV:17]
- D=[D:66] [D_INV:0]
- FFY_INIT_ATTR=[INIT0:66]
- FFY_SR_ATTR=[SRLOW:66]
- LATCH_OR_FF=[FF:66]
- SR=[SR:17] [SR_INV:21]
- SYNC_ATTR=[ASYNC:28] [SYNC:38]

SLICEL_XORF

- 1=[1_INV:0] [1:24]

Pin Data

BUFGMUX

- I0=1
- O=1
- S=1

BUFGMUX_GCLKMUX

- I0=1
- OUT=1
- S=1

BUFGMUX_GCLK_BUFFER

- IN=1
- OUT=1

IBUF

- I=4
- ICLK1=19
- IQ1=19
- PAD=22

IBUF_IFD_DELAY

- IN=19
- OUT=19

IBUF_IFF1

- CK=19
- D=19
- Q=19

IBUF_INBUF

- IN=22
- OUT=22

IBUF_PAD

- PAD=22

IOB

- ICLK1=8
- IQ1=8
- O1=12
- PAD=12
- T1=8

IOB_IFD_DELAY

- IN=8
- OUT=8

IOB_IFF1

- CK=8
- D=8
- Q=8

IOB_INBUF

- IN=8
- OUT=8

IOB_OUTBUF

- IN=12
- OUT=12
- TRI=8

IOB_PAD

- PAD=12

RAMB16

- ADDRA10=4
- ADDRA11=4
- ADDRA12=4
- ADDRA13=4
- ADDRA3=4
- ADDRA4=4
- ADDRA5=4
- ADDRA6=4
- ADDRA7=4
- ADDRA8=4
- ADDRA9=4
- ADDRB10=2
- ADDRB11=2
- ADDRB12=2
- ADDRB13=2
- ADDRB3=2
- ADDRB4=2
- ADDRB5=2
- ADDRB6=2
- ADDRB7=2
- ADDRB8=2
- ADDRB9=2
- CLKA=4
- CLKB=2
- DIA0=2
- DIA1=2
- DIA2=2
- DIA3=2
- DIA4=2
- DIA5=2
- DIA6=2
- DIA7=2
- DIB0=2
- DIB1=2
- DIB2=2
- DIB3=2
- DIB4=2
- DIB5=2
- DIB6=2
- DIB7=2
- DIPA0=2
- DIPB0=2
- DOA0=4
- DOA1=4
- DOA2=4
- DOA3=4
- DOA4=4
- DOA5=4
- DOA6=4
- DOA7=4
- ENA=4
- ENB=2
- SSRA=4
- SSRB=2
- WEA=4
- WEB=2

RAMB16_RAMB16

- ADDRA=4
- ADDRB=2
- DIA=4
- DIB=2
- DOA=4
- DOB=2

RAMB16_RAMB16A

- ADDRA=4
- ADDRA10=4
- ADDRA11=4
- ADDRA12=4
- ADDRA13=4
- ADDRA3=4
- ADDRA4=4
- ADDRA5=4
- ADDRA6=4
- ADDRA7=4
- ADDRA8=4
- ADDRA9=4
- CLKA=4
- DIA=4
- DIA0=2
- DIA1=2
- DIA2=2
- DIA3=2
- DIA4=2
- DIA5=2
- DIA6=2
- DIA7=2
- DIPA0=2
- DOA=4
- DOA0=4
- DOA1=4
- DOA2=4
- DOA3=4
- DOA4=4
- DOA5=4
- DOA6=4
- DOA7=4
- ENA=4
- SSRA=4
- WEA=4

RAMB16_RAMB16B

- ADDRB=2
- ADDRB10=2
- ADDRB11=2
- ADDRB12=2
- ADDRB13=2
- ADDRB3=2
- ADDRB4=2
- ADDRB5=2
- ADDRB6=2
- ADDRB7=2
- ADDRB8=2
- ADDRB9=2
- CLKB=2
- DIB=2
- DIB0=2
- DIB1=2
- DIB2=2
- DIB3=2
- DIB4=2
- DIB5=2
- DIB6=2
- DIB7=2
- DIPB0=2
- DOB=2
- ENB=2
- SSRB=2
- WEB=2

SLICEL

- BX=60
- BY=41
- CE=25
- CIN=30
- CLK=66
- COUT=34
- F1=74
- F2=58
- F3=37
- F4=20
- G1=64
- G2=48
- G3=29
- G4=11
- SR=38
- X=35
- XQ=65
- Y=13
- YQ=66

SLICEL_C1VDD

- 1=4

SLICEL_CYMUXF

- 0=40
- 1=40
- OUT=40
- S0=40

SLICEL_CYMUXG

- 0=34
- 1=34
- OUT=34
- S0=34

SLICEL_F

- A1=74
- A2=58
- A3=37
- A4=20
- D=76

SLICEL_F5MUX

- F=10
- G=10
- OUT=10
- S0=10

SLICEL_FFX

- CE=24
- CK=65
- D=65
- Q=65
- SR=37

SLICEL_FFY

- CE=25
- CK=66
- D=66
- Q=66
- SR=38

SLICEL_G

- A1=64
- A2=48
- A3=29
- A4=11
- D=64

SLICEL_GNDF

- 0=12

SLICEL_GNDG

- 0=12

SLICEL_XORF

- 0=24
- 1=24
- O=24

SLICEL_XORG

- 0=24
- 1=24
- O=24

Software Quality
Run Statistics
bitgen | 94 | 94 | 0 | 0 | 0 | 0 | 0
map | 117 | 113 | 0 | 0 | 0 | 0 | 0
ngdbuild | 121 | 121 | 0 | 0 | 0 | 0 | 0
par | 112 | 112 | 0 | 0 | 0 | 0 | 0
trce | 112 | 112 | 0 | 0 | 0 | 0 | 0
xst | 214 | 211 | 0 | 0 | 0 | 0 | 0

Unisim Statistics
NGDBUILD_PRE_UNISIM_SUMMARY
NGDBUILD_NUM_BUFGP=1 | NGDBUILD_NUM_FD=44 | NGDBUILD_NUM_FDE=16 | NGDBUILD_NUM_FDR=42
NGDBUILD_NUM_FDRE_1=33 | NGDBUILD_NUM_FD_1=23 | NGDBUILD_NUM_GND=1 | NGDBUILD_NUM_IBUF=21
NGDBUILD_NUM_INV=10 | NGDBUILD_NUM_IOBUF=8 | NGDBUILD_NUM_LUT1=28 | NGDBUILD_NUM_LUT2=40
NGDBUILD_NUM_LUT3=35 | NGDBUILD_NUM_LUT4=31 | NGDBUILD_NUM_MUXCY=74 | NGDBUILD_NUM_MUXF5=10
NGDBUILD_NUM_OBUF=4 | NGDBUILD_NUM_RAMB16_S9=2 | NGDBUILD_NUM_RAMB16_S9_S9=2 | NGDBUILD_NUM_VCC=1
NGDBUILD_NUM_XORCY=48
NGDBUILD_POST_UNISIM_SUMMARY
NGDBUILD_NUM_BUFG=1 | NGDBUILD_NUM_FD=44 | NGDBUILD_NUM_FDE=16 | NGDBUILD_NUM_FDR=42
NGDBUILD_NUM_FDRE_1=33 | NGDBUILD_NUM_FD_1=23 | NGDBUILD_NUM_GND=1 | NGDBUILD_NUM_IBUF=29
NGDBUILD_NUM_IBUFG=1 | NGDBUILD_NUM_INV=10 | NGDBUILD_NUM_LUT1=28 | NGDBUILD_NUM_LUT2=40
NGDBUILD_NUM_LUT3=35 | NGDBUILD_NUM_LUT4=31 | NGDBUILD_NUM_MUXCY=74 | NGDBUILD_NUM_MUXF5=10
NGDBUILD_NUM_OBUF=4 | NGDBUILD_NUM_OBUFT=8 | NGDBUILD_NUM_RAMB16_S9=2 | NGDBUILD_NUM_RAMB16_S9_S9=2
NGDBUILD_NUM_VCC=1 | NGDBUILD_NUM_XORCY=48