Release 12.2 - par M.63c (lin64)
Copyright (c) 1995-2010 Xilinx, Inc.  All rights reserved.

Sun Oct 31 12:21:06 2010


# NOTE: This file is designed to be imported into a spreadsheet program
# such as Microsoft Excel for viewing, printing and sorting. The |
# character is used as the data field separator. This file is also designed
# to support parsing.
#
INPUT FILE:       project.ncd
OUTPUT FILE:      project_r.pad
PART TYPE:        xc3s500e
SPEED GRADE:      -4
PACKAGE:          vq100

Pinout by Pin Number:

-----|-----|-----|-----|-----|-----|-----|-----|-----|-----|-----|-----|-----|-----|-----|
Pin Number|Signal Name|Pin Usage|Pin Name|Direction|IO Standard|IO Bank Number|Drive (mA)|Slew Rate|Termination|IOB Delay|Voltage|Constraint|IO Register|Signal Integrity|
P1|||PROG_B||||||||||||
P2|addr<4>|IBUF|IO_L01P_3|INPUT|LVCMOS25*|3||||IFD||LOCATED|YES|NONE|
P3|addr<5>|IBUF|IO_L01N_3|INPUT|LVCMOS25*|3||||IFD||LOCATED|YES|NONE|
P4|sram_data<7>|IOB|IO_L02P_3|BIDIR|LVCMOS25*|3|12|SLOW|NONE**|IFD||LOCATED|YES|NONE|
P5|sram_data<6>|IOB|IO_L02N_3/VREF_3|BIDIR|LVCMOS25*|3|12|SLOW|NONE**|IFD||LOCATED|YES|NONE|
P6|||VCCINT||||||||1.2||||
P7|||GND||||||||||||
P8|||VCCO_3|||3|||||2.50||||
P9|sram_data<5>|IOB|IO_L03P_3/LHCLK0|BIDIR|LVCMOS25*|3|12|SLOW|NONE**|IFD||LOCATED|YES|NONE|
P10|sram_data<4>|IOB|IO_L03N_3/LHCLK1|BIDIR|LVCMOS25*|3|12|SLOW|NONE**|IFD||LOCATED|YES|NONE|
P11|sram_data<3>|IOB|IO_L04P_3/LHCLK2|BIDIR|LVCMOS25*|3|12|SLOW|NONE**|IFD||LOCATED|YES|NONE|
P12|sram_data<2>|IOB|IO_L04N_3/LHCLK3/IRDY2|BIDIR|LVCMOS25*|3|12|SLOW|NONE**|IFD||LOCATED|YES|NONE|
P13||IBUF|IP|UNUSED||3|||||||||
P14|||GND||||||||||||
P15|sram_data<1>|IOB|IO_L05P_3/LHCLK4/TRDY2|BIDIR|LVCMOS25*|3|12|SLOW|NONE**|IFD||LOCATED|YES|NONE|
P16|sram_data<0>|IOB|IO_L05N_3/LHCLK5|BIDIR|LVCMOS25*|3|12|SLOW|NONE**|IFD||LOCATED|YES|NONE|
P17||DIFFM|IO_L06P_3/LHCLK6|UNUSED||3|||||||||
P18||DIFFS|IO_L06N_3/LHCLK7|UNUSED||3|||||||||
P19|||GND||||||||||||
P20|||VCCO_3|||3|||||2.50||||
P21|||VCCAUX||||||||2.5||||
P22||DIFFM|IO_L07P_3|UNUSED||3|||||||||
P23||DIFFS|IO_L07N_3|UNUSED||3|||||||||
P24||DIFFM|IO_L01P_2/CSO_B|UNUSED||2|||||||||
P25||DIFFS|IO_L01N_2/INIT_B|UNUSED||2|||||||||
P26||DIFFM|IO_L02P_2/DOUT/BUSY|UNUSED||2|||||||||
P27||DIFFS|IO_L02N_2/MOSI/CSI_B|UNUSED||2|||||||||
P28|||VCCINT||||||||1.2||||
P29|||GND||||||||||||
P30|reset|IBUF|IP/VREF_2|INPUT|LVCMOS25*|2||||NONE||LOCATED|NO|NONE|
P31|||VCCO_2|||2|||||2.50||||
P32||DIFFM|IO_L03P_2/D7/GCLK12|UNUSED||2|||||||||
P33|quadD|IBUF|IO_L03N_2/D6/GCLK13|INPUT|LVCMOS25*|2||||IFD||LOCATED|YES|NONE|
P34|quadC|IBUF|IO/D5|INPUT|LVCMOS25*|2||||IFD||LOCATED|YES|NONE|
P35|quadB|IBUF|IO_L04P_2/D4/GCLK14|INPUT|LVCMOS25*|2||||IFD||LOCATED|YES|NONE|
P36|quadA|IBUF|IO_L04N_2/D3/GCLK15|INPUT|LVCMOS25*|2||||IFD||LOCATED|YES|NONE|
P37|||GND||||||||||||
P38|clk|IBUF|IP_L05P_2/RDWR_B/GCLK0|INPUT|LVCMOS25*|2||||NONE||LOCATED|NO|NONE|
P39||DIFFSI|IP_L05N_2/M2/GCLK1|UNUSED||2|||||||||
P40||DIFFM|IO_L06P_2/D2/GCLK2|UNUSED||2|||||||||
P41||DIFFS|IO_L06N_2/D1/GCLK3|UNUSED||2|||||||||
P42||IOB|IO/M1|UNUSED||2|||||||||
P43||DIFFM|IO_L07P_2/M0|UNUSED||2|||||||||
P44||DIFFS|IO_L07N_2/DIN/D0|UNUSED||2|||||||||
P45|||VCCO_2|||2|||||2.50||||
P46|||VCCAUX||||||||2.5||||
P47||DIFFM|IO_L08P_2/VS2|UNUSED||2|||||||||
P48||DIFFS|IO_L08N_2/VS1|UNUSED||2|||||||||
P49||DIFFM|IO_L09P_2/VS0|UNUSED||2|||||||||
P50||DIFFS|IO_L09N_2/CCLK|UNUSED||2|||||||||
P51|||DONE||||||||||||
P52|||GND||||||||||||
P53||DIFFM|IO_L01P_1|UNUSED||1|||||||||
P54||DIFFS|IO_L01N_1|UNUSED||1|||||||||
P55|||VCCO_1|||1|||||2.50||||
P56|||VCCINT||||||||1.2||||
P57||DIFFM|IO_L02P_1|UNUSED||1|||||||||
P58||DIFFS|IO_L02N_1|UNUSED||1|||||||||
P59|||GND||||||||||||
P60||DIFFM|IO_L03P_1/RHCLK0|UNUSED||1|||||||||
P61||DIFFS|IO_L03N_1/RHCLK1|UNUSED||1|||||||||
P62||DIFFM|IO_L04P_1/RHCLK2|UNUSED||1|||||||||
P63||DIFFS|IO_L04N_1/RHCLK3/TRDY1|UNUSED||1|||||||||
P64|||GND||||||||||||
P65||DIFFM|IO_L05P_1/RHCLK4/IRDY1|UNUSED||1|||||||||
P66|hbridge<0>|IOB|IO_L05N_1/RHCLK5|OUTPUT|LVCMOS25*|1|12|SLOW|NONE**|||LOCATED|NO|NONE|
P67||DIFFM|IO_L06P_1/RHCLK6|UNUSED||1|||||||||
P68|hbridge<1>|IOB|IO_L06N_1/RHCLK7|OUTPUT|LVCMOS25*|1|12|SLOW|NONE**|||LOCATED|NO|NONE|
P69|ncs|IBUF|IP/VREF_1|INPUT|LVCMOS25*|1||||IFD||LOCATED|YES|NONE|
P70|hbridge<2>|IOB|IO_L07P_1|OUTPUT|LVCMOS25*|1|12|SLOW|NONE**|||LOCATED|NO|NONE|
P71|hbridge<3>|IOB|IO_L07N_1|OUTPUT|LVCMOS25*|1|12|SLOW|NONE**|||LOCATED|NO|NONE|
P72|||GND||||||||||||
P73|||VCCO_1|||1|||||2.50||||
P74|||VCCAUX||||||||2.5||||
P75|||TMS||||||||||||
P76|||TDO||||||||||||
P77|||TCK||||||||||||
P78|addr<3>|IBUF|IO_L01P_0|INPUT|LVCMOS25*|0||||IFD||LOCATED|YES|NONE|
P79|addr<2>|IBUF|IO_L01N_0|INPUT|LVCMOS25*|0||||IFD||LOCATED|YES|NONE|
P80|||VCCINT||||||||1.2||||
P81|||GND||||||||||||
P82|||VCCO_0|||0|||||2.50||||
P83|addr<1>|IBUF|IO_L02P_0/GCLK4|INPUT|LVCMOS25*|0||||IFD||LOCATED|YES|NONE|
P84|addr<0>|IBUF|IO_L02N_0/GCLK5|INPUT|LVCMOS25*|0||||IFD||LOCATED|YES|NONE|
P85|addr<10>|IBUF|IO_L03P_0/GCLK6|INPUT|LVCMOS25*|0||||IFD||LOCATED|YES|NONE|
P86|noe|IBUF|IO_L03N_0/GCLK7|INPUT|LVCMOS25*|0||||NONE||LOCATED|NO|NONE|
P87|||GND||||||||||||
P88|nwe|IBUF|IP_L04P_0/GCLK8|INPUT|LVCMOS25*|0||||IFD||LOCATED|YES|NONE|
P89||DIFFSI|IP_L04N_0/GCLK9|UNUSED||0|||||||||
P90|addr<12>|IBUF|IO_L05P_0/GCLK10|INPUT|LVCMOS25*|0||||IFD||LOCATED|YES|NONE|
P91|addr<11>|IBUF|IO_L05N_0/GCLK11|INPUT|LVCMOS25*|0||||IFD||LOCATED|YES|NONE|
P92|addr<9>|IBUF|IO|INPUT|LVCMOS25*|0||||IFD||LOCATED|YES|NONE|
P93|||GND||||||||||||
P94|addr<8>|IBUF|IO_L06P_0|INPUT|LVCMOS25*|0||||IFD||LOCATED|YES|NONE|
P95|addr<7>|IBUF|IO_L06N_0/VREF_0|INPUT|LVCMOS25*|0||||IFD||LOCATED|YES|NONE|
P96|||VCCAUX||||||||2.5||||
P97|||VCCO_0|||0|||||2.50||||
P98|addr<6>|IBUF|IO_L07P_0|INPUT|LVCMOS25*|0||||IFD||LOCATED|YES|NONE|
P99||DIFFS|IO_L07N_0/HSWAP|UNUSED||0|||||||||
P100|||TDI||||||||||||

-----|-----|-----|-----|-----|-----|-----|-----|-----|-----|-----|-----|-----|-----|-----|

* Default value.
** This default Pullup/Pulldown value can be overridden in Bitgen. 
****** Special VCCO requirements may apply. Please consult the device 
       family datasheet for specific guideline on VCCO requirements. 


