#!/bin/sh

jtag -q <<EOF
cable milkymist
detect
instruction CFG_OUT  000100 BYPASS
instruction CFG_IN   000101 BYPASS
pld load fjmem.bit
initbus fjmem opcode=000010
frequency 6000000
detectflash 0
poke 0 0x90
peek 0x102
peek 0x104
peek 0x106
peek 0x108
peek 0x10a
peek 0x10c
peek 0x10e
peek 0x110
poke 0 0xff
EOF
