# Mappings for Faderfox LV3
#
# These mappings translate all controls of an LV3 with factory settings to
# channel 0. To do a factory reset, do this:
#
# - press and hold FX and Master for one second, until the LED above Shift
#   turns yello
# - press FX1 and FX2 together (near the joystick)
# - press and hold FX and Master until the yellow LED turns off
# - the LV3 will reset within a few seconds
#

#
# "Radio" buttons change the LED assignment and only emit a 127 for the
# function that's been activated, but never a 0. Pressing a button that's
# already on repeats it.
#
# The radio buttons also affect the channel the rotary decoders use.
#

c.24=c0.1	# Rotary encoders, turn, differential (without decay)
c.25=c0.2
c.26=c0.3
c.27=c0.4
c.28=c0.5	# Rotary encoders, push, toggle (with LED)
c.29=c0.6	# if shifted, push, tact (127/0)
c.30=c0.7
c.31=c0.8
c8.8=c0.9=8	# FX, push when off, radio (LED on)
c9.8=c0.9=9	# FX, push when on, radio (LED blinking)
c10.8=c0.9=10	# Master, push, radio (LED on)
c0.8=c0.9=0	# Black, push, buttons, radio
c1.8=c0.9=1
c2.8=c0.9=2
c3.8=c0.9=3
c4.8=c0.9=4
c5.8=c0.9=5
c6.8=c0.9=6
c7.8=c0.9=7
c0.22=c0.10	# Black + Shift, push, toggle (with LED)
c1.22=c0.11
c2.22=c0.12
c3.22=c0.13
c4.22=c0.14
c5.22=c0.15
c6.22=c0.16
c7.22=c0.17
# c0.18, c0.19 unused
c0.7=c0.20	# Faders
c1.7=c0.21
c2.7=c0.22
c3.7=c0.23
c4.7=c0.24
c5.7=c0.25
c6.7=c0.26
c7.7=c0.27
# c0.28, c0.29 unused
c0.16=c0.30	# Green buttons, push, tact (127/0)
c1.16=c0.31
c2.16=c0.32
c3.16=c0.33
c4.16=c0.34
c5.16=c0.35
c6.16=c0.36
c7.16=c0.37
c0.17=c0.38=0	# Blue buttons, push, tact (127 only)
c1.17=c0.38=1	# since we don't have pulsed buttons (yet), treat them as radio
c2.17=c0.38=2
c3.17=c0.38=3
c4.17=c0.38=4
c5.17=c0.38=5
c6.17=c0.38=6
c7.17=c0.38=7
# c0.39 unused
c0.18=c0.40	# Green + Shift, push, toggle (with LED)
c1.18=c0.41
c2.18=c0.42
c3.18=c0.43
c4.18=c0.44
c5.18=c0.45
c6.18=c0.47
c7.18=c0.48
# c0.48, c0.49 unused
c8.1=c0.50	# Left joystick, X
c8.2=c0.51	# Left joystick, Y
c8.4=c0.52	# FX1, push, toggle (with LED)
c8.5=c0.53	# FX1 + Shift, push, toggle (with LED)
# c0.54 unused
c9.1=c0.55	# Right joystick, X
c9.2=c0.56	# Right joystick, Y
c9.4=c0.57	# FX2, push, toggle (with LED)
c9.5=c0.58	# FX2 + Shift, push, toggle (with LED)
# c0.59 unused
c10.6=c0.60	# Scene, turn, differential (no decay)
c11.9=c0.61	# Scene + Shift
c10.3=c0.6	# Scene, push, tact (127/0)
# c10.0 is Scene + Shift, push, tact (127 only)

#
# MIDI In controls:
#
# c0.6			Scene display (0-99)
# c0.16 through c7.16	LEDs green buttons (0, non-zero)
# c0.17 through c7.17	LEDs blue buttons (0, non-zero)
# ...
#
