This patch moves MIDI message detection from higher layers to the MIDI
interrupt handler. This way, MIDI receivers only need to wake up once
per complete message and not for every single byte.

The /dev/midi queue size is changed from 64 bytes to 32 messages
(typically 3 bytes each).

Index: rtems/c/src/lib/libbsp/lm32/shared/milkymist_midi/midi.c
===================================================================
--- rtems.orig/c/src/lib/libbsp/lm32/shared/milkymist_midi/midi.c	2011-12-01 19:45:37.000000000 -0300
+++ rtems/c/src/lib/libbsp/lm32/shared/milkymist_midi/midi.c	2011-12-02 16:05:30.000000000 -0300
@@ -26,6 +26,8 @@
 #define DEVICE_NAME "/dev/midi"
 
 static rtems_id midi_q;
+static unsigned char *midi_p = NULL;
+static unsigned char midi_msg[3];
 
 static rtems_isr interrupt_handler(rtems_vector_number n)
 {
@@ -34,7 +36,23 @@
   while (MM_READ(MM_MIDI_STAT) & MIDI_STAT_RX_EVT) {
     msg = MM_READ(MM_MIDI_RXTX);
     MM_WRITE(MM_MIDI_STAT, MIDI_STAT_RX_EVT);
-    rtems_message_queue_send(midi_q, &msg, 1);
+
+    if ((msg & 0xf8) == 0xf8)
+      continue; /* ignore system real-time */
+
+    if (msg & 0x80)
+      midi_p = midi_msg; /* status byte */
+
+    if (!midi_p)
+      continue; /* ignore extra or unsynchronized data */
+
+    *midi_p++ = msg;
+
+    if (midi_p == midi_msg+3) {
+      /* received a complete MIDI message */
+      rtems_message_queue_send(midi_q, midi_msg, 3);
+      midi_p = NULL;
+    }
   }
   lm32_interrupt_ack(1 << MM_IRQ_MIDI);
 }
@@ -53,8 +71,8 @@
 
  sc = rtems_message_queue_create(
     rtems_build_name('M', 'I', 'D', 'I'),
-    64,
-    1,
+    32,
+    3,
     0,
     &midi_q
   );
