#!/bin/sh
#
# lockmost - lock standby, soc-rescue, bios-rescue, splash-rescue, and
#            flickernoise-rescue, but leave standby unlocked
#

jtag -q <<EOF
cable milkymist
detect
instruction CFG_OUT  000100 BYPASS
instruction CFG_IN   000101 BYPASS
pld load fjmem.bit
initbus fjmem opcode=000010
frequency 6000000
detectflash 0
endian big
lockflash 0xa0000 50
EOF
