|***************************************************************************
|T69M EBD Model for 240-Ball QCT PoP 14 x 14 x 0.80mm WFBGA
|Dual Die LP-DDR DRAM
| 
|Part Number      VDD/VDDQ  Architecture  Package
|-----------      --------  ------------  -------
|MT46H128M32L2MC  1.8/1.8V  128Mb x32     240-Ball QCT PoP
|
|***************************************************************************
|
[IBIS Ver]    4.0
[File name]   t69m_240b_2dp.ebd
[File rev]    1.0
[Date]        02/15/2010
[Source]      From SPICE model at Micron Technology, Inc.
                  Micron Technology, Inc.
                  8000 S. Federal Way
                  P.O. Box 6, M/S: 01-711
                  Boise, ID 83707-0006
              For support send e-mail to modelsupport@micron.com              
|
[Notes]       Rev 1.0: 02/15/2010
               - Initial revision of packaging ebd
|
              Notes:
               - U1, U2 are the LPDRAM bare die components
                 (MT46H64M32LFT69M_DS)defined in the IBIS file t69m.ibs
               - Please choose the appropriate speed grade and drive 
                 strength models from the bare die ibis components
               - In order to perform simulation using this model, 
                 *.ebd and *.ibs files must be in the same directory
|
[Disclaimer]  This software code and all associated documentation, comments
              or other information (collectively "Software") is provided
              "AS IS" without warranty of any kind. MICRON TECHNOLOGY, INC.
              ("MTI") EXPRESSLY DISCLAIMS ALL WARRANTIES EXPRESS OR IMPLIED,
              INCLUDING BUT NOT LIMITED TO, NONINFRINGEMENT OF THIRD PARTY
              RIGHTS, AND ANY IMPLIED WARRANTIES OF MERCHANTABILITY OR
              FITNESS FOR ANY PARTICULAR PURPOSE. MTI DOES NOT WARRANT THAT 
              THE SOFTWARE WILL MEET YOUR REQUIREMENTS, OR THAT THE 
              OPERATION OF THE SOFTWARE WILL BE UNINTERRUPTED OR ERROR-FREE. 
              FURTHERMORE, MTI DOES NOT MAKE ANY REPRESENTATIONS REGARDING
              THE USE OR THE RESULTS OF THE USE OF THE SOFTWARE IN TERMS OF
              ITS CORRECTNESS, ACCURACY, RELIABILITY, OR OTHERWISE. THE
              ENTIRE RISK ARISING OUT OF USE OR PERFORMANCE OF THE SOFTWARE
              REMAINS WITH YOU. IN NO EVENT SHALL MTI, ITS AFFILIATED
              COMPANIES OR THEIR SUPPLIERS BE LIABLE FOR ANY DIRECT,
              INDIRECT, CONSEQUENTIAL, INCIDENTAL, OR SPECIAL DAMAGES
              (INCLUDING, WITHOUT LIMITATION, DAMAGES FOR LOSS OF PROFITS,
              BUSINESS INTERRUPTION, OR LOSS OF INFORMATION) ARISING OUT OF
              YOUR USE OF OR INABILITY TO USE THE SOFTWARE, EVEN IF MTI HAS
              BEEN ADVISED OF THE POSSIBILITY OF SUCH DAMAGES. Because some
              jurisdictions prohibit the exclusion or limitation of 
              liability for consequential or incidental damages, the above
              limitation may not apply to you.
| 
[Copyright]   Copyright 2010 Micron Technology, Inc. All rights reserved.
|
|***************************************************************************
| Component MT46H128M32L2MC  (240-Ball 14mm x 14mm x 0.80mm QCT PoP) 
|***************************************************************************
|
[Begin Board Description] MT46H128M32L2MC
[Manufacturer] Micron Technology, Inc.
|
[Number Of Pins]  240
|
[Pin List]     signal_name
A1             NC
A2             GND
A3             POWER
A4             DQ31
A5             POWER
A6             GND
A7             DQ26
A8             DQ24
A9             DQS3
A10            DM3
A11            DQ23
A12            DQ21
A13            GND
A14            POWER
A15            DQ16
A16            GND
A17            NC
A18            NC
A19            POWER
A20            GND
A21            DQ15
A22            DQ13
A23            GND
A24            POWER
A25            NC
A26            GND
A27            NC
B1             GND
B2             NC
B3             GND
B4             DQ30
B5             DQ29
B6             DQ27
B7             POWER
B8             GND
B9             NC
B10            GND
B11            DQ22
B12            DQ20
B13            DQ19
B14            DQ17
B15            NC
B16            POWER
B17            GND
B18            POWER
B19            NC
B20            DQS1
B21            DQ14
B22            DQ12
B23            DQ11
B24            DQ9
B25            DQ8
B26            NC
B27            GND
C1             NC
C2             NC
C5             DQ28
C7             DQ25
C9             POWER
C11            POWER
C13            DQ18
C15            DQS2
C17            DM2
C19            DM1
C21            POWER
C23            DQ10
C26            DM0
C27            POWER
D1             NC
D2             POWER
D26            POWER
D27            NC
E1             NC
E2             NC
E3             NC
E25            GND
E26            DQS0
E27            DQ7
F1             NC
F2             NC
F26            DQ6
F27            POWER
G1             NC
G2             NC
G3             NC
G25            DQ5
G26            DQ4
G27            GND
H1             GND
H2             NC
H26            DQ3
H27            DQ2
J1             NC
J2             NC
J3             NC
J25            POWER
J26            DQ1
J27            DQ0
K1             GND
K2             NC
K26            GND
K27            POWER
L1             NC
L2             POWER
L3             NC
L25            NC
L26            NC
L27            GND
M1             NC
M2             GND
M26            NC
M27            NC
N1             NC
N2             NC
N3             NC
N25            NC
N26            NC
N27            NC
P1             NC
P2             NC
P26            NC
P27            NC
R1             NC
R2             NC
R3             NC
R25            NC
R26            NC
R27            NC
T1             GND
T2             GND
T26            NC
T27            NC
U1             NC
U2             GND
U3             NC
U25            NC
U26            NC
U27            NC
V1             NC
V2             NC
V26            NC
V27            NC
W1             NC
W2             POWER
W3             POWER
W25            NC
W26            NC
W27            NC
Y1             POWER
Y2             GND
Y26            NC
Y27            NC
AA1            NC
AA2            NC
AA3            NC
AA25           NC
AA26           NC
AA27           NC
AB1            POWER
AB2            NC
AB26           NC
AB27           NC
AC1            NC
AC2            NC
AC3            GND
AC25           NC
AC26           NC
AC27           NC
AD1            NC
AD2            NC
AD26           A13
AD27           A3
AE1            NC
AE2            NC
AE5            NC
AE7            NC
AE9            NC
AE11           POWER
AE13           A4
AE15           A6
AE17           POWER
AE19           A11
AE21           GND
AE23           NC
AE26           A2
AE27           A1
AF1            NC
AF2            POWER
AF3            NC
AF4            NC
AF5            NC
AF6            NC
AF7            NC
AF8            NC
AF9            NC
AF10           NC
AF11           POWER
AF12           A5
AF13           A7
AF14           POWER
AF15           GND
AF16           POWER
AF17           CK
AF18           CKE0
AF19           CS0#
AF20           A12
AF21           GND
AF22           CAS#
AF23           POWER
AF24           BA0
AF25           A0
AF26           POWER
AF27           NC
AG1            NC
AG2            GND
AG3            POWER
AG4            NC
AG5            NC
AG6            NC
AG7            NC
AG8            NC
AG9            NC
AG10           NC
AG11           NC
AG12           A9
AG13           A8
AG14           GND
AG15           NC
AG16           GND
AG17           CK#
AG18           CKE1
AG19           CS1#
AG20           WE#
AG21           POWER
AG22           RAS#
AG23           NC
AG24           BA1
AG25           A10
AG26           GND
AG27           NC
|
[Path Description] DQ31
Pin A4
  Len = 1 R = 0.249 L = 1.883E-09 C = 9.035E-13 / | substrate RLC
Fork
  Len = 1.619 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.4
Endfork
Fork
  Len = 1.781 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.4
Endfork
|
[Path Description] DQ26
Pin A7
  Len = 1 R = 0.294 L = 2.045E-09 C = 9.494E-13 / | substrate RLC
Fork
  Len = 1.607 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.11
Endfork
Fork
  Len = 1.768 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.11
Endfork
|
[Path Description] DQ24
Pin A8
  Len = 1 R = 0.261 L = 1.798E-09 C = 8.976E-13 / | substrate RLC
Fork
  Len = 1.607 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.15
Endfork
Fork
  Len = 1.767 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.15
Endfork
|
[Path Description] DQS3
Pin A9
  Len = 1 R = 0.341 L = 2.354E-09 C = 1.098E-12 / | substrate RLC
Fork
  Len = 1.609 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.16
Endfork
Fork
  Len = 1.769 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.16
Endfork
|
[Path Description] DM3
Pin A10
  Len = 1 R = 0.357 L = 2.414E-09 C = 1.147E-12 / | substrate RLC
Fork
  Len = 1.611 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.17
Endfork
Fork
  Len = 1.772 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.17
Endfork
|
[Path Description] DQ23
Pin A11
  Len = 1 R = 0.332 L = 2.184E-09 C = 1.002E-12 / | substrate RLC
Fork
  Len = 1.610 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.20
Endfork
Fork
  Len = 1.771 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.20
Endfork
|
[Path Description] DQ21
Pin A12
  Len = 1 R = 0.357 L = 2.533E-09 C = 1.108E-12 / | substrate RLC
Fork
  Len = 1.617 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.22
Endfork
Fork
  Len = 1.779 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.22
Endfork
|
[Path Description] DQ16
Pin A15
  Len = 1 R = 0.358 L = 2.877E-09 C = 1.129E-12 / | substrate RLC
Fork
  Len = 1.670 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.29
Endfork
Fork
  Len = 1.837 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.29
Endfork
|
[Path Description] DQ15
Pin A21
  Len = 1 R = 0.319 L = 2.224E-09 C = 9.924E-13 / | substrate RLC
Fork
  Len = 1.635 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.68
Endfork
Fork
  Len = 1.798 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.68
Endfork
|
[Path Description] DQ13
Pin A22
  Len = 1 R = 0.356 L = 2.364E-09 C = 1.042E-12 / | substrate RLC
Fork
  Len = 1.623 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.70
Endfork
Fork
  Len = 1.785 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.70
Endfork
|
[Path Description] DQ30
Pin B4
  Len = 1 R = 0.243 L = 1.717E-09 C = 9.653E-13 / | substrate RLC
Fork
  Len = 1.615 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.5
Endfork
Fork
  Len = 1.777 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.5
Endfork
|
[Path Description] DQ29
Pin B5
  Len = 1 R = 0.253 L = 1.757E-09 C = 9.889E-13 / | substrate RLC
Fork
  Len = 1.615 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.8
Endfork
Fork
  Len = 1.776 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.8
Endfork
|
[Path Description] DQ27
Pin B6
  Len = 1 R = 0.287 L = 1.895E-09 C = 9.669E-13 / | substrate RLC
Fork
  Len = 1.609 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.10
Endfork
Fork
  Len = 1.770 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.10
Endfork
|
[Path Description] DQ22
Pin B11
  Len = 1 R = 0.269 L = 1.778E-09 C = 9.097E-13 / | substrate RLC
Fork
  Len = 1.613 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.21
Endfork
Fork
  Len = 1.775 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.21
Endfork
|
[Path Description] DQ20
Pin B12
  Len = 1 R = 0.306 L = 2.160E-09 C = 1.051E-12 / | substrate RLC
Fork
  Len = 1.622 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.23
Endfork
Fork
  Len = 1.784 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.23
Endfork
|
[Path Description] DQ19
Pin B13
  Len = 1 R = 0.308 L = 2.254E-09 C = 1.037E-12 / | substrate RLC
Fork
  Len = 1.641 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.26
Endfork
Fork
  Len = 1.806 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.26
Endfork
|
[Path Description] DQ17
Pin B14
  Len = 1 R = 0.338 L = 2.600E-09 C = 1.106E-12 / | substrate RLC
Fork
  Len = 1.659 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.28
Endfork
Fork
  Len = 1.825 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.28
Endfork
|
[Path Description] DQS1
Pin B20
  Len = 1 R = 0.325 L = 2.342E-09 C = 1.061E-12 / | substrate RLC
Fork
  Len = 1.633 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.65
Endfork
Fork
  Len = 1.797 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.65
Endfork
|
[Path Description] DQ14
Pin B21
  Len = 1 R = 0.326 L = 2.110E-09 C = 1.016E-12 / | substrate RLC
Fork
  Len = 1.628 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.69
Endfork
Fork
  Len = 1.791 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.69
Endfork
|
[Path Description] DQ12
Pin B22
  Len = 1 R = 0.348 L = 2.255E-09 C = 1.050E-12 / | substrate RLC
Fork
  Len = 1.618 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.71
Endfork
Fork
  Len = 1.780 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.71
Endfork
|
[Path Description] DQ11
Pin B23
  Len = 1 R = 0.304 L = 2.156E-09 C = 1.032E-12 / | substrate RLC
Fork
  Len = 1.608 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.74
Endfork
Fork
  Len = 1.769 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.74
Endfork
|
[Path Description] DQ9
Pin B24
  Len = 1 R = 0.409 L = 2.932E-09 C = 1.215E-12 / | substrate RLC
Fork
  Len = 1.606 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.76
Endfork
Fork
  Len = 1.766 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.76
Endfork
|
[Path Description] DQ8
Pin B25
  Len = 1 R = 0.378 L = 2.860E-09 C = 1.179E-12 / | substrate RLC
Fork
  Len = 1.605 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.77
Endfork
Fork
  Len = 1.766 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.77
Endfork
|
[Path Description] DQ28
Pin C5
  Len = 1 R = 0.238 L = 1.569E-09 C = 9.461E-13 / | substrate RLC
Fork
  Len = 1.611 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.9
Endfork
Fork
  Len = 1.773 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.9
Endfork
|
[Path Description] DQ25
Pin C7
  Len = 1 R = 0.210 L = 1.319E-09 C = 8.090E-13 / | substrate RLC
Fork
  Len = 1.606 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.14
Endfork
Fork
  Len = 1.766 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.14
Endfork
|
[Path Description] DQ18
Pin C13
  Len = 1 R = 0.280 L = 2.037E-09 C = 9.866E-13 / | substrate RLC
Fork
  Len = 1.650 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.27
Endfork
Fork
  Len = 1.815 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.27
Endfork
|
[Path Description] DQS2
Pin C15
  Len = 1 R = 0.345 L = 2.663E-09 C = 1.097E-12 / | substrate RLC
Fork
  Len = 1.670 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.32
Endfork
Fork
  Len = 1.837 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.32
Endfork
|
[Path Description] DM2
Pin C17
  Len = 1 R = 0.347 L = 2.798E-09 C = 1.115E-12 / | substrate RLC
Fork
  Len = 1.682 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.33
Endfork
Fork
  Len = 1.850 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.33
Endfork
|
[Path Description] DM1
Pin C19
  Len = 1 R = 0.287 L = 1.978E-09 C = 1.000E-12 / | substrate RLC
Fork
  Len = 1.641 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.64
Endfork
Fork
  Len = 1.805 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.64
Endfork
|
[Path Description] DQ10
Pin C23
  Len = 1 R = 0.331 L = 2.263E-09 C = 1.058E-12 / | substrate RLC
Fork
  Len = 1.607 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.75
Endfork
Fork
  Len = 1.767 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.75
Endfork
|
[Path Description] DM0
Pin C26
  Len = 1 R = 0.359 L = 2.710E-09 C = 1.124E-12 / | substrate RLC
Fork
  Len = 1.605 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.80
Endfork
Fork
  Len = 1.766 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.80
Endfork
|
[Path Description] DQS0
Pin E26
  Len = 1 R = 0.425 L = 3.072E-09 C = 1.291E-12 / | substrate RLC
Fork
  Len = 1.606 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.81
Endfork
Fork
  Len = 1.766 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.81
Endfork
|
[Path Description] DQ7
Pin E27
  Len = 1 R = 0.348 L = 2.665E-09 C = 1.122E-12 / | substrate RLC
Fork
  Len = 1.607 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.82
Endfork
Fork
  Len = 1.767 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.82
Endfork
|
[Path Description] DQ6
Pin F26
  Len = 1 R = 0.433 L = 3.260E-09 C = 1.309E-12 / | substrate RLC
Fork
  Len = 1.608 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.83
Endfork
Fork
  Len = 1.769 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.83
Endfork
|
[Path Description] DQ5
Pin G25
  Len = 1 R = 0.394 L = 2.976E-09 C = 1.235E-12 / | substrate RLC
Fork
  Len = 1.618 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.86
Endfork
Fork
  Len = 1.780 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.86
Endfork
|
[Path Description] DQ4
Pin G26
  Len = 1 R = 0.467 L = 3.605E-09 C = 1.328E-12 / | substrate RLC
Fork
  Len = 1.623 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.87
Endfork
Fork
  Len = 1.786 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.87
Endfork
|
[Path Description] DQ3
Pin H26
  Len = 1 R = 0.395 L = 3.177E-09 C = 1.208E-12 / | substrate RLC
Fork
  Len = 1.629 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.88
Endfork
Fork
  Len = 1.792 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.88
Endfork
|
[Path Description] DQ2
Pin H27
  Len = 1 R = 0.403 L = 3.137E-09 C = 1.222E-12 / | substrate RLC
Fork
  Len = 1.636 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.89
Endfork
Fork
  Len = 1.799 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.89
Endfork
|
[Path Description] DQ1
Pin J26
  Len = 1 R = 0.407 L = 3.056E-09 C = 1.187E-12 / | substrate RLC
Fork
  Len = 1.637 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.92
Endfork
Fork
  Len = 1.801 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.92
Endfork
|
[Path Description] DQ0
Pin J27
  Len = 1 R = 0.392 L = 2.969E-09 C = 1.197E-12 / | substrate RLC
Fork
  Len = 1.645 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.93
Endfork
Fork
  Len = 1.809 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.93
Endfork
|
[Path Description] A13
Pin AD26
  Len = 1 R = 0.597 L = 5.220E-09 C = 1.499E-12 / | substrate RLC
Fork
  Len = 1.556 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.124
Endfork
Fork
  Len = 1.711 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.124
Endfork
|
[Path Description] A3
Pin AD27
  Len = 1 R = 0.409 L = 3.832E-09 C = 1.137E-12 / | substrate RLC
Fork
  Len = 1.584 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.109
Endfork
Fork
  Len = 1.743 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.109
Endfork
|
[Path Description] A4
Pin AE13
  Len = 1 R = 0.325 L = 2.224E-09 C = 9.231E-13 / | substrate RLC
Fork
  Len = 1.558 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.132
Endfork
Fork
  Len = 1.713 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.132
Endfork
|
[Path Description] A6
Pin AE15
  Len = 1 R = 0.332 L = 2.280E-09 C = 1.026E-12 / | substrate RLC
Fork
  Len = 1.555 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.130
Endfork
Fork
  Len = 1.711 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.130
Endfork
|
[Path Description] A11
Pin AE19
  Len = 1 R = 0.473 L = 4.091E-09 C = 1.268E-12 / | substrate RLC
Fork
  Len = 1.564 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.126
Endfork
Fork
  Len = 1.721 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.126
Endfork
|
[Path Description] A2
Pin AE26
  Len = 1 R = 0.396 L = 3.792E-09 C = 1.224E-12 / | substrate RLC
Fork
  Len = 1.564 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.110
Endfork
Fork
  Len = 1.721 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.110
Endfork
|
[Path Description] A1
Pin AE27
  Len = 1 R = 0.464 L = 4.318E-09 C = 1.299E-12 / | substrate RLC
Fork
  Len = 1.563 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.111
Endfork
Fork
  Len = 1.720 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.111
Endfork
|
[Path Description] A5
Pin AF12
  Len = 1 R = 0.313 L = 2.111E-09 C = 9.625E-13 / | substrate RLC
Fork
  Len = 1.555 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.131
Endfork
Fork
  Len = 1.711 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.131
Endfork
|
[Path Description] A7
Pin AF13
  Len = 1 R = 0.282 L = 1.904E-09 C = 8.979E-13 / | substrate RLC
Fork
  Len = 1.558 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.129
Endfork
Fork
  Len = 1.714 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.129
Endfork
|
[Path Description] CK
Pin AF17
  Len = 1 R = 0.880 L = 7.445E-09 C = 2.262E-12 / | substrate RLC
Fork
  Len = 1.557 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.51
Endfork
Fork
  Len = 1.713 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.51
Endfork
|
[Path Description] CKE0
Pin AF18
  Len = 1 R = 0.346 L = 2.838E-09 C = 9.967E-13 / | substrate RLC
Fork
  Len = 1.654 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.120
Endfork
|
[Path Description] CS0#
Pin AF19
  Len = 1 R = 0.174 L = 1.672E-09 C = 8.266E-13 / | substrate RLC
Fork
  Len = 1.554 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.116
Endfork
|
[Path Description] A12
Pin AF20
  Len = 1 R = 0.558 L = 4.982E-09 C = 1.402E-12 / | substrate RLC
Fork
  Len = 1.587 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.125
Endfork
Fork
  Len = 1.745 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.125
Endfork
|
[Path Description] CAS#
Pin AF22
  Len = 1 R = 0.452 L = 4.053E-09 C = 1.292E-12 / | substrate RLC
Fork
  Len = 1.558 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.118
Endfork
Fork
  Len = 1.714 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.118
Endfork
|
[Path Description] BA0
Pin AF24
  Len = 1 R = 0.402 L = 3.731E-09 C = 1.207E-12 / | substrate RLC
Fork
  Len = 1.555 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.114
Endfork
Fork
  Len = 1.711 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.114
Endfork
|
[Path Description] A0
Pin AF25
  Len = 1 R = 0.415 L = 3.886E-09 C = 1.253E-12 / | substrate RLC
Fork
  Len = 1.559 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.112
Endfork
Fork
  Len = 1.714 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.112
Endfork
|
[Path Description] A9
Pin AG12
  Len = 1 R = 0.446 L = 3.380E-09 C = 1.173E-12 / | substrate RLC
Fork
  Len = 1.564 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.127
Endfork
Fork
  Len = 1.720 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.127
Endfork
|
[Path Description] A8
Pin AG13
  Len = 1 R = 0.267 L = 1.857E-09 C = 8.241E-13 / | substrate RLC
Fork
  Len = 1.559 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.128
Endfork
Fork
  Len = 1.715 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.128
Endfork
|
[Path Description] CK#
Pin AG17
  Len = 1 R = 0.895 L = 7.584E-09 C = 2.240E-12 / | substrate RLC
Fork
  Len = 1.645 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.52
Endfork
Fork
  Len = 1.810 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.52
Endfork
|
[Path Description] CKE1
Pin AG18
  Len = 1 R = 0.192 L = 1.705E-09 C = 8.299E-13 / | substrate RLC
Fork
  Len = 1.819 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.120
Endfork
|
[Path Description] CS1#
Pin AG19
  Len = 1 R = 0.191 L = 1.698E-09 C = 8.263E-13 / | substrate RLC
Fork
  Len = 1.710 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.116
Endfork
|
[Path Description] WE#
Pin AG20
  Len = 1 R = 0.438 L = 3.817E-09 C = 1.206E-12 / | substrate RLC
Fork
  Len = 1.558 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.119
Endfork
Fork
  Len = 1.714 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.119
Endfork
|
[Path Description] RAS#
Pin AG22
  Len = 1 R = 0.440 L = 3.978E-09 C = 1.193E-12 / | substrate RLC
Fork
  Len = 1.572 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.117
Endfork
Fork
  Len = 1.729 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.117
Endfork
|
[Path Description] BA1
Pin AG24
  Len = 1 R = 0.435 L = 3.937E-09 C = 1.254E-12 / | substrate RLC
Fork
  Len = 1.555 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.115
Endfork
Fork
  Len = 1.711 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.115
Endfork
|
[Path Description] A10
Pin AG25
  Len = 1 R = 0.456 L = 4.207E-09 C = 1.283E-12 / | substrate RLC
Fork
  Len = 1.558 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.113
Endfork
Fork
  Len = 1.714 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.113
Endfork
|
[Reference Designator Map]
|
| Ref Des  File name      Component name
U1         t69m.ibs       MT46H64M32LFT69M_DS
U2         t69m.ibs       MT46H64M32LFT69M_DS
[End Board Description]
|
[End]
