|***************************************************************************
|T69M EBD Model for 152-Ball TI-OMAP PoP 14 x 14 x 1.2mm TFBGA
|Quad Die LP-DDR DRAM
| 
|Part Number      VDD/VDDQ  Architecture  Package
|-----------      --------  ------------  -------
|MT46H256M32L4KZ  1.8/1.8V  256Mb x32     152-Ball OMAP PoP
|
|***************************************************************************
|
[IBIS Ver]    4.0
[File name]   t69m_152b_4dp.ebd
[File rev]    1.0
[Date]        02/15/2010
[Source]      From SPICE model at Micron Technology, Inc.
                  Micron Technology, Inc.
                  8000 S. Federal Way
                  P.O. Box 6, M/S: 01-711
                  Boise, ID 83707-0006
              For support send e-mail to modelsupport@micron.com              
|
[Notes]       Rev 1.0: 02/15/2010
               - Initial revision of packaging ebd
|
              Notes:
               - U1, U2, U3, U4 are the LPDRAM bare die components
                 (MT46H64M32LFT69M_DS) defined in the IBIS file t69m.ibs
               - Please choose the appropriate speed grade and drive 
                 strength models from the bare die ibis components
               - In order to perform simulation using this model, 
                 *.ebd and *.ibs files must be in the same directory
|
[Disclaimer]  This software code and all associated documentation, comments
              or other information (collectively "Software") is provided
              "AS IS" without warranty of any kind. MICRON TECHNOLOGY, INC.
              ("MTI") EXPRESSLY DISCLAIMS ALL WARRANTIES EXPRESS OR IMPLIED,
              INCLUDING BUT NOT LIMITED TO, NONINFRINGEMENT OF THIRD PARTY
              RIGHTS, AND ANY IMPLIED WARRANTIES OF MERCHANTABILITY OR
              FITNESS FOR ANY PARTICULAR PURPOSE. MTI DOES NOT WARRANT THAT 
              THE SOFTWARE WILL MEET YOUR REQUIREMENTS, OR THAT THE 
              OPERATION OF THE SOFTWARE WILL BE UNINTERRUPTED OR ERROR-FREE. 
              FURTHERMORE, MTI DOES NOT MAKE ANY REPRESENTATIONS REGARDING
              THE USE OR THE RESULTS OF THE USE OF THE SOFTWARE IN TERMS OF
              ITS CORRECTNESS, ACCURACY, RELIABILITY, OR OTHERWISE. THE
              ENTIRE RISK ARISING OUT OF USE OR PERFORMANCE OF THE SOFTWARE
              REMAINS WITH YOU. IN NO EVENT SHALL MTI, ITS AFFILIATED
              COMPANIES OR THEIR SUPPLIERS BE LIABLE FOR ANY DIRECT,
              INDIRECT, CONSEQUENTIAL, INCIDENTAL, OR SPECIAL DAMAGES
              (INCLUDING, WITHOUT LIMITATION, DAMAGES FOR LOSS OF PROFITS,
              BUSINESS INTERRUPTION, OR LOSS OF INFORMATION) ARISING OUT OF
              YOUR USE OF OR INABILITY TO USE THE SOFTWARE, EVEN IF MTI HAS
              BEEN ADVISED OF THE POSSIBILITY OF SUCH DAMAGES. Because some
              jurisdictions prohibit the exclusion or limitation of 
              liability for consequential or incidental damages, the above
              limitation may not apply to you.
| 
[Copyright]   Copyright 2010 Micron Technology, Inc. All rights reserved.
|
|***************************************************************************
| Component MT46H256M32L4KZ (168-Ball TFBGA 14 x 14 x 1.2mm TI-OMAP PoP) 
|***************************************************************************
|
[Begin Board Description] MT46H256M32L4KZ 
[Manufacturer] Micron Technology, Inc.
|
[Number Of Pins]  152
|
[Pin List]     signal_name
A1             NC
A2             NC
A3             POWER
A4             DM1
A5             DQ13
A6             DQ15
A7             GND
A8             DQ10
A9             DQ12
A10            DQ16
A11            DQ19
A12            CK
A13            GND
A14            DM2
A15            POWER
A16            DQ21
A17            DQ20
A18            DM3
A19            DQS3
A20            NC
A21            NC
B1             NC
B2             NC
B3             DQ6
B4             DQ7
B5             POWER
B6             DQ9
B7             DQ14
B8             DQS1
B9             DQ11
B10            DQ8
B11            DQ17
B12            DQ18
B13            CK#
B14            GND
B15            DQS2
B16            POWER
B17            DQ23
B18            DQ22
B19            DQ28
B20            NC
B21            NC
C1             GND
C2             DQS0
C20            DQ24
C21            DQ26
D1             DQ3
D2             DQ5
D20            DQ25
D21            DQ29
E1             DQ0
E2             DQ1
E20            DQ27
E21            DQ31
F1             GND
F2             POWER
F20            GND
F21            POWER
G1             DQ4
G2             DQ2
G20            A0
G21            DQ30
H1             DM0
H2             GND
H20            GND
H21            POWER
J1             POWER
J2             NC
J20            A2
J21            A3
K1             NC
K2             NC
K20            A1
K21            A9
L1             NC
L2             NC
L20            POWER
L21            GND
M1             NC
M2             GND
M20            A7
M21            A6
N1             NC
N2             NC
N20            A8
N21            A11
P1             NC
P2             NC
P20            GND
P21            POWER
R1             NC
R2             GND
R20            A5
R21            A12
T1             NC
T2             NC
T20            CS1#
T21            CS0#
U1             NC
U2             NC
U20            CAS#
U21            A4
V1             NC
V2             NC
V20            BA1
V21            RAS#
W1             NC
W2             NC
W20            GND
W21            POWER
Y1             NC
Y2             NC
Y3             NC
Y4             NC
Y5             NC
Y6             GND
Y7             NC
Y8             NC
Y9             NC
Y10            NC
Y11            GND
Y12            A14
Y13            CKE1
Y14            POWER
Y15            CKE0
Y16            A10
Y17            GND
Y18            WE#
Y19            GND
Y20            NC
Y21            NC
AA1            NC
AA2            NC
AA3            NC
AA4            NC
AA5            NC
AA6            NC
AA7            GND
AA8            NC
AA9            NC
AA10           NC
AA11           POWER
AA12           NC
AA13           GND
AA14           POWER
AA15           A13
AA16           GND
AA17           POWER
AA18           BA0
AA19           POWER
AA20           NC
AA21           NC
|
[Path Description] DM1
Pin A4
  Len = 1 R = 0.456 L = 4.407E-09 C = 1.177E-12 / | substrate RLC
Fork
  Len = 1.957 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.33
Endfork
Fork
  Len = 2.003 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.33
Endfork
|
[Path Description] DQ13
Pin A5
  Len = 1 R = 0.105 L = 9.164E-10 C = 5.284E-13 / | substrate RLC
Fork
  Len = 1.803 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.27
Endfork
Fork
  Len = 1.853 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.27
Endfork
|
[Path Description] DQ15
Pin A6
  Len = 1 R = 0.123 L = 1.115E-09 C = 5.666E-13 / | substrate RLC
Fork
  Len = 1.734 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.26
Endfork
Fork
  Len = 1.786 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.26
Endfork
|
[Path Description] DQ10
Pin A8
  Len = 1 R = 0.173 L = 1.615E-09 C = 6.556E-13 / | substrate RLC
Fork
  Len = 1.717 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.76
Endfork
Fork
  Len = 1.753 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.76
Endfork
|
[Path Description] DQ12
Pin A9
  Len = 1 R = 0.220 L = 2.276E-09 C = 7.566E-13 / | substrate RLC
Fork
  Len = 1.713 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.27
Endfork
Fork
  Len = 1.749 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.27
Endfork
|
[Path Description] DQ16
Pin A10
  Len = 1 R = 0.371 L = 3.973E-09 C = 1.026E-12 / | substrate RLC
Fork
  Len = 1.841 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.23
Endfork
Fork
  Len = 1.874 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.23
Endfork
|
[Path Description] DQ19
Pin A11
  Len = 1 R = 0.344 L = 3.756E-09 C = 9.319E-13 / | substrate RLC
Fork
  Len = 1.737 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.22
Endfork
Fork
  Len = 1.788 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.22
Endfork
|
[Path Description] CK
Pin A12
  Len = 1 R = 0.144 L = 1.447E-09 C = 6.121E-13 / | substrate RLC
Fork
  Len = 1.751 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.51
Endfork
Fork
  Len = 1.765 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.51
Endfork
Fork
  Len = 1.787 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.51
Endfork
Fork
  Len = 1.816 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.51
Endfork
|
[Path Description] DM2
Pin A14
  Len = 1 R = 0.226 L = 2.174E-09 C = 7.240E-13 / | substrate RLC
Fork
  Len = 1.892 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.64
Endfork
Fork
  Len = 1.924 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.64
Endfork
|
[Path Description] DQ21
Pin A16
  Len = 1 R = 0.099 L = 9.233E-10 C = 5.232E-13 / | substrate RLC
Fork
  Len = 1.930 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.20
Endfork
Fork
  Len = 1.962 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.20
Endfork
|
[Path Description] DQ20
Pin A17
  Len = 1 R = 0.211 L = 1.996E-09 C = 7.351E-13 / | substrate RLC
Fork
  Len = 1.814 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.21
Endfork
Fork
  Len = 1.863 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.21
Endfork
|
[Path Description] DM3
Pin A18
  Len = 1 R = 0.517 L = 5.569E-09 C = 1.268E-12 / | substrate RLC
Fork
  Len = 1.979 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.64
Endfork
Fork
  Len = 2.024 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.64
Endfork
|
[Path Description] DQS3
Pin A19
  Len = 1 R = 0.542 L = 5.803E-09 C = 1.334E-12 / | substrate RLC
Fork
  Len = 1.824 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.65
Endfork
Fork
  Len = 1.873 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.65
Endfork
|
[Path Description] DQ6
Pin B3
  Len = 1 R = 0.185 L = 1.707E-09 C = 7.654E-13 / | substrate RLC
Fork
  Len = 1.725 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.29
Endfork
Fork
  Len = 1.761 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.29
Endfork
|
[Path Description] DQ7
Pin B4
  Len = 1 R = 0.176 L = 1.769E-09 C = 7.638E-13 / | substrate RLC
Fork
  Len = 1.874 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.29
Endfork
Fork
  Len = 1.922 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.29
Endfork
|
[Path Description] DQ9
Pin B6
  Len = 1 R = 0.095 L = 8.232E-10 C = 5.869E-13 / | substrate RLC
Fork
  Len = 1.756 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.28
Endfork
Fork
  Len = 1.807 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.28
Endfork
|
[Path Description] DQ14
Pin B7
  Len = 1 R = 0.134 L = 1.052E-09 C = 6.433E-13 / | substrate RLC
Fork
  Len = 1.713 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.26
Endfork
Fork
  Len = 1.749 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.26
Endfork
|
[Path Description] DQS1
Pin B8
  Len = 1 R = 0.324 L = 3.022E-09 C = 1.000E-12 / | substrate RLC
Fork
  Len = 1.811 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.32
Endfork
Fork
  Len = 1.861 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.32
Endfork
|
[Path Description] DQ11
Pin B9
  Len = 1 R = 0.115 L = 1.155E-09 C = 6.401E-13 / | substrate RLC
Fork
  Len = 1.963 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.76
Endfork
Fork
  Len = 2.009 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.76
Endfork
|
[Path Description] DQ8
Pin B10
  Len = 1 R = 0.174 L = 1.694E-09 C = 7.470E-13 / | substrate RLC
Fork
  Len = 1.759 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.28
Endfork
Fork
  Len = 1.794 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.28
Endfork
|
[Path Description] DQ17
Pin B11
  Len = 1 R = 0.287 L = 3.254E-09 C = 9.590E-13 / | substrate RLC
Fork
  Len = 2.059 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.23
Endfork
Fork
  Len = 2.102 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.23
Endfork
|
[Path Description] DQ18
Pin B12
  Len = 1 R = 0.277 L = 3.070E-09 C = 9.041E-13 / | substrate RLC
Fork
  Len = 1.776 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.22
Endfork
Fork
  Len = 1.811 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.22
Endfork
|
[Path Description] CK#
Pin B13
  Len = 1 R = 0.142 L = 1.306E-09 C = 6.765E-13 / | substrate RLC
Fork
  Len = 1.742 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.52
Endfork
Fork
  Len = 1.756 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.52
Endfork
Fork
  Len = 1.778 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.52
Endfork
Fork
  Len = 1.807 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.52
Endfork
|
[Path Description] DQS2
Pin B15
  Len = 1 R = 0.151 L = 1.618E-09 C = 6.993E-13 / | substrate RLC
Fork
  Len = 1.868 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.65
Endfork
Fork
  Len = 1.901 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.65
Endfork
|
[Path Description] DQ23
Pin B17
  Len = 1 R = 0.092 L = 7.014E-10 C = 5.098E-13 / | substrate RLC
Fork
  Len = 1.751 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.75
Endfork
Fork
  Len = 1.786 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.75
Endfork
|
[Path Description] DQ22
Pin B18
  Len = 1 R = 0.144 L = 1.289E-09 C = 6.993E-13 / | substrate RLC
Fork
  Len = 1.763 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.20
Endfork
Fork
  Len = 1.814 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.20
Endfork
|
[Path Description] DQ28
Pin B19
  Len = 1 R = 0.219 L = 2.130E-09 C = 8.280E-13 / | substrate RLC
Fork
  Len = 1.727 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.71
Endfork
Fork
  Len = 1.779 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.71
Endfork
|
[Path Description] DQS0
Pin C2
  Len = 1 R = 0.432 L = 4.485E-09 C = 1.204E-12 / | substrate RLC
Fork
  Len = 1.852 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.32
Endfork
Fork
  Len = 1.885 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.32
Endfork
|
[Path Description] DQ24
Pin C20
  Len = 1 R = 0.267 L = 2.889E-09 C = 9.421E-13 / | substrate RLC
Fork
  Len = 1.741 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.75
Endfork
Fork
  Len = 1.792 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.75
Endfork
|
[Path Description] DQ26
Pin C21
  Len = 1 R = 0.347 L = 3.546E-09 C = 9.852E-13 / | substrate RLC
Fork
  Len = 1.735 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.74
Endfork
Fork
  Len = 1.786 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.74
Endfork
|
[Path Description] DQ3
Pin D1
  Len = 1 R = 0.273 L = 2.875E-09 C = 8.716E-13 / | substrate RLC
Fork
  Len = 2.085 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.70
Endfork
Fork
  Len = 2.128 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.70
Endfork
|
[Path Description] DQ5
Pin D2
  Len = 1 R = 0.242 L = 2.570E-09 C = 8.959E-13 / | substrate RLC
Fork
  Len = 1.869 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.68
Endfork
Fork
  Len = 1.917 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.68
Endfork
|
[Path Description] DQ25
Pin D20
  Len = 1 R = 0.322 L = 3.334E-09 C = 1.035E-12 / | substrate RLC
Fork
  Len = 1.802 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.74
Endfork
Fork
  Len = 1.836 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.74
Endfork
|
[Path Description] DQ29
Pin D21
  Len = 1 R = 0.403 L = 4.251E-09 C = 1.098E-12 / | substrate RLC
Fork
  Len = 1.787 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.70
Endfork
Fork
  Len = 1.821 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.70
Endfork
|
[Path Description] DQ0
Pin E1
  Len = 1 R = 0.372 L = 3.749E-09 C = 1.020E-12 / | substrate RLC
Fork
  Len = 1.714 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.77
Endfork
Fork
  Len = 1.750 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.77
Endfork
|
[Path Description] DQ1
Pin E2
  Len = 1 R = 0.347 L = 3.570E-09 C = 1.072E-12 / | substrate RLC
Fork
  Len = 1.802 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.77
Endfork
Fork
  Len = 1.852 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.77
Endfork
|
[Path Description] DQ27
Pin E20
  Len = 1 R = 0.370 L = 4.248E-09 C = 1.115E-12 / | substrate RLC
Fork
  Len = 1.742 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.71
Endfork
Fork
  Len = 1.777 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.71
Endfork
|
[Path Description] DQ31
Pin E21
  Len = 1 R = 0.433 L = 4.578E-09 C = 1.183E-12 / | substrate RLC
Fork
  Len = 1.763 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.69
Endfork
Fork
  Len = 1.814 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.69
Endfork
|
[Path Description] DQ4
Pin G1
  Len = 1 R = 0.396 L = 4.082E-09 C = 1.115E-12 / | substrate RLC
Fork
  Len = 1.878 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.68
Endfork
Fork
  Len = 1.911 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.68
Endfork
|
[Path Description] DQ2
Pin G2
  Len = 1 R = 0.360 L = 4.090E-09 C = 1.026E-12 / | substrate RLC
Fork
  Len = 1.960 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.21
Endfork
Fork
  Len = 1.991 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.21
Endfork
|
[Path Description] A0
Pin G20
  Len = 1 R = 0.636 L = 6.452E-09 C = 1.706E-12 / | substrate RLC
Fork
  Len = 1.693 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.112
Endfork
Fork
  Len = 1.707 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.112
Endfork
Fork
  Len = 1.730 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.112
Endfork
Fork
  Len = 1.760 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.112
Endfork
|
[Path Description] DQ30
Pin G21
  Len = 1 R = 0.460 L = 4.359E-09 C = 1.251E-12 / | substrate RLC
Fork
  Len = 1.982 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.69
Endfork
Fork
  Len = 2.013 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.69
Endfork
|
[Path Description] DM0
Pin H1
  Len = 1 R = 0.461 L = 5.171E-09 C = 1.189E-12 / | substrate RLC
Fork
  Len = 1.873 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.33
Endfork
Fork
  Len = 1.906 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.33
Endfork
|
[Path Description] A2
Pin J20
  Len = 1 R = 0.521 L = 5.870E-09 C = 1.478E-12 / | substrate RLC
Fork
  Len = 1.691 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.110
Endfork
Fork
  Len = 1.705 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.110
Endfork
Fork
  Len = 1.727 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.110
Endfork
Fork
  Len = 1.757 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.110
Endfork
|
[Path Description] A3
Pin J21
  Len = 1 R = 0.536 L = 5.618E-09 C = 1.445E-12 / | substrate RLC
Fork
  Len = 1.695 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.109
Endfork
Fork
  Len = 1.709 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.109
Endfork
Fork
  Len = 1.731 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.109
Endfork
Fork
  Len = 1.761 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.109
Endfork
|
[Path Description] A1
Pin K20
  Len = 1 R = 0.496 L = 5.692E-09 C = 1.414E-12 / | substrate RLC
Fork
  Len = 1.691 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.111
Endfork
Fork
  Len = 1.705 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.111
Endfork
Fork
  Len = 1.727 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.111
Endfork
Fork
  Len = 1.757 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.111
Endfork
|
[Path Description] A9
Pin K21
  Len = 1 R = 0.606 L = 6.895E-09 C = 1.507E-12 / | substrate RLC
Fork
  Len = 1.709 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.127
Endfork
Fork
  Len = 1.723 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.127
Endfork
Fork
  Len = 1.745 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.127
Endfork
Fork
  Len = 1.775 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.127
Endfork
|
[Path Description] A7
Pin M20
  Len = 1 R = 0.549 L = 6.537E-09 C = 1.459E-12 / | substrate RLC
Fork
  Len = 1.701 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.129
Endfork
Fork
  Len = 1.715 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.129
Endfork
Fork
  Len = 1.737 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.129
Endfork
Fork
  Len = 1.767 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.129
Endfork
|
[Path Description] A6
Pin M21
  Len = 1 R = 0.608 L = 6.951E-09 C = 1.567E-12 / | substrate RLC
Fork
  Len = 1.695 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.130
Endfork
Fork
  Len = 1.710 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.130
Endfork
Fork
  Len = 1.732 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.130
Endfork
Fork
  Len = 1.762 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.130
Endfork
|
[Path Description] A8
Pin N20
  Len = 1 R = 0.528 L = 6.294E-09 C = 1.496E-12 / | substrate RLC
Fork
  Len = 1.701 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.128
Endfork
Fork
  Len = 1.715 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.128
Endfork
Fork
  Len = 1.738 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.128
Endfork
Fork
  Len = 1.768 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.128
Endfork
|
[Path Description] A11
Pin N21
  Len = 1 R = 0.553 L = 5.985E-09 C = 1.436E-12 / | substrate RLC
Fork
  Len = 1.709 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.126
Endfork
Fork
  Len = 1.723 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.126
Endfork
Fork
  Len = 1.746 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.126
Endfork
Fork
  Len = 1.775 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.126
Endfork
|
[Path Description] A5
Pin R20
  Len = 1 R = 0.562 L = 6.377E-09 C = 1.474E-12 / | substrate RLC
Fork
  Len = 1.695 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.131
Endfork
Fork
  Len = 1.709 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.131
Endfork
Fork
  Len = 1.731 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.131
Endfork
Fork
  Len = 1.761 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.131
Endfork
|
[Path Description] A12
Pin R21
  Len = 1 R = 0.534 L = 5.475E-09 C = 1.385E-12 / | substrate RLC
Fork
  Len = 1.719 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.125
Endfork
Fork
  Len = 1.733 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.125
Endfork
Fork
  Len = 1.755 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.125
Endfork
Fork
  Len = 1.784 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.125
Endfork
|
[Path Description] CS1#
Pin T20
  Len = 1 R = 0.364 L = 4.044E-09 C = 1.154E-12 / | substrate RLC
Fork
  Len = 1.741 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.116
Endfork
Fork
  Len = 1.771 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.116
Endfork
|
[Path Description] CS0#
Pin T21
  Len = 1 R = 0.430 L = 4.752E-09 C = 1.202E-12 / | substrate RLC
Fork
  Len = 1.729 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.116
Endfork
Fork
  Len = 1.743 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.116
Endfork
|
[Path Description] CAS#
Pin U20
  Len = 1 R = 0.381 L = 4.426E-09 C = 1.166E-12 / | substrate RLC
Fork
  Len = 1.690 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.118
Endfork
Fork
  Len = 1.704 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.118
Endfork
Fork
  Len = 1.727 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.118
Endfork
Fork
  Len = 1.757 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.118
Endfork
|
[Path Description] A4
Pin U21
  Len = 1 R = 0.600 L = 6.791E-09 C = 1.415E-12 / | substrate RLC
Fork
  Len = 1.691 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.132
Endfork
Fork
  Len = 1.705 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.132
Endfork
Fork
  Len = 1.728 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.132
Endfork
Fork
  Len = 1.758 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.132
Endfork
|
[Path Description] BA1
Pin V20
  Len = 1 R = 0.351 L = 3.577E-09 C = 1.124E-12 / | substrate RLC
Fork
  Len = 1.698 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.115
Endfork
Fork
  Len = 1.712 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.115
Endfork
Fork
  Len = 1.735 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.115
Endfork
Fork
  Len = 1.765 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.115
Endfork
|
[Path Description] RAS#
Pin V21
  Len = 1 R = 0.413 L = 4.731E-09 C = 1.132E-12 / | substrate RLC
Fork
  Len = 1.692 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.117
Endfork
Fork
  Len = 1.706 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.117
Endfork
Fork
  Len = 1.729 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.117
Endfork
Fork
  Len = 1.759 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.117
Endfork
|
[Path Description] A14
Pin Y12
  Len = 1 R = 0.246 L = 2.421E-09 C = 8.794E-13 / | substrate RLC
|
[Path Description] CKE1
Pin Y13
  Len = 1 R = 0.248 L = 2.462E-09 C = 8.998E-13 / | substrate RLC
Fork
  Len = 1.727 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.120
Endfork
Fork
  Len = 1.757 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.120
Endfork
|
[Path Description] CKE0
Pin Y15
  Len = 1 R = 0.329 L = 3.482E-09 C = 1.085E-12 / | substrate RLC
Fork
  Len = 1.699 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.120
Endfork
Fork
  Len = 1.713 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.120
Endfork
|
[Path Description] A10
Pin Y16
  Len = 1 R = 0.166 L = 1.989E-09 C = 7.163E-13 / | substrate RLC
Fork
  Len = 1.693 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.113
Endfork
Fork
  Len = 1.708 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.113
Endfork
Fork
  Len = 1.730 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.113
Endfork
Fork
  Len = 1.760 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.113
Endfork
|
[Path Description] WE#
Pin Y18
  Len = 1 R = 0.391 L = 4.302E-09 C = 1.123E-12 / | substrate RLC
Fork
  Len = 1.690 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.119
Endfork
Fork
  Len = 1.704 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.119
Endfork
Fork
  Len = 1.727 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.119
Endfork
Fork
  Len = 1.757 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.119
Endfork
|
[Path Description] A13
Pin AA15
  Len = 1 R = 0.424 L = 4.392E-09 C = 1.146E-12 / | substrate RLC
Fork
  Len = 1.695 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.124
Endfork
Fork
  Len = 1.710 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.124
Endfork
Fork
  Len = 1.732 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.124
Endfork
Fork
  Len = 1.762 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.124
Endfork
|
[Path Description] BA0
Pin AA18
  Len = 1 R = 0.308 L = 3.272E-09 C = 9.080E-13 / | substrate RLC
Fork
  Len = 1.698 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.114
Endfork
Fork
  Len = 1.712 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.114
Endfork
Fork
  Len = 1.734 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.114
Endfork
Fork
  Len = 1.764 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.114
Endfork
|
[Reference Designator Map]
|
| Ref Des  File name      Component name
U1         t69m.ibs       MT46H128M16LFT69M_DS
U2         t69m.ibs       MT46H128M16LFT69M_DS
U3         t69m.ibs       MT46H128M16LFT69M_DS
U4         t69m.ibs       MT46H128M16LFT69M_DS
[End Board Description]
|
[End]
