|***************************************************************************
|T69M EBD Model for 168-Ball TI-OMAP PoP 12 x 12 x 1.0mm VFBGA
|Quad Die LP-DDR DRAM
| 
|Part Number      VDD/VDDQ  Architecture  Package
|-----------      --------  ------------  -------
|MT46H256M32L4JV  1.8/1.8V  256Mb x32     168-Ball OMAP PoP
|
|***************************************************************************
|
[IBIS Ver]    4.0
[File name]   t69m_168b_4dp.ebd
[File rev]    1.1
[Date]        02/15/2010
[Source]      From SPICE model at Micron Technology, Inc.
                  Micron Technology, Inc.
                  8000 S. Federal Way
                  P.O. Box 6, M/S: 01-711
                  Boise, ID 83707-0006
              For support send e-mail to modelsupport@micron.com              
|
[Notes]       Rev 1.0: 06/19/2009
               - Initial revision of packaging ebd
              Rev 1.1: 02/15/2010
               - Updated EBD formatting
               - Updated Bondwire parasitics
               - Corrected the Part Number
|
              Notes:
               - U1, U2, U3, U4 are the LPDRAM bare die components
                 (MT46H128M16LFT69M_DS) defined in the IBIS file t69m.ibs
               - Please choose the appropriate speed grade and drive 
                 strength models from the bare die ibis components
               - In order to perform simulation using this model, 
                 *.ebd and *.ibs files must be in the same directory
|
[Disclaimer]  This software code and all associated documentation, comments
              or other information (collectively "Software") is provided
              "AS IS" without warranty of any kind. MICRON TECHNOLOGY, INC.
              ("MTI") EXPRESSLY DISCLAIMS ALL WARRANTIES EXPRESS OR IMPLIED,
              INCLUDING BUT NOT LIMITED TO, NONINFRINGEMENT OF THIRD PARTY
              RIGHTS, AND ANY IMPLIED WARRANTIES OF MERCHANTABILITY OR
              FITNESS FOR ANY PARTICULAR PURPOSE. MTI DOES NOT WARRANT THAT 
              THE SOFTWARE WILL MEET YOUR REQUIREMENTS, OR THAT THE 
              OPERATION OF THE SOFTWARE WILL BE UNINTERRUPTED OR ERROR-FREE. 
              FURTHERMORE, MTI DOES NOT MAKE ANY REPRESENTATIONS REGARDING
              THE USE OR THE RESULTS OF THE USE OF THE SOFTWARE IN TERMS OF
              ITS CORRECTNESS, ACCURACY, RELIABILITY, OR OTHERWISE. THE
              ENTIRE RISK ARISING OUT OF USE OR PERFORMANCE OF THE SOFTWARE
              REMAINS WITH YOU. IN NO EVENT SHALL MTI, ITS AFFILIATED
              COMPANIES OR THEIR SUPPLIERS BE LIABLE FOR ANY DIRECT,
              INDIRECT, CONSEQUENTIAL, INCIDENTAL, OR SPECIAL DAMAGES
              (INCLUDING, WITHOUT LIMITATION, DAMAGES FOR LOSS OF PROFITS,
              BUSINESS INTERRUPTION, OR LOSS OF INFORMATION) ARISING OUT OF
              YOUR USE OF OR INABILITY TO USE THE SOFTWARE, EVEN IF MTI HAS
              BEEN ADVISED OF THE POSSIBILITY OF SUCH DAMAGES. Because some
              jurisdictions prohibit the exclusion or limitation of 
              liability for consequential or incidental damages, the above
              limitation may not apply to you.
| 
[Copyright]   Copyright 2010 Micron Technology, Inc. All rights reserved.
|
|***************************************************************************
| Component MT46H256M32L4JV  (168-Ball 12mm x 12mm x 1.0mm TI-OMAP PoP) 
|***************************************************************************
|
[Begin Board Description] MT46H256M32L4JV 
[Manufacturer] Micron Technology, Inc.
|
[Number Of Pins]  168
|
[Pin List]     signal_name
A1             NC
A2             NC
A3             DQ17
A4             POWER
A5             DQ19
A6             DM2
A7             POWER
A8             DQ21
A9             DQ23
A10            POWER
A11            CK
A12            POWER
A13            DQ9
A14            DQ11
A15            POWER
A16            DQ13
A17            DM1
A18            POWER
A19            DQ15
A20            DM3
A21            DQ25
A22            NC
A23            NC
B1             NC
B2             NC
B3             DQ16
B4             GND
B5             DQ18
B6             DQS2
B7             GND
B8             DQ20
B9             DQ22
B10            GND
B11            CK#
B12            GND
B13            DQ8
B14            DQ10
B15            GND
B16            DQ12
B17            DQS1
B18            GND
B19            DQ14
B20            DQS3
B21            DQ24
B22            NC
B23            NC
C1             DM0
C2             DQS0
C22            GND
C23            POWER
D1             DQ7
D2             DQ6
D22            DQ26
D23            DQ27
E1             POWER
E2             GND
E22            DQ28
E23            DQ29
F1             DQ5
F2             DQ4
F22            GND
F23            POWER
G1             DQ3
G2             DQ2
G22            DQ30
G23            DQ31
H1             POWER
H2             GND
H22            GND
H23            POWER
J1             DQ1
J2             DQ0
J22            CKE0
J23            CKE1
K1             POWER
K2             GND
K22            GND
K23            WE#
L1             NC
L2             GND
L22            CAS#
L23            RAS#
M1             NC
M2             NC
M22            CS0#
M23            CS1#
N1             NC
N2             NC
N22            A0
N23            A1
P1             NC
P2             GND
P22            A2
P23            A3
R1             NC
R2             NC
R22            A4
R23            A5
T1             NC
T2             NC
T22            A6
T23            A7
U1             NC
U2             GND
U22            A8
U23            A9
V1             NC
V2             NC
V22            A10
V23            A11
W1             NC
W2             NC
W22            A12
W23            A13
Y1             NC
Y2             NC
Y22            A14
Y23            POWER
AA1            NC
AA2            GND
AA22           GND
AA23           POWER
AB1            NC
AB2            NC
AB3            NC
AB4            NC
AB5            GND
AB6            NC
AB7            NC
AB8            GND
AB9            NC
AB10           NC
AB11           NC
AB12           NC
AB13           GND
AB14           GND
AB15           NC
AB16           NC
AB17           NC
AB18           NC
AB19           NC
AB20           GND
AB21           BA0
AB22           NC
AB23           NC
AC1            NC
AC2            NC
AC3            NC
AC4            NC
AC5            GND
AC6            NC
AC7            NC
AC8            NC
AC9            NC
AC10           NC
AC11           NC
AC12           NC
AC13           NC
AC14           NC
AC15           NC
AC16           NC
AC17           NC
AC18           NC
AC19           NC
AC20           NC
AC21           BA1
AC22           NC
AC23           NC
|
[Path Description] DQ17
Pin A3
  Len = 1 R = 0.198 L = 1.963E-09 C = 1.118E-12 / | substrate RLC
Fork
  Len = 1.648 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.21
Endfork
Fork
  Len = 1.995 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.21
Endfork
|
[Path Description] DQ19
Pin A5
  Len = 1 R = 0.208 L = 1.781E-09 C = 1.151E-12 / | substrate RLC
Fork
  Len = 1.518 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.23
Endfork
Fork
  Len = 1.836 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.23
Endfork
|
[Path Description] DM2
Pin A6
  Len = 1 R = 0.402 L = 3.949E-09 C = 1.690E-12 / | substrate RLC
Fork
  Len = 1.688 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.33
Endfork
Fork
  Len = 2.043 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.33
Endfork
|
[Path Description] DQ21
Pin A8
  Len = 1 R = 0.114 L = 1.153E-09 C = 8.658E-13 / | substrate RLC
Fork
  Len = 1.479 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.27
Endfork
Fork
  Len = 1.789 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.27
Endfork
|
[Path Description] DQ23
Pin A9
  Len = 1 R = 0.170 L = 1.581E-09 C = 1.022E-12 / | substrate RLC
Fork
  Len = 1.542 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.29
Endfork
Fork
  Len = 1.865 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.29
Endfork
|
[Path Description] CK
Pin A11
  Len = 1 R = 0.233 L = 2.084E-09 C = 1.267E-12 / | substrate RLC
Fork
  Len = 1.536 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.51
Endfork
Fork
  Len = 1.690 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.51
Endfork
Fork
  Len = 1.859 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.51
Endfork
Fork
  Len = 2.045 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.51
Endfork
|
[Path Description] DQ9
Pin A13
  Len = 1 R = 0.233 L = 2.572E-09 C = 1.490E-12 / | substrate RLC
Fork
  Len = 1.471 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.69
Endfork
Fork
  Len = 1.780 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.69
Endfork
|
[Path Description] DQ11
Pin A14
  Len = 1 R = 0.186 L = 1.820E-09 C = 1.323E-12 / | substrate RLC
Fork
  Len = 1.466 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.71
Endfork
Fork
  Len = 1.774 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.71
Endfork
|
[Path Description] DQ13
Pin A16
  Len = 1 R = 0.187 L = 1.987E-09 C = 1.402E-12 / | substrate RLC
Fork
  Len = 1.576 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.75
Endfork
Fork
  Len = 1.907 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.75
Endfork
|
[Path Description] DM1
Pin A17
  Len = 1 R = 0.411 L = 4.668E-09 C = 2.040E-12 / | substrate RLC
Fork
  Len = 1.636 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.64
Endfork
Fork
  Len = 1.979 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.64
Endfork
|
[Path Description] DQ15
Pin A19
  Len = 1 R = 0.094 L = 8.311E-10 C = 1.198E-12 / | substrate RLC
Fork
  Len = 1.778 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.77
Endfork
Fork
  Len = 2.151 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.77
Endfork
|
[Path Description] DM3
Pin A20
  Len = 1 R = 0.471 L = 5.432E-09 C = 1.872E-12 / | substrate RLC
Fork
  Len = 1.729 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.64
Endfork
Fork
  Len = 2.092 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.64
Endfork
|
[Path Description] DQ25
Pin A21
  Len = 1 R = 0.482 L = 4.826E-09 C = 1.795E-12 / | substrate RLC
Fork
  Len = 1.516 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.69
Endfork
Fork
  Len = 1.834 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.69
Endfork
|
[Path Description] DQ16
Pin B3
  Len = 1 R = 0.166 L = 1.741E-09 C = 1.115E-12 / | substrate RLC
Fork
  Len = 1.753 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.20
Endfork
Fork
  Len = 2.121 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.20
Endfork
|
[Path Description] DQ18
Pin B5
  Len = 1 R = 0.146 L = 1.303E-09 C = 1.054E-12 / | substrate RLC
Fork
  Len = 1.571 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.22
Endfork
Fork
  Len = 1.901 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.22
Endfork
|
[Path Description] DQS2
Pin B6
  Len = 1 R = 0.342 L = 3.467E-09 C = 1.609E-12 / | substrate RLC
Fork
  Len = 1.598 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.32
Endfork
Fork
  Len = 1.934 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.32
Endfork
|
[Path Description] DQ20
Pin B8
  Len = 1 R = 0.114 L = 1.084E-09 C = 9.935E-13 / | substrate RLC
Fork
  Len = 1.480 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.26
Endfork
Fork
  Len = 1.791 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.26
Endfork
|
[Path Description] DQ22
Pin B9
  Len = 1 R = 0.102 L = 1.037E-09 C = 9.567E-13 / | substrate RLC
Fork
  Len = 1.499 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.28
Endfork
Fork
  Len = 1.814 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.28
Endfork
|
[Path Description] CK#
Pin B11
  Len = 1 R = 0.248 L = 2.294E-09 C = 1.419E-12 / | substrate RLC
Fork
  Len = 1.523 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.52
Endfork
Fork
  Len = 1.675 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.52
Endfork
Fork
  Len = 1.843 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.52
Endfork
Fork
  Len = 2.027 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.52
Endfork
|
[Path Description] DQ8
Pin B13
  Len = 1 R = 0.241 L = 2.657E-09 C = 1.653E-12 / | substrate RLC
Fork
  Len = 1.506 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.68
Endfork
Fork
  Len = 1.823 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.68
Endfork
|
[Path Description] DQ10
Pin B14
  Len = 1 R = 0.163 L = 1.829E-09 C = 1.377E-12 / | substrate RLC
Fork
  Len = 1.458 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.70
Endfork
Fork
  Len = 1.764 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.70
Endfork
|
[Path Description] DQ12
Pin B16
  Len = 1 R = 0.168 L = 1.695E-09 C = 1.423E-12 / | substrate RLC
Fork
  Len = 1.514 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.74
Endfork
Fork
  Len = 1.832 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.74
Endfork
|
[Path Description] DQS1
Pin B17
  Len = 1 R = 0.335 L = 3.860E-09 C = 1.888E-12 / | substrate RLC
Fork
  Len = 1.555 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.65
Endfork
Fork
  Len = 1.881 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.65
Endfork
|
[Path Description] DQ14
Pin B19
  Len = 1 R = 0.085 L = 7.371E-10 C = 1.177E-12 / | substrate RLC
Fork
  Len = 1.663 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.76
Endfork
Fork
  Len = 2.012 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.76
Endfork
|
[Path Description] DQS3
Pin B20
  Len = 1 R = 0.386 L = 4.500E-09 C = 1.701E-12 / | substrate RLC
Fork
  Len = 1.631 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.65
Endfork
Fork
  Len = 1.973 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.65
Endfork
|
[Path Description] DQ24
Pin B21
  Len = 1 R = 0.399 L = 4.213E-09 C = 1.737E-12 / | substrate RLC
Fork
  Len = 1.568 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.68
Endfork
Fork
  Len = 1.897 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.68
Endfork
|
[Path Description] DM0
Pin C1
  Len = 1 R = 0.506 L = 5.615E-09 C = 2.303E-12 / | substrate RLC
Fork
  Len = 1.756 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.33
Endfork
Fork
  Len = 2.125 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.33
Endfork
|
[Path Description] DQS0
Pin C2
  Len = 1 R = 0.427 L = 4.771E-09 C = 2.148E-12 / | substrate RLC
Fork
  Len = 1.646 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.32
Endfork
Fork
  Len = 1.992 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.32
Endfork
|
[Path Description] DQ7
Pin D1
  Len = 1 R = 0.414 L = 4.488E-09 C = 2.059E-12 / | substrate RLC
Fork
  Len = 1.573 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.29
Endfork
Fork
  Len = 1.904 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.29
Endfork
|
[Path Description] DQ6
Pin D2
  Len = 1 R = 0.341 L = 4.007E-09 C = 1.903E-12 / | substrate RLC
Fork
  Len = 1.512 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.28
Endfork
Fork
  Len = 1.830 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.28
Endfork
|
[Path Description] DQ26
Pin D22
  Len = 1 R = 0.354 L = 3.821E-09 C = 1.624E-12 / | substrate RLC
Fork
  Len = 1.485 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.70
Endfork
Fork
  Len = 1.797 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.70
Endfork
|
[Path Description] DQ27
Pin D23
  Len = 1 R = 0.405 L = 4.352E-09 C = 1.685E-12 / | substrate RLC
Fork
  Len = 1.477 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.71
Endfork
Fork
  Len = 1.787 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.71
Endfork
|
[Path Description] DQ28
Pin E22
  Len = 1 R = 0.303 L = 3.158E-09 C = 1.545E-12 / | substrate RLC
Fork
  Len = 1.500 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.74
Endfork
Fork
  Len = 1.815 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.74
Endfork
|
[Path Description] DQ29
Pin E23
  Len = 1 R = 0.345 L = 3.530E-09 C = 1.572E-12 / | substrate RLC
Fork
  Len = 1.544 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.75
Endfork
Fork
  Len = 1.868 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.75
Endfork
|
[Path Description] DQ5
Pin F1
  Len = 1 R = 0.387 L = 4.498E-09 C = 1.903E-12 / | substrate RLC
Fork
  Len = 1.474 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.27
Endfork
Fork
  Len = 1.784 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.27
Endfork
|
[Path Description] DQ4
Pin F2
  Len = 1 R = 0.305 L = 3.503E-09 C = 1.832E-12 / | substrate RLC
Fork
  Len = 1.458 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.26
Endfork
Fork
  Len = 1.764 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.26
Endfork
|
[Path Description] DQ3
Pin G1
  Len = 1 R = 0.348 L = 3.730E-09 C = 1.806E-12 / | substrate RLC
Fork
  Len = 1.472 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.23
Endfork
Fork
  Len = 1.781 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.23
Endfork
|
[Path Description] DQ2
Pin G2
  Len = 1 R = 0.259 L = 3.074E-09 C = 1.637E-12 / | substrate RLC
Fork
  Len = 1.509 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.22
Endfork
Fork
  Len = 1.825 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.22
Endfork
|
[Path Description] DQ30
Pin G22
  Len = 1 R = 0.259 L = 2.804E-09 C = 1.452E-12 / | substrate RLC
Fork
  Len = 1.612 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.76
Endfork
Fork
  Len = 1.950 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.76
Endfork
|
[Path Description] DQ31
Pin G23
  Len = 1 R = 0.326 L = 3.428E-09 C = 1.574E-12 / | substrate RLC
Fork
  Len = 1.706 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.77
Endfork
Fork
  Len = 2.065 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.77
Endfork
|
[Path Description] DQ1
Pin J1
  Len = 1 R = 0.373 L = 4.279E-09 C = 1.931E-12 / | substrate RLC
Fork
  Len = 1.569 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.21
Endfork
Fork
  Len = 1.898 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.21
Endfork
|
[Path Description] DQ0
Pin J2
  Len = 1 R = 0.322 L = 3.389E-09 C = 1.945E-12 / | substrate RLC
Fork
  Len = 1.655 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.20
Endfork
Fork
  Len = 2.003 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.20
Endfork
|
[Path Description] CKE0
Pin J22
  Len = 1 R = 0.460 L = 5.708E-09 C = 1.984E-12 / | substrate RLC
Fork
  Len = 1.452 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.120
Endfork
Fork
  Len = 1.597 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.120
Endfork
|
[Path Description] CKE1
Pin J23
  Len = 1 R = 0.479 L = 6.173E-09 C = 1.827E-12 / | substrate RLC
Fork
  Len = 1.796 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.120
Endfork
Fork
  Len = 1.975 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.120
Endfork
|
[Path Description] WE#
Pin K23
  Len = 1 R = 0.459 L = 5.976E-09 C = 2.108E-12 / | substrate RLC
Fork
  Len = 1.483 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.119
Endfork
Fork
  Len = 1.631 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.119
Endfork
Fork
  Len = 1.794 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.119
Endfork
Fork
  Len = 1.973 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.119
Endfork
|
[Path Description] CAS#
Pin L22
  Len = 1 R = 0.412 L = 5.462E-09 C = 2.027E-12 / | substrate RLC
Fork
  Len = 1.483 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.118
Endfork
Fork
  Len = 1.631 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.118
Endfork
Fork
  Len = 1.794 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.118
Endfork
Fork
  Len = 1.973 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.118
Endfork
|
[Path Description] RAS#
Pin L23
  Len = 1 R = 0.426 L = 5.577E-09 C = 1.820E-12 / | substrate RLC
Fork
  Len = 1.485 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.117
Endfork
Fork
  Len = 1.633 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.117
Endfork
Fork
  Len = 1.797 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.117
Endfork
Fork
  Len = 1.976 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.117
Endfork
|
[Path Description] CS0#
Pin M22
  Len = 1 R = 0.349 L = 4.761E-09 C = 1.693E-12 / | substrate RLC
Fork
  Len = 1.477 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.116
Endfork
Fork
  Len = 1.625 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.116
Endfork
|
[Path Description] CS1#
Pin M23
  Len = 1 R = 0.376 L = 5.186E-09 C = 1.378E-12 / | substrate RLC
Fork
  Len = 1.810 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.116
Endfork
Fork
  Len = 1.991 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.116
Endfork
|
[Path Description] A0
Pin N22
  Len = 1 R = 0.304 L = 4.403E-09 C = 1.672E-12 / | substrate RLC
Fork
  Len = 1.483 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.112
Endfork
Fork
  Len = 1.631 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.112
Endfork
Fork
  Len = 1.794 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.112
Endfork
Fork
  Len = 1.974 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.112
Endfork
|
[Path Description] A1
Pin N23
  Len = 1 R = 0.324 L = 4.590E-09 C = 1.609E-12 / | substrate RLC
Fork
  Len = 1.483 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.111
Endfork
Fork
  Len = 1.631 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.111
Endfork
Fork
  Len = 1.794 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.111
Endfork
Fork
  Len = 1.974 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.111
Endfork
|
[Path Description] A2
Pin P22
  Len = 1 R = 0.268 L = 4.015E-09 C = 1.424E-12 / | substrate RLC
Fork
  Len = 1.483 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.110
Endfork
Fork
  Len = 1.632 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.110
Endfork
Fork
  Len = 1.795 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.110
Endfork
Fork
  Len = 1.974 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.110
Endfork
|
[Path Description] A3
Pin P23
  Len = 1 R = 0.278 L = 4.077E-09 C = 1.103E-12 / | substrate RLC
Fork
  Len = 1.505 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.109
Endfork
Fork
  Len = 1.655 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.109
Endfork
Fork
  Len = 1.821 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.109
Endfork
Fork
  Len = 2.003 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.109
Endfork
|
[Path Description] A4
Pin R22
  Len = 1 R = 0.402 L = 5.532E-09 C = 1.627E-12 / | substrate RLC
Fork
  Len = 1.504 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.132
Endfork
Fork
  Len = 1.654 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.132
Endfork
Fork
  Len = 1.819 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.132
Endfork
Fork
  Len = 2.001 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.132
Endfork
|
[Path Description] A5
Pin R23
  Len = 1 R = 0.416 L = 5.699E-09 C = 1.766E-12 / | substrate RLC
Fork
  Len = 1.483 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.131
Endfork
Fork
  Len = 1.632 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.131
Endfork
Fork
  Len = 1.795 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.131
Endfork
Fork
  Len = 1.974 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.131
Endfork
|
[Path Description] A6
Pin T22
  Len = 1 R = 0.370 L = 5.207E-09 C = 1.848E-12 / | substrate RLC
Fork
  Len = 1.483 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.130
Endfork
Fork
  Len = 1.631 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.130
Endfork
Fork
  Len = 1.794 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.130
Endfork
Fork
  Len = 1.974 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.130
Endfork
|
[Path Description] A7
Pin T23
  Len = 1 R = 0.392 L = 5.389E-09 C = 1.776E-12 / | substrate RLC
Fork
  Len = 1.483 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.129
Endfork
Fork
  Len = 1.631 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.129
Endfork
Fork
  Len = 1.794 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.129
Endfork
Fork
  Len = 1.974 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.129
Endfork
|
[Path Description] A8
Pin U22
  Len = 1 R = 0.343 L = 4.916E-09 C = 1.735E-12 / | substrate RLC
Fork
  Len = 1.483 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.128
Endfork
Fork
  Len = 1.632 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.128
Endfork
Fork
  Len = 1.795 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.128
Endfork
Fork
  Len = 1.975 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.128
Endfork
|
[Path Description] A9
Pin U23
  Len = 1 R = 0.373 L = 5.197E-09 C = 1.673E-12 / | substrate RLC
Fork
  Len = 1.487 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.127
Endfork
Fork
  Len = 1.636 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.127
Endfork
Fork
  Len = 1.800 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.127
Endfork
Fork
  Len = 1.979 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.127
Endfork
|
[Path Description] A10
Pin V22
  Len = 1 R = 0.236 L = 3.237E-09 C = 1.381E-12 / | substrate RLC
Fork
  Len = 1.483 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.113
Endfork
Fork
  Len = 1.632 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.113
Endfork
Fork
  Len = 1.795 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.113
Endfork
Fork
  Len = 1.974 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.113
Endfork
|
[Path Description] A11
Pin V23
  Len = 1 R = 0.365 L = 4.975E-09 C = 1.637E-12 / | substrate RLC
Fork
  Len = 1.488 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.126
Endfork
Fork
  Len = 1.637 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.126
Endfork
Fork
  Len = 1.801 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.126
Endfork
Fork
  Len = 1.981 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.126
Endfork
|
[Path Description] A12
Pin W22
  Len = 1 R = 0.316 L = 4.465E-09 C = 1.387E-12 / | substrate RLC
Fork
  Len = 1.496 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.125
Endfork
Fork
  Len = 1.645 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.125
Endfork
Fork
  Len = 1.810 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.125
Endfork
Fork
  Len = 1.991 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.125
Endfork
|
[Path Description] A13
Pin W23
  Len = 1 R = 0.335 L = 4.278E-09 C = 1.327E-12 / | substrate RLC
Fork
  Len = 1.501 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.124
Endfork
Fork
  Len = 1.651 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.124
Endfork
Fork
  Len = 1.816 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.124
Endfork
Fork
  Len = 1.998 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.124
Endfork
|
[Path Description] A14
Pin Y22
  Len = 1 R = 0.304 L = 3.631E-09 C = 1.440E-12 / | substrate RLC
|
[Path Description] BA0
Pin AB21
  Len = 1 R = 0.199 L = 2.406E-09 C = 1.183E-12 / | substrate RLC
Fork
  Len = 1.487 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.114
Endfork
Fork
  Len = 1.636 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.114
Endfork
Fork
  Len = 1.799 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.114
Endfork
Fork
  Len = 1.979 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.114
Endfork
|
[Path Description] BA1
Pin AC21
  Len = 1 R = 0.203 L = 2.672E-09 C = 1.050E-12 / | substrate RLC
Fork
  Len = 1.488 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U1.115
Endfork
Fork
  Len = 1.637 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U2.115
Endfork
Fork
  Len = 1.801 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U3.115
Endfork
Fork
  Len = 1.981 R = 0.07764 L = 4.22e-10 C = 6.05e-14 / | bondwire RLC
  Node U4.115
Endfork
| 
[Reference Designator Map]
|
| Ref Des  File name      Component name
U1         t69m.ibs       MT46H128M16LFT69M_DS
U2         t69m.ibs       MT46H128M16LFT69M_DS
U3         t69m.ibs       MT46H128M16LFT69M_DS
U4         t69m.ibs       MT46H128M16LFT69M_DS
[End Board Description]
|
[End]

