#
# Tags:
#
# S	Symbol name (must be first)
# M	Package marking
# N	Data sheet identifier (N tag of BOOKSHELF; can be omitted if equal to S)
#

# Atmel AT86RF230 2.4 GHz Transceiver for IEEE 802.15.4
S: at86rf230

# Atmel AT86RF231 2.4 GHz Transceiver for IEEE 802.15.4
S: at86rf231

# Fairly generic crystal package with 4 pins (crystal connects pins 1 and 3,
# the rest is ground)
S: xtal-4
N: nx3225sa

# Generic antenna with ground on pin 1, feed on pin 2
S: antenna

# SMT balun configuration (using 5 contacts)
# Example: Wuerth 748421245 balun/filter
S: balun
N: 748421245

# SMT balun configuration (using 6 contacts)
# Example: Johanson 2450FB15L0001 balun/filter
S: balun-smt6
N: 2450FB15L0001
