Cmp-Mod V01 Created by CvPCB (2010-08-11 BZR 2448)-unstable date = Sat Nov  6 02:05:09 2010

BeginCmp
TimeStamp = /4C6401B3;
Reference = C1;
ValeurCmp = 100nF;
IdModule  = 0603-M;
EndCmp

BeginCmp
TimeStamp = /4C6401AA;
Reference = C2;
ValeurCmp = 1uF;
IdModule  = 0603-M;
EndCmp

BeginCmp
TimeStamp = /4CC53108;
Reference = CON1;
ValeurCmp = USB_A_PLUG_;
IdModule  = USB-A-PLUG-SMT;
EndCmp

BeginCmp
TimeStamp = /4C6402EE;
Reference = D1;
ValeurCmp = LTST-C190KRKT;
IdModule  = 0603-M;
EndCmp

BeginCmp
TimeStamp = /4C640203;
Reference = P1;
ValeurCmp = CONN_1;
IdModule  = PAD_120x60;
EndCmp

BeginCmp
TimeStamp = /4C6401FE;
Reference = P2;
ValeurCmp = CONN_1;
IdModule  = PAD_120x60;
EndCmp

BeginCmp
TimeStamp = /4C640200;
Reference = P3;
ValeurCmp = CONN_1;
IdModule  = PAD_120x60;
EndCmp

BeginCmp
TimeStamp = /4C640202;
Reference = P4;
ValeurCmp = CONN_1;
IdModule  = PAD_120x60;
EndCmp

BeginCmp
TimeStamp = /4CD4DF6F;
Reference = P5;
ValeurCmp = CONN_1;
IdModule  = PAD_120x60;
EndCmp

BeginCmp
TimeStamp = /4CD4DF72;
Reference = P6;
ValeurCmp = CONN_1;
IdModule  = PAD_120x60;
EndCmp

BeginCmp
TimeStamp = /4CD4DF74;
Reference = P7;
ValeurCmp = CONN_1;
IdModule  = PAD_120x60;
EndCmp

BeginCmp
TimeStamp = /4C71B06B;
Reference = R1;
ValeurCmp = 1k;
IdModule  = 0603-M;
EndCmp

BeginCmp
TimeStamp = /4CC5326F;
Reference = R2;
ValeurCmp = 330;
IdModule  = 0603-M;
EndCmp

BeginCmp
TimeStamp = /4C6402F2;
Reference = R3;
ValeurCmp = 68;
IdModule  = 0603-M;
EndCmp

BeginCmp
TimeStamp = /4C71AEC6;
Reference = U1;
ValeurCmp = C8051F320;
IdModule  = LQFP32;
EndCmp

BeginCmp
TimeStamp = /4C6402FB;
Reference = VR1;
ValeurCmp = 5V6;
IdModule  = 0402-M;
EndCmp

BeginCmp
TimeStamp = /4C640343;
Reference = VR2;
ValeurCmp = 5V6;
IdModule  = 0402-M;
EndCmp

BeginCmp
TimeStamp = /4C64034D;
Reference = VR3;
ValeurCmp = 5V6;
IdModule  = 0402-M;
EndCmp

BeginCmp
TimeStamp = /4C71BA9B;
Reference = VR4;
ValeurCmp = 5V6;
IdModule  = 0402-M;
EndCmp

EndListe
