Cmp-Mod V01 Created by CvPCB (2010-12-27 BZR 2685)-unstable date = Wed Mar 30 12:33:00 2011

BeginCmp
TimeStamp = /4C609C08/4C63FE17;
Reference = ANT1;
ValeurCmp = 50R;
IdModule  = MEANDER-110;
EndCmp

BeginCmp
TimeStamp = /4C609C08/4CF4B034;
Reference = B1;
ValeurCmp = 2450FB15L0001;
IdModule  = 0805-6;
EndCmp

BeginCmp
TimeStamp = /4C609BEF/4C6401AA;
Reference = C1;
ValeurCmp = 10uF;
IdModule  = 0603;
EndCmp

BeginCmp
TimeStamp = /4C609BEF/4C6401B3;
Reference = C2;
ValeurCmp = 1uF;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4C609C08/4C641710;
Reference = C3;
ValeurCmp = 22pF/RF;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4C609C08/4C641506;
Reference = C8;
ValeurCmp = 22pF/RF;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4C609C08/4C641509;
Reference = C9;
ValeurCmp = 22pF/RF;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4C609C08/4C640A76;
Reference = C10;
ValeurCmp = 1uF;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4C609C08/4C641004;
Reference = C11;
ValeurCmp = 1uF;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4C609C08/4C640A84;
Reference = C12;
ValeurCmp = 1uF;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4C609C08/4C640A7E;
Reference = C13;
ValeurCmp = 1uF;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4C609C08/4C640A73;
Reference = C14;
ValeurCmp = 12pF;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4C609C08/4C640A7B;
Reference = C15;
ValeurCmp = 12pF;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4C609C08/4D3B018B;
Reference = C16;
ValeurCmp = NC;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4C609C08/4D425FF1;
Reference = C17;
ValeurCmp = 2.2pF;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4C609BEF/4CF4AD1B;
Reference = CON1;
ValeurCmp = USB_A_PLUG;
IdModule  = USB-A-PLUG-SMT;
EndCmp

BeginCmp
TimeStamp = /4C609BEF/4C6402EE;
Reference = D1;
ValeurCmp = LTST-C190KRKT;
IdModule  = 0603;
EndCmp

BeginCmp
TimeStamp = /4C609BEF/4C6401FE;
Reference = P11;
ValeurCmp = CONN_1;
IdModule  = PAD_60x60;
EndCmp

BeginCmp
TimeStamp = /4C609BEF/4C640200;
Reference = P12;
ValeurCmp = CONN_1;
IdModule  = PAD_60x60;
EndCmp

BeginCmp
TimeStamp = /4C609BEF/4C640202;
Reference = P13;
ValeurCmp = CONN_1;
IdModule  = PAD_60x60;
EndCmp

BeginCmp
TimeStamp = /4C609BEF/4C640203;
Reference = P14;
ValeurCmp = CONN_1;
IdModule  = PAD_60x60;
EndCmp

BeginCmp
TimeStamp = /4C609BEF/4D425D53;
Reference = P15;
ValeurCmp = CONN_1;
IdModule  = PAD_60x60;
EndCmp

BeginCmp
TimeStamp = /4C609BEF/4D425D62;
Reference = P16;
ValeurCmp = CONN_1;
IdModule  = PAD_60x60;
EndCmp

BeginCmp
TimeStamp = /4C609BEF/4C6402F2;
Reference = R1;
ValeurCmp = 180;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4C609C08/4CF4B07E;
Reference = R3;
ValeurCmp = 0R;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4C609BEF/4D4258D9;
Reference = R4;
ValeurCmp = 22;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4C609BEF/4D4258DC;
Reference = R5;
ValeurCmp = 22;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4C609C08/4D425FEE;
Reference = R6;
ValeurCmp = 180;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4C609BEF/4D425860;
Reference = U1;
ValeurCmp = ATMEGA32U2;
IdModule  = QFN32-VHHD-2;
EndCmp

BeginCmp
TimeStamp = /4C609C08/4D229690;
Reference = U2;
ValeurCmp = AT86RF231;
IdModule  = QFN32-VHHD-6;
EndCmp

BeginCmp
TimeStamp = /4C609BEF/4C6402FB;
Reference = VR1;
ValeurCmp = 5V6;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4C609BEF/4C640343;
Reference = VR2;
ValeurCmp = 5V6;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4C609BEF/4C64034D;
Reference = VR3;
ValeurCmp = 5V6;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4C609C08/4C63FA9F;
Reference = X1;
ValeurCmp = 16MHz;
IdModule  = xtal4-3.2mmx2.5mm;
EndCmp

EndListe
