Cmp-Mod V01 Created by CvPCB (2010-12-27 BZR 2685)-unstable date = Fri Feb 18 15:23:11 2011

BeginCmp
TimeStamp = /4C63FE17;
Reference = ANT1;
ValeurCmp = 50R;
IdModule  = MEANDER-110;
EndCmp

BeginCmp
TimeStamp = /4D22A4C6;
Reference = B1;
ValeurCmp = 2450FB15L0001;
IdModule  = 0805-6;
EndCmp

BeginCmp
TimeStamp = /4C7FBF1B;
Reference = C1;
ValeurCmp = 22pF/RF;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4C7FBF1E;
Reference = C2;
ValeurCmp = 22pF/RF;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4C640A76;
Reference = C3;
ValeurCmp = 1uF;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4C641004;
Reference = C4;
ValeurCmp = 1uF;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4C640A84;
Reference = C5;
ValeurCmp = 1uF;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4C640A7E;
Reference = C6;
ValeurCmp = 1uF;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4D317091;
Reference = C10;
ValeurCmp = 12pF;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4D317089;
Reference = C11;
ValeurCmp = 12pF;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4D3AF01F;
Reference = C12;
ValeurCmp = NC;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4C640CD5;
Reference = P1;
ValeurCmp = TST;
IdModule  = PAD_2mm;
EndCmp

BeginCmp
TimeStamp = /4C7FB8B3;
Reference = P2;
ValeurCmp = CONN_8;
IdModule  = 8:10-card;
EndCmp

BeginCmp
TimeStamp = /4C8C121C;
Reference = R1;
ValeurCmp = 0R;
IdModule  = 0402;
EndCmp

BeginCmp
TimeStamp = /4D22A108;
Reference = U1;
ValeurCmp = AT86RF231;
IdModule  = QFN32-VHHD-6;
EndCmp

BeginCmp
TimeStamp = /4D317045;
Reference = X1;
ValeurCmp = 16MHz;
IdModule  = xtal4-3.2mmx2.5mm;
EndCmp

EndListe
