# EESchema Netlist Version 1.1 created  8/10/2009-21:32:20
(
 ( /4AABD9C0 $noname  H5 HD {Lib=HD}
 )
 ( /4AABD9BE $noname  H4 HD {Lib=HD}
 )
 ( /4AABD9BB $noname  H3 HD {Lib=HD}
 )
 ( /4AABD9B8 $noname  H2 HD {Lib=HD}
 )
 ( /4AABD9A9 $noname  H1 HD {Lib=HD}
 )
 ( /4AABC76A $noname  SW1 BOOT_SWITCH {Lib=SWITCH}
  (    1 GND )
  (    2 /BOOT_SEL1_HIGH )
  (    3 /BOOT_SEL1 )
 )
 ( /4A6D21E5 $noname  CON3 SERIAL_CON {Lib=SERIAL_CON}
  (  GND GND )
  (    1 GND )
  (    2 /TXD )
  (    3 /RXD )
 )
 ( /4A69AE84 $noname  C33 0.1uF/16V {Lib=C}
  (    1 /+V3.3 )
  (    2 GND )
 )
 ( /4A69AE83 $noname  C32 0.1uF/16V {Lib=C}
  (    1 /+V3.3 )
  (    2 GND )
 )
 ( /4A69AE82 $noname  C31 0.1uF/16V {Lib=C}
  (    1 /+V3.3 )
  (    2 GND )
 )
 ( /4A69AE81 $noname  C30 0.1uF/16V {Lib=C}
  (    1 /+V3.3 )
  (    2 GND )
 )
 ( /4A69AE80 $noname  C29 0.1uF/16V {Lib=C}
  (    1 /+V3.3 )
  (    2 GND )
 )
 ( /4A69AE7F $noname  C28 10uF/10V {Lib=C}
  (    1 /+V3.3 )
  (    2 GND )
 )
 ( /4A69AD04 $noname  C27 0.1uF/16V {Lib=C}
  (    1 /+V1.8 )
  (    2 GND )
 )
 ( /4A69AD03 $noname  C26 0.1uF/16V {Lib=C}
  (    1 /+V1.8 )
  (    2 GND )
 )
 ( /4A69ACF8 $noname  C25 0.1uF/16V {Lib=C}
  (    1 /+V1.8 )
  (    2 GND )
 )
 ( /4A69ACF7 $noname  C24 0.1uF/16V {Lib=C}
  (    1 /+V1.8 )
  (    2 GND )
 )
 ( /4A69ACCA $noname  C23 0.1uF/16V {Lib=C}
  (    1 /+V1.8 )
  (    2 GND )
 )
 ( /4A69AC9D $noname  C22 10uF/10V {Lib=C}
  (    1 /+V1.8 )
  (    2 GND )
 )
 ( /4A4747A9 $noname  U1 JZ4720_186P {Lib=JZ4720_186P}
  (    1 /LCD_USB/LCDD0 )
  (    2 /LCD_USB/DCLK )
  (    3 /MEMORY/D13 )
  (    4 /MEMORY/D14 )
  (    5 /MEMORY/D15 )
  (    6 /MEMORY/D11 )
  (    7 /+V3.3 )
  (    8 GND )
  (    9 GND )
  (   10 /+V1.8 )
  (   11 /MEMORY/D12 )
  (   12 /MEMORY/A3 )
  (   13 /MEMORY/A2 )
  (   14 /MEMORY/A1 )
  (   15 /MEMORY/A0 )
  (   16 /MEMORY/A10 )
  (   17 /MEMORY/DCS0_N )
  (   18 /MEMORY/RAS_N )
  (   19 /MEMORY/CAS_N )
  (   20 /MEMORY/RDWR_N )
  (   21 /+V1.8 )
  (   22 GND )
  (   23 /MEMORY/WE0_N )
  (   24 /MEMORY/WE1_N )
  (   25 /MEMORY/CKO )
  (   26 /MEMORY/CKE )
  (   27 /MEMORY/A12 )
  (   28 /MEMORY/A11 )
  (   29 GND )
  (   30 /+V1.8 )
  (   31 /MEMORY/A9 )
  (   32 /MEMORY/A8 )
  (   33 /+V3.3 )
  (   34 GND )
  (   35 /MEMORY/A7 )
  (   36 /MEMORY/A6 )
  (   37 /MEMORY/A5 )
  (   38 /MEMORY/A4 )
  (   39 /MEMORY/A13 )
  (   40 /MEMORY/A14 )
  (   41 /MEMORY/D4 )
  (   42 /MEMORY/D5 )
  (   43 /MEMORY/D6 )
  (   44 /+V1.8 )
  (   45 GND )
  (   46 /MEMORY/D7 )
  (   47 /MEMORY/D8 )
  (   48 GND )
  (   49 /+V3.3 )
  (   50 /MEMORY/D9 )
  (   51 /MEMORY/D10 )
  (   52 /MEMORY/D0 )
  (   53 /MEMORY/D1 )
  (   54 /MEMORY/D2 )
  (   55 /MEMORY/D3 )
  (   56 N-000129 )
  (   57 /MEMORY/BUZPWM )
  (   58 /MEMORY/FALE/GPB16 )
  (   59 /MEMORY/FCLE/GPB15 )
  (   60 /MEMORY/GPB30 )
  (   61 /MEMORY/POP )
  (   62 N-000086 )
  (   63 ? )
  (   64 /MEMORY/FWE_N )
  (   65 /MEMORY/FRE_N )
  (   66 /+V3.3 )
  (   67 GND )
  (   68 /MEMORY/FRB_N )
  (   69 /CHARGE_N )
  (   70 /MEMORY/CS2_N )
  (   71 /MEMORY/CS1_N )
  (   72 /RXD )
  (   73 /TXD )
  (   74 /KEY_MATRIX/KEYIN7 )
  (   75 /KEY_MATRIX/KEYIN6 )
  (   76 /+V1.8 )
  (   77 GND )
  (   78 N-000135 )
  (   79 N-000092 )
  (   80 N-000090 )
  (   81 N-000136 )
  (   82 N-000134 )
  (   83 N-000091 )
  (   84 /KEY_MATRIX/KEYIN1 )
  (   85 /KEY_MATRIX/KEYIN2 )
  (   86 /KEY_MATRIX/KEYIN5 )
  (   87 /KEY_MATRIX/KEYIN3 )
  (   88 /KEY_MATRIX/KEYIN4 )
  (   89 /XTAL )
  (   90 /EXTAL )
  (   91 /+V3.3 )
  (   92 /LCD_USB/BATIN )
  (   93 N-000186 )
  (   94 GND )
  (   95 /VDDADC )
  (   96 ? )
  (   97 ? )
  (   98 ? )
  (   99 ? )
  (  100 /+V1.8 )
  (  101 GND )
  (  102 GND )
  (  103 /+V1.8 )
  (  104 GND )
  (  105 /+V3.3 )
  (  106 /LCD_USB/HOST_DP1 )
  (  107 /LCD_USB/HOST_DM1 )
  (  108 GND )
  (  109 N-000208 )
  (  110 N-000210 )
  (  111 /+V3.3 )
  (  112 /+V3.3 )
  (  113 /LCD_USB/DN )
  (  114 /LCD_USB/DN )
  (  115 /LCD_USB/DP )
  (  116 /LCD_USB/DP )
  (  117 GND )
  (  118 GND )
  (  119 GND )
  (  120 /RCLK )
  (  121 /RCLKO )
  (  122 /+VRTC )
  (  123 /RESETP_N )
  (  124 /WAKEUP_N )
  (  125 /PW_ON_N )
  (  126 /+VDDHP )
  (  127 /+VDDHP )
  (  128 N-000077 )
  (  129 N-000077 )
  (  130 GND )
  (  131 GND )
  (  132 GND )
  (  133 GND )
  (  134 N-000063 )
  (  135 N-000063 )
  (  136 /+VDDHP )
  (  137 /+VDDHP )
  (  138 GND )
  (  139 /+VDDHP )
  (  140 /LCD_USB/VREF )
  (  141 /+VDDHP )
  (  142 GND )
  (  143 /AUDIO/MICBIAS )
  (  144 /AUDIO/MICIN )
  (  145 /BOOT_SEL1 )
  (  146 /BOOT_SEL0 )
  (  147 /TDO )
  (  148 /TDI )
  (  149 /TCLK )
  (  150 /TMS )
  (  151 /TRST_N )
  (  152 /SHUTDOWN )
  (  153 N-000073 )
  (  154 N-000132 )
  (  155 N-000085 )
  (  156 /LCD_USB/GPD15 )
  (  157 /MEMORY/GPB18 )
  (  158 N-000148 )
  (  159 N-000127 )
  (  160 N-000128 )
  (  161 /LCD_USB/VSYNC )
  (  162 /LCD_USB/HSYNC )
  (  163 /LCD_USB/LCDCS )
  (  164 /KEY_MATRIX/KEYOUT8 )
  (  165 /KEY_MATRIX/KEYOUT7 )
  (  166 /KEY_MATRIX/KEYOUT6 )
  (  167 /KEY_MATRIX/KEYOUT5 )
  (  168 /KEY_MATRIX/KEYOUT4 )
  (  169 /KEY_MATRIX/KEYOUT3 )
  (  170 /KEY_MATRIX/KEYOUT2 )
  (  171 GND )
  (  172 /+V1.8 )
  (  173 /KEY_MATRIX/KEYOUT1 )
  (  174 /LCD_USB/GPC9 )
  (  175 /LCD_USB/GPC8 )
  (  176 /LCD_USB/LCDD7 )
  (  177 /LCD_USB/LCDD6 )
  (  178 /LCD_USB/LCDD5 )
  (  179 /LCD_USB/LCDD4 )
  (  180 N-000027 )
  (  181 GND )
  (  182 /LCD_USB/LCDD3 )
  (  183 /LCD_USB/LCDD2 )
  (  184 GND )
  (  185 /+V3.3 )
  (  186 /LCD_USB/LCDD1 )
  (  187 GND )
 )
 ( /4A47775F $noname  C18 0.1uF/16V {Lib=C}
  (    1 /+VDDHP )
  (    2 GND )
 )
 ( /4A47773C $noname  BD3 PZ1608D221 {Lib=INDUCTOR}
  (    1 /+VDDHP )
  (    2 /+V3.3 )
 )
 ( /4A47773B $noname  C17 10uF/10V {Lib=C}
  (    1 /+VDDHP )
  (    2 GND )
 )
 ( /4A477662 $noname  BD2 PZ1608D221 {Lib=INDUCTOR}
  (    1 /VDDADC )
  (    2 /+V3.3 )
 )
 ( /4A477634 $noname  C15 0.1uF/16V {Lib=C}
  (    1 /VDDADC )
  (    2 GND )
 )
 ( /4A4774E2 $noname  R7 10K/5% {Lib=R}
  (    1 /+V3.3 )
  (    2 N-000027 )
 )
 ( /4A4774D7 $noname  R9 0 {Lib=R}
  (    1 /BOOT_SEL1_HIGH )
  (    2 GND )
 )
 ( /4A4774D0 $noname  R5 10K/5% {Lib=R}
  (    1 /+V3.3 )
  (    2 /BOOT_SEL1_HIGH )
 )
 ( /4A4774BC $noname  R4 10K/5% {Lib=R}
  (    1 /+V3.3 )
  (    2 /BOOT_SEL0 )
 )
 ( /4A47747E $noname  TP5 TESTPOINT {Lib=TESTPOINT}
  (    1 /TDO )
 )
 ( /4A477474 $noname  TP4 TESTPOINT {Lib=TESTPOINT}
  (    1 /TDI )
 )
 ( /4A477473 $noname  TP3 TESTPOINT {Lib=TESTPOINT}
  (    1 /TMS )
 )
 ( /4A47746C $noname  TP2 TESTPOINT {Lib=TESTPOINT}
  (    1 /TCLK )
 )
 ( /4A477446 $noname  TP1 TESTPOINT {Lib=TESTPOINT}
  (    1 /TRST_N )
 )
 ( /4A4772C9 $noname  C21 0.1uF/16V {Lib=C}
  (    1 /+VRTC )
  (    2 GND )
 )
 ( /4A477209 $noname  C13 10uF/10V {Lib=C}
  (    1 /+V1.8 )
  (    2 GND )
 )
 ( /4A4771E8 $noname  C14 0.1uF/16V {Lib=C}
  (    1 /+V1.8 )
  (    2 GND )
 )
 ( /4A477199 $noname  C16 0.01uF/16V {Lib=C}
  (    1 /+V1.8 )
  (    2 GND )
 )
 ( /4A47702A $noname  C4 33pF/16V {Lib=C}
  (    1 /RCLKO )
  (    2 GND )
 )
 ( /4A477029 $noname  C1 33pF/16V {Lib=C}
  (    1 /RCLK )
  (    2 GND )
 )
 ( /4A476FCC $noname  Y1 32768Hz {Lib=CRYSTAL}
  (    1 /RCLKO )
  (    2 /RCLK )
  (    3 GND )
 )
 ( /4A476F4D $noname  C8 33pF/16V {Lib=C}
  (    1 N-000022 )
  (    2 GND )
 )
 ( /4A476F10 $noname  C5 33pF/16V {Lib=C}
  (    1 /XTAL )
  (    2 GND )
 )
 ( /4A476EAC $noname  Y2 12MHz {Lib=CRYSTAL}
  (    1 N-000022 )
  (    2 /XTAL )
  (    3 GND )
 )
 ( /4A476E30 $noname  R8 330/5% {Lib=R}
  (    1 /EXTAL )
  (    2 N-000022 )
 )
 ( /4A476D68 $noname  R2 1M/5% {Lib=R}
  (    1 /XTAL )
  (    2 N-000022 )
 )
 ( /4A476D5E $noname  R1 1M/5% {Lib=R}
  (    1 /RCLK )
  (    2 /RCLKO )
 )
 ( /4A4493DC $noname  S1 RESETK {Lib=SW_METALDOMN}
  (    1 GND )
  (    2 /RESETP_N )
 )
 ( /4A4492F8 $noname  R16 100K/5% {Lib=R}
  (    1 /+VRTC )
  (    2 /WAKEUP_N )
 )
 ( /4A4492C8 $noname  Q2 TM2301N {Lib=TM2301N}
  (    1 /PW_ON_N )
  (    2 /+VRTC )
  (    3 /PWEN )
 )
 ( /4A4492AF $noname  S9 ONOFFK {Lib=SW_METALDOMN}
  (    1 GND )
  (    2 /WAKEUP_N )
 )
 ( /4A44929E $noname  R18 100K/5% {Lib=R}
  (    1 /PWEN )
  (    2 GND )
 )
 ( /4A449298 $noname  R17 100K/5% {Lib=R}
  (    1 /+VRTC )
  (    2 /PW_ON_N )
 )
 ( /4A439C70 $noname  R13 470K/5% {Lib=R}
  (    1 /+VRTC )
  (    2 /RESETP_N )
 )
 ( /4A439974 $noname  R19 470K/5% {Lib=R}
  (    1 /SHUTDOWN )
  (    2 /+V3.3 )
 )
 ( /4A439868 $noname  U6 BL8509-263DNRM {Lib=BL8509-263DNRM}
  (    1 GND )
  (    2 /RESETP_N )
  (    3 /+VRTC )
 )
 ( /4A439857 $noname  U7 BL8506-30NRM {Lib=BL8506-30NRM}
  (    1 /SHUTDOWN )
  (    2 GND )
  (    3 N-000018 )
 )
 ( /4A438B55 $noname  TP10 TESTPOINT {Lib=TESTPOINT}
  (    1 /+V1.8 )
 )
 ( /4A438B47 $noname  TP9 TESTPOINT {Lib=TESTPOINT}
  (    1 /+V3.3 )
 )
 ( /4A438B46 $noname  TP8 TESTPOINT {Lib=TESTPOINT}
  (    1 /+VBAT )
 )
 ( /4A438B45 $noname  TP7 TESTPOINT {Lib=TESTPOINT}
  (    1 N-000002 )
 )
 ( /4A438B44 $noname  TP6 TESTPOINT {Lib=TESTPOINT}
  (    1 /RESETP_N )
 )
 ( /4A438B3F $noname  TP76 TESTPOINT {Lib=TESTPOINT}
  (    1 GND )
 )
 ( /4A438B3E $noname  TP77 TESTPOINT {Lib=TESTPOINT}
  (    1 /WAKEUP_N )
 )
 ( /4A438B33 $noname  TP78 TESTPOINT {Lib=TESTPOINT}
  (    1 /SHUTDOWN )
 )
 ( /4A438A93 $noname  TP32 TESTPOINT {Lib=TESTPOINT}
  (    1 /CHARGE_N )
 )
 ( /4A41ABF6 $noname  R6 150K/1% {Lib=R}
  (    1 N-000013 )
  (    2 GND )
 )
 ( /4A41ABF5 $noname  R3 680K/1% {Lib=R}
  (    1 /+V3.3 )
  (    2 N-000013 )
 )
 ( /4A41ABF4 $noname  C3 0.1uF/16V {Lib=C}
  (    1 /+V3.3 )
  (    2 GND )
 )
 ( /4A41ABF3 $noname  C2 10uF/10V {Lib=C}
  (    1 /+V3.3 )
  (    2 GND )
 )
 ( /4A41ABF2 $noname  C7 10pF/16V {Lib=C}
  (    1 /+V3.3 )
  (    2 N-000013 )
 )
 ( /4A41ABF1 $noname  L1 4.7uH/1A {Lib=INDUCTORP}
  (    1 N-000015 )
  (    2 /+V3.3 )
 )
 ( /4A41ABEC $noname  C6 10uF/10V {Lib=C}
  (    1 N-000018 )
  (    2 GND )
 )
 ( /4A41ABEA $noname  U2 EUP3406 {Lib=EUP3406}
  (    1 /PWEN )
  (    2 GND )
  (    3 N-000015 )
  (    4 N-000018 )
  (    5 N-000013 )
 )
 ( /4A41A947 $noname  R11 150K/1% {Lib=R}
  (    1 N-000016 )
  (    2 GND )
 )
 ( /4A41A896 $noname  R10 300K/1% {Lib=R}
  (    1 /+V1.8 )
  (    2 N-000016 )
 )
 ( /4A41A891 $noname  C12 0.1uF/16V {Lib=C}
  (    1 /+V1.8 )
  (    2 GND )
 )
 ( /4A41A886 $noname  C11 10uF/10V {Lib=C}
  (    1 /+V1.8 )
  (    2 GND )
 )
 ( /4A41A880 $noname  C10 10pF/16V {Lib=C}
  (    1 /+V1.8 )
  (    2 N-000016 )
 )
 ( /4A41A6DA $noname  L2 4.7uH/1A {Lib=INDUCTORP}
  (    1 N-000020 )
  (    2 /+V1.8 )
 )
 ( /4A41A383 $noname  R46 10K/5% {Lib=R}
  (    1 N-000017 )
  (    2 /PWEN )
 )
 ( /4A41A30B $noname  C69 0.1uF/16V {Lib=C}
  (    1 N-000017 )
  (    2 GND )
 )
 ( /4A41A1FB $noname  C9 10uF/10V {Lib=C}
  (    1 N-000018 )
  (    2 GND )
 )
 ( /4A419E6D $noname  U3 EUP3406 {Lib=EUP3406}
  (    1 N-000017 )
  (    2 GND )
  (    3 N-000020 )
  (    4 N-000018 )
  (    5 N-000016 )
 )
 ( /4A418570 $noname  C20 47uF/6.3V {Lib=CPOLARIZED}
  (    1 /+VRTC )
  (    2 GND )
 )
 ( /4A417FD3 $noname  C19 1uF/16V {Lib=C}
  (    1 N-000018 )
  (    2 GND )
 )
 ( /4A40EE54 $noname  D1 MSCD104 {Lib=DIODESCH}
  (    1 N-000019 )
  (    2 /+VRTC )
 )
 ( /4A40ED7D $noname  U4 BL8555-33PRA {Lib=BL8555-33PRA}
  (    1 N-000018 )
  (    2 GND )
  (    3 N-000018 )
  (    4 N-000019 )
  (    5 N-000019 )
 )
 ( /4A40E3C5 $noname  Q1 TM2301N {Lib=TM2301N}
  (    1 N-000002 )
  (    2 N-000018 )
  (    3 /+VBAT )
 )
 ( /4A40CCF7 $noname  D2 MSCD104 {Lib=DIODESCH}
  (    1 N-000002 )
  (    2 N-000018 )
 )
 ( /4A40A66D $noname  D4 MSCD104 {Lib=DIODESCH}
  (    1 /CHARGE_N )
  (    2 N-000007 )
 )
 ( /4A409EE2 $noname  D3 RED_LED {Lib=LED}
  (    1 N-000028 )
  (    2 N-000007 )
 )
 ( /4A409E5B $noname  R12 510/5% {Lib=R}
  (    1 N-000002 )
  (    2 N-000028 )
 )
 ( /4A409CEB $noname  C35 1uF/16V {Lib=C}
  (    1 GND )
  (    2 N-000002 )
 )
 ( /4A404BF9 $noname  R14 2.5K/5% {Lib=R}
  (    1 N-000006 )
  (    2 N-000005 )
 )
 ( /4A40422D $noname  R15 10K/5% {Lib=R}
  (    1 N-000006 )
  (    2 GND )
 )
 ( /4A403664 $noname  Q3 TM2302N {Lib=TM2302N}
  (    1 /PW_ON_N )
  (    2 GND )
  (    3 N-000005 )
 )
 ( /4A403157 $noname  CON1 BAT_CON {Lib=BAT_CON}
  (    1 GND )
  (    3 /+VBAT )
 )
 ( /4A4030C0 $noname  U5 SE9016 {Lib=SE9016}
  (    1 N-000007 )
  (    2 GND )
  (    3 /+VBAT )
  (    4 N-000002 )
  (    5 N-000006 )
 )
 ( /4A3F4087 $noname  C36 1uF/16V {Lib=C}
  (    1 /+VBAT )
  (    2 GND )
 )
 ( /4A481D3C/4ACE4835 $noname  U13 USBDF {Lib=USBDF}
  (    1 /LCD_USB/HOST_DP1 )
  (    2 GND )
  (    3 /LCD_USB/HOST_DM1 )
  (    4 N-000181 )
  (    5 N-000188 )
 )
 ( /4A481D3C/4A837C30 $noname  D6 MSCD104 {Lib=DIODESCH}
  (    1 N-000183 )
  (    2 /LCD_USB/VHOST )
 )
 ( /4A481D3C/4A7C2400 $noname  R48 1M/5% {Lib=R}
  (    1 N-000186 )
  (    2 /+VBAT )
 )
 ( /4A481D3C/4A7C2342 $noname  R49 1M/5% {Lib=R}
  (    1 GND )
  (    2 N-000186 )
 )
 ( /4A481D3C/4A7C1D22 $noname  R50 1M/5% {Lib=R}
  (    1 N-000187 )
  (    2 N-000018 )
 )
 ( /4A481D3C/4A7C12A2 $noname  C73 3.3uF/16V {Lib=C}
  (    1 GND )
  (    2 N-000018 )
 )
 ( /4A481D3C/4A7C10EC $noname  C72 10uF/10V {Lib=C}
  (    1 GND )
  (    2 /LCD_USB/VHOST )
 )
 ( /4A481D3C/4A7C101A $noname  L4 4.7uH/1A {Lib=INDUCTORP}
  (    1 N-000018 )
  (    2 N-000183 )
 )
 ( /4A481D3C/4A7C0E4A $noname  U12 LT3925EDCB {Lib=LT3925EDCB}
  (    1 /LCD_USB/VHOST )
  (    2 N-000183 )
  (    3 N-000148 )
  (    4 GND )
  (    5 N-000187 )
  (    6 GND )
  (    7 GND )
  (    8 N-000018 )
  (    9 GND )
 )
 ( /4A481D3C/4A7BE0B1 $noname  R45 10K/5% {Lib=R}
  (    1 N-000086 )
  (    2 /LCD_USB/VHOST )
 )
 ( /4A481D3C/4A7BDFFD $noname  Q11 TM2301N {Lib=TM2301N}
  (    1 N-000086 )
  (    2 /LCD_USB/VHOST )
  (    3 N-000217 )
 )
 ( /4A481D3C/4A7BDF6A $noname  D5 MSCD104 {Lib=DIODESCH}
  (    1 N-000217 )
  (    2 N-000189 )
 )
 ( /4A481D3C/4A7BDD77 $noname  R43 100K/5% {Lib=R}
  (    1 N-000191 )
  (    2 GND )
 )
 ( /4A481D3C/4A7BDCBB $noname  C71 0.01uF/16V {Lib=C}
  (    1 GND )
  (    2 N-000191 )
 )
 ( /4A481D3C/4A7BDB67 $noname  BD10 PZ1608D221 {Lib=INDUCTOR}
  (    1 N-000190 )
  (    2 GND )
 )
 ( /4A481D3C/4A7BD8B4 $noname  J4 USB_MICRO_AB {Lib=USB_MICRO_AB}
  (    1 N-000189 )
  (    2 N-000181 )
  (    3 N-000188 )
  (    4 N-000086 )
  (    5 N-000190 )
  (    6 N-000191 )
  (    7 N-000191 )
  (    8 N-000191 )
  (    9 N-000191 )
 )
 ( /4A481D3C/4A4830BE $noname  C70 0.1uF/16V {Lib=C}
  (    1 N-000215 )
  (    2 /+V3.3 )
 )
 ( /4A481D3C/4A4830AE $noname  R47 47K/5% {Lib=R}
  (    1 GND )
  (    2 N-000215 )
 )
 ( /4A481D3C/4A48307F $noname  U11 SCIC {Lib=SCIC}
  (    1 GND )
  (    2 N-000215 )
  (    3 ? )
  (    4 GND )
  (    5 /LCD_USB/GPC9 )
  (    6 /LCD_USB/GPC8 )
  (    7 ? )
  (    8 /+V3.3 )
 )
 ( /4A481D3C/4A482F5F $noname  BD4 33/5% {Lib=INDUCTOR}
  (    1 /LCD_USB/DCLK )
  (    2 /LCD_USB/LCDDCLK )
 )
 ( /4A481D3C/4A482E6F $noname  BN2 33/5% {Lib=R_PACK4}
  (    1 /LCD_USB/LCD3 )
  (    2 /LCD_USB/LCD2 )
  (    3 /LCD_USB/LCD1 )
  (    4 /LCD_USB/LCD0 )
  (    5 /LCD_USB/LCDD0 )
  (    6 /LCD_USB/LCDD1 )
  (    7 /LCD_USB/LCDD2 )
  (    8 /LCD_USB/LCDD3 )
 )
 ( /4A481D3C/4A482E22 $noname  BN1 33/5% {Lib=R_PACK4}
  (    1 /LCD_USB/LCD7 )
  (    2 /LCD_USB/LCD6 )
  (    3 /LCD_USB/LCD5 )
  (    4 /LCD_USB/LCD4 )
  (    5 /LCD_USB/LCDD4 )
  (    6 /LCD_USB/LCDD5 )
  (    7 /LCD_USB/LCDD6 )
  (    8 /LCD_USB/LCDD7 )
 )
 ( /4A481D3C/4A482D6E $noname  C50 10uF/10V {Lib=C}
  (    1 /+V3.3 )
  (    2 GND )
 )
 ( /4A481D3C/4A482CC3 $noname  CON2 FPCCON24 {Lib=FPCCON24}
  (    1 GND )
  (    2 GND )
  (    3 GND )
  (    4 /+V3.3 )
  (    5 /+V3.3 )
  (    6 /+V3.3 )
  (    7 /+V3.3 )
  (    8 GND )
  (    9 /LCD_USB/LCD7 )
  (   10 /LCD_USB/LCD6 )
  (   11 /LCD_USB/LCD5 )
  (   12 /LCD_USB/LCD4 )
  (   13 /LCD_USB/LCD3 )
  (   14 /LCD_USB/LCD2 )
  (   15 /LCD_USB/LCD1 )
  (   16 /LCD_USB/LCD0 )
  (   17 /LCD_USB/LCDDCLK )
  (   18 /LCD_USB/VSYNC )
  (   19 /LCD_USB/HSYNC )
  (   20 /LCD_USB/LCDCS )
  (   21 N-000127 )
  (   22 N-000128 )
  (   23 GND )
  (   24 GND )
  (   25 GND )
  (   26 GND )
 )
 ( /4A481D3C/4A482A1C $noname  Q5 2N3904 {Lib=NPN}
  (    1 N-000182 )
  (    2 GND )
  (    3 N-000129 )
 )
 ( /4A481D3C/4A482978 $noname  R35 1K/5% {Lib=R}
  (    1 N-000182 )
  (    2 GND )
 )
 ( /4A481D3C/4A482970 $noname  R34 10K/5% {Lib=R}
  (    1 /+V3.3 )
  (    2 N-000129 )
 )
 ( /4A481D3C/4A482941 $noname  R33 1K/5% {Lib=R}
  (    1 N-000002 )
  (    2 N-000182 )
 )
 ( /4A481D3C/4A482875 $noname  C57 0.1uF/16V {Lib=C}
  (    1 GND )
  (    2 N-000002 )
 )
 ( /4A481D3C/4A48284F $noname  BD6 PZ1608D221 {Lib=INDUCTOR}
  (    1 N-000203 )
  (    2 N-000002 )
 )
 ( /4A481D3C/4A48278C $noname  L3 SDCW2012-2-900 {Lib=SDCW2012}
  (    1 N-000211 )
  (    2 /LCD_USB/DP )
  (    3 /LCD_USB/DN )
  (    4 N-000206 )
 )
 ( /4A481D3C/4A482731 $noname  BD7 PZ1608D221 {Lib=INDUCTOR}
  (    1 N-000204 )
  (    2 GND )
 )
 ( /4A481D3C/4A4826C7 $noname  C58 0.1uF/16V {Lib=C}
  (    1 GND )
  (    2 N-000207 )
 )
 ( /4A481D3C/4A4826AA $noname  J2 USB_MINIB {Lib=USB_MINIB}
  (    1 N-000203 )
  (    2 N-000206 )
  (    3 N-000211 )
  (    4 N-000204 )
  (    5 N-000204 )
  (    6 N-000207 )
  (    7 N-000207 )
  (    8 N-000207 )
  (    9 N-000207 )
 )
 ( /4A481D3C/4A4825EA $noname  C54 0.1uF/16V {Lib=C}
  (    1 N-000208 )
  (    2 GND )
 )
 ( /4A481D3C/4A4825B1 $noname  C55 0.1uF/16V {Lib=C}
  (    1 /+V3.3 )
  (    2 GND )
 )
 ( /4A481D3C/4A482569 $noname  R32 2.5K/5% {Lib=R}
  (    1 GND )
  (    2 N-000210 )
 )
 ( /4A481D3C/4A4824B2 $noname  R31 0 {Lib=R}
  (    1 /+VBAT )
  (    2 /LCD_USB/BATIN )
 )
 ( /4A481D3C/4A482361 $noname  TP36 TESTPOINT {Lib=TESTPOINT}
  (    1 /LCD_USB/GPC9 )
 )
 ( /4A481D3C/4A482346 $noname  TP35 TESTPOINT {Lib=TESTPOINT}
  (    1 /LCD_USB/GPC8 )
 )
 ( /4A481D3C/4A48222D $noname  C51 0.1uF/16V {Lib=C}
  (    1 /+VDDHP )
  (    2 GND )
 )
 ( /4A481D3C/4A482162 $noname  C53 0.1uF/16V {Lib=C}
  (    1 /LCD_USB/VREF )
  (    2 GND )
 )
 ( /4A481D3C/4A482120 $noname  C52 10uF/10V {Lib=C}
  (    1 /LCD_USB/VREF )
  (    2 GND )
 )
 ( /4A481D3C/4A4820CF $noname  TP38 TESTPOINT {Lib=TESTPOINT}
  (    1 /LCD_USB/GPD15 )
 )
 ( /4A4779DA/4A4818D2 $noname  C49 1uF/16V {Lib=C}
  (    1 /+V3.3 )
  (    2 GND )
 )
 ( /4A4779DA/4A4818CC $noname  C48 0.1uF/16V {Lib=C}
  (    1 /+V3.3 )
  (    2 GND )
 )
 ( /4A4779DA/4A4818BC $noname  R22 10K/5% {Lib=R}
  (    1 /MEMORY/FRB_N )
  (    2 /+V3.3 )
 )
 ( /4A4779DA/4A4818AF $noname  C47 0.1uF/16V {Lib=C}
  (    1 /+V3.3 )
  (    2 GND )
 )
 ( /4A4779DA/4A4818A9 $noname  R30 10K/5% {Lib=R}
  (    1 /MEMORY/WP_N )
  (    2 /+V3.3 )
 )
 ( /4A4779DA/4A481896 $noname  U9 K9GAG08U0M-PCB0 {Lib=HY27UG088G5M}
  (    1 ? )
  (    2 ? )
  (    3 ? )
  (    4 ? )
  (    5 ? )
  (    6 /MEMORY/FRB_N )
  (    7 /MEMORY/FRB_N )
  (    8 /MEMORY/FRE_N )
  (    9 /MEMORY/CS1_N )
  (   10 /MEMORY/CS2_N )
  (   11 ? )
  (   12 /+V3.3 )
  (   13 GND )
  (   14 ? )
  (   15 ? )
  (   16 /MEMORY/FCLE/GPB15 )
  (   17 /MEMORY/FALE/GPB16 )
  (   18 /MEMORY/FWE_N )
  (   19 /MEMORY/WP_N )
  (   20 ? )
  (   21 ? )
  (   22 ? )
  (   23 ? )
  (   24 ? )
  (   25 ? )
  (   26 ? )
  (   27 ? )
  (   28 ? )
  (   29 /MEMORY/D0 )
  (   30 /MEMORY/D1 )
  (   31 /MEMORY/D2 )
  (   32 /MEMORY/D3 )
  (   33 ? )
  (   34 ? )
  (   35 ? )
  (   36 GND )
  (   37 /+V3.3 )
  (   38 GND )
  (   39 ? )
  (   40 ? )
  (   41 /MEMORY/D4 )
  (   42 /MEMORY/D5 )
  (   43 /MEMORY/D6 )
  (   44 /MEMORY/D7 )
  (   45 ? )
  (   46 ? )
  (   47 ? )
  (   48 ? )
 )
 ( /4A4779DA/4A4801A3 $noname  R26 10K/5% {Lib=R}
  (    1 N-000085 )
  (    2 /+V3.3 )
 )
 ( /4A4779DA/4A480197 $noname  R29 10K/5% {Lib=R}
  (    1 N-000133 )
  (    2 N-000092 )
 )
 ( /4A4779DA/4A480194 $noname  R28 10K/5% {Lib=R}
  (    1 N-000133 )
  (    2 N-000135 )
 )
 ( /4A4779DA/4A480193 $noname  R27 10K/5% {Lib=R}
  (    1 N-000133 )
  (    2 N-000091 )
 )
 ( /4A4779DA/4A48017F $noname  R24 10K/5% {Lib=R}
  (    1 N-000133 )
  (    2 N-000136 )
 )
 ( /4A4779DA/4A480143 $noname  R23 10K/5% {Lib=R}
  (    1 N-000133 )
  (    2 N-000090 )
 )
 ( /4A4779DA/4A48012D $noname  J1 MS_1D77 {Lib=MS_1D77}
  (    1 N-000092 )
  (    2 N-000135 )
  (    3 N-000091 )
  (    4 N-000133 )
  (    5 N-000134 )
  (    6 GND )
  (    7 N-000136 )
  (    8 N-000090 )
  (    9 N-000085 )
  (   10 GND )
  (   11 GND )
  (   12 GND )
  (   13 GND )
 )
 ( /4A4779DA/4A47FF82 $noname  Q4 TM2301N {Lib=TM2301N}
  (    1 N-000132 )
  (    2 /+V3.3 )
  (    3 N-000133 )
 )
 ( /4A4779DA/4A47FF6E $noname  C46 0.1uF/16V {Lib=C}
  (    1 N-000133 )
  (    2 GND )
 )
 ( /4A4779DA/4A47FF6A $noname  C45 10uF/10V {Lib=C}
  (    1 N-000133 )
  (    2 GND )
 )
 ( /4A4779DA/4A47FE53 $noname  C39 0.1uF/16V {Lib=C}
  (    1 /+V3.3 )
  (    2 GND )
 )
 ( /4A4779DA/4A47FE61 $noname  C44 0.1uF/16V {Lib=C}
  (    1 /+V3.3 )
  (    2 GND )
 )
 ( /4A4779DA/4A47FE60 $noname  C43 0.1uF/16V {Lib=C}
  (    1 /+V3.3 )
  (    2 GND )
 )
 ( /4A4779DA/4A47FE5F $noname  C42 0.1uF/16V {Lib=C}
  (    1 /+V3.3 )
  (    2 GND )
 )
 ( /4A4779DA/4A47FE5E $noname  C41 0.1uF/16V {Lib=C}
  (    1 /+V3.3 )
  (    2 GND )
 )
 ( /4A4779DA/4A47FE54 $noname  C40 0.1uF/16V {Lib=C}
  (    1 /+V3.3 )
  (    2 GND )
 )
 ( /4A4779DA/4A47FE31 $noname  C38 0.1uF/16V {Lib=C}
  (    1 /+V3.3 )
  (    2 GND )
 )
 ( /4A4779DA/4A47FDDE $noname  C37 10uF/10V {Lib=C}
  (    1 /+V3.3 )
  (    2 GND )
 )
 ( /4A4779DA/4A47F884 $noname  U8 P3V56S40ETP-G6 {Lib=P3V56S40ETP-G6}
  (    1 /+V3.3 )
  (    2 /MEMORY/D0 )
  (    3 /+V3.3 )
  (    4 /MEMORY/D1 )
  (    5 /MEMORY/D2 )
  (    6 GND )
  (    7 /MEMORY/D3 )
  (    8 /MEMORY/D4 )
  (    9 /+V3.3 )
  (   10 /MEMORY/D5 )
  (   11 /MEMORY/D6 )
  (   12 GND )
  (   13 /MEMORY/D7 )
  (   14 /+V3.3 )
  (   15 /MEMORY/WE0_N )
  (   16 /MEMORY/MRDWR_N )
  (   17 /MEMORY/CAS_N )
  (   18 /MEMORY/RAS_N )
  (   19 /MEMORY/DCS0_N )
  (   20 /MEMORY/A13 )
  (   21 /MEMORY/A14 )
  (   22 /MEMORY/A10 )
  (   23 /MEMORY/A0 )
  (   24 /MEMORY/A1 )
  (   25 /MEMORY/A2 )
  (   26 /MEMORY/A3 )
  (   27 /+V3.3 )
  (   28 GND )
  (   29 /MEMORY/A4 )
  (   30 /MEMORY/A5 )
  (   31 /MEMORY/A6 )
  (   32 /MEMORY/A7 )
  (   33 /MEMORY/A8 )
  (   34 /MEMORY/A9 )
  (   35 /MEMORY/A11 )
  (   36 /MEMORY/A12 )
  (   37 /MEMORY/CKE )
  (   38 /MEMORY/MCKO )
  (   39 /MEMORY/WE1_N )
  (   40 ? )
  (   41 GND )
  (   42 /MEMORY/D8 )
  (   43 /+V3.3 )
  (   44 /MEMORY/D9 )
  (   45 /MEMORY/D10 )
  (   46 GND )
  (   47 /MEMORY/D11 )
  (   48 /MEMORY/D12 )
  (   49 /+V3.3 )
  (   50 /MEMORY/D13 )
  (   51 /MEMORY/D14 )
  (   52 GND )
  (   53 /MEMORY/D15 )
  (   54 GND )
 )
 ( /4A4779DA/4A47F6D0 $noname  R21 33/5% {Lib=R}
  (    1 /MEMORY/MRDWR_N )
  (    2 /MEMORY/RDWR_N )
 )
 ( /4A4779DA/4A47F6A8 $noname  R20 33/5% {Lib=R}
  (    1 /MEMORY/MCKO )
  (    2 /MEMORY/CKO )
 )
 ( /4A4779DA/4A47F401 $noname  BUZ-1 SOLDERPASTE {Lib=SOLDERPASTE}
  (    1 GND )
 )
 ( /4A4779DA/4A47F3CC $noname  BUZ+1 SOLDERPASTE {Lib=SOLDERPASTE}
  (    1 /MEMORY/BUZPWM )
 )
 ( /4A4779DA/4A4783D4 $noname  TP23 TESTPOINT {Lib=TESTPOINT}
  (    1 /MEMORY/GPB18 )
 )
 ( /4A4779DA/4A4782DD $noname  TP25 TESTPOINT {Lib=TESTPOINT}
  (    1 /MEMORY/GPB30 )
 )
 ( /4A46EDD2/4A46EA0A $noname  C62 100uF/4V {Lib=CPOLARIZED}
  (    1 N-000077 )
  (    2 N-000064 )
 )
 ( /4A46EDD2/4A46E9CC $noname  C59 100uF/4V {Lib=CPOLARIZED}
  (    1 N-000063 )
  (    2 N-000076 )
 )
 ( /4A46EDD2/4A46E906 $noname  R40 100/5% {Lib=R}
  (    1 GND )
  (    2 N-000076 )
 )
 ( /4A46EDD2/4A46E8DF $noname  R41 100/5% {Lib=R}
  (    1 GND )
  (    2 N-000064 )
 )
 ( /4A46EDD2/4A46E868 $noname  Q10 TM2302N {Lib=TM2302N}
  (    1 /MEMORY/POP )
  (    2 N-000074 )
  (    3 N-000064 )
 )
 ( /4A46EDD2/4A46E82E $noname  Q9 TM2302N {Lib=TM2302N}
  (    1 /MEMORY/POP )
  (    2 N-000065 )
  (    3 N-000076 )
 )
 ( /4A46EDD2/4A46E6D7 $noname  R38 33/5% {Lib=R}
  (    1 /AUDIO/HPOR )
  (    2 N-000074 )
 )
 ( /4A46EDD2/4A46E6C2 $noname  R37 33/5% {Lib=R}
  (    1 /AUDIO/HPOL )
  (    2 N-000065 )
 )
 ( /4A46EDD2/4A46E548 $noname  BD8 PZ1608D221 {Lib=INDUCTOR}
  (    1 GND )
  (    2 /AUDIO/HPGND )
 )
 ( /4A46EDD2/4A46E543 $noname  R36 100K/5% {Lib=R}
  (    1 /+V3.3 )
  (    2 /AUDIO/AMPIN )
 )
 ( /4A46EDD2/4A46E402 $noname  J3 PHONEJACK {Lib=PHONEJACK}
  (    1 /AUDIO/HPGND )
  (    2 /AUDIO/HPOL )
  (    3 /AUDIO/HPOR )
  (    4 /AUDIO/AMPIN )
  (    5 /AUDIO/AMPIN )
 )
 ( /4A46EDD2/4A46E205 $noname  C61 0.1uF/16V {Lib=C}
  (    1 GND )
  (    2 /AUDIO/MICBIAS )
 )
 ( /4A46EDD2/4A46E174 $noname  C60 47uF/6.3V {Lib=CPOLARIZED}
  (    1 /AUDIO/MICBIAS )
  (    2 GND )
 )
 ( /4A46EDD2/4A46E171 $noname  C63 1uF/16V {Lib=C}
  (    1 N-000067 )
  (    2 /AUDIO/MICIN )
 )
 ( /4A46EDD2/4A46E16E $noname  R39 22K/5% {Lib=R}
  (    1 /AUDIO/MICBIAS )
  (    2 N-000067 )
 )
 ( /4A46EDD2/4A46E14A $noname  MIC-1 SOLDERPASTE {Lib=SOLDERPASTE}
  (    1 GND )
 )
 ( /4A46EDD2/4A46E136 $noname  MIC+1 SOLDERPASTE {Lib=SOLDERPASTE}
  (    1 N-000067 )
 )
 ( /4A46EDD2/4A46DF25 $noname  Q6 TM2301N {Lib=TM2301N}
  (    1 /AUDIO/AMPIN )
  (    2 N-000073 )
  (    3 N-000068 )
 )
 ( /4A46EDD2/4A46DF0D $noname  R42 100K/5% {Lib=R}
  (    1 GND )
  (    2 N-000068 )
 )
 ( /4A46EDD2/4A46DD80 $noname  BD9 PZ1608D221 {Lib=INDUCTOR}
  (    1 N-000018 )
  (    2 N-000069 )
 )
 ( /4A46EDD2/4A46DD12 $noname  C66 0.1uF/16V {Lib=C}
  (    1 GND )
  (    2 N-000069 )
 )
 ( /4A46EDD2/4A46DCB5 $noname  C67 0.1uF/16V {Lib=C}
  (    1 N-000072 )
  (    2 /AUDIO/AMPIN )
 )
 ( /4A46EDD2/4A46DB8E $noname  R44 10K/5% {Lib=R}
  (    1 N-000070 )
  (    2 N-000072 )
 )
 ( /4A46EDD2/4A46DB7A $noname  C65 47uF/6.3V {Lib=CPOLARIZED}
  (    1 N-000069 )
  (    2 GND )
 )
 ( /4A46EDD2/4A46DB70 $noname  C68 0.1uF/16V {Lib=C}
  (    1 N-000071 )
  (    2 GND )
 )
 ( /4A46EDD2/4A46DB15 $noname  U10 GPY0030A {Lib=SPY0030A}
  (    1 /AUDIO/SP- )
  (    2 /AUDIO/SP+ )
  (    3 GND )
  (    4 N-000071 )
  (    5 N-000070 )
  (    6 N-000071 )
  (    7 N-000068 )
  (    8 N-000069 )
 )
 ( /4A46EDD2/4A46DA2F $noname  SP+1 SOLDERPASTE {Lib=SOLDERPASTE}
  (    1 /AUDIO/SP+ )
 )
 ( /4A46EDD2/4A46D9F6 $noname  SP-1 SOLDERPASTE {Lib=SOLDERPASTE}
  (    1 /AUDIO/SP- )
 )
 ( /4A46ED00/4A4635D4 $noname  S59 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT2 )
  (    2 /RXD )
 )
 ( /4A46ED00/4A4635D3 $noname  S58 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT1 )
  (    2 /RXD )
 )
 ( /4A46ED00/4A4635D1 $noname  S60 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT3 )
  (    2 /RXD )
 )
 ( /4A46ED00/4A4635D0 $noname  S55 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT6 )
  (    2 /KEY_MATRIX/KEYIN7 )
 )
 ( /4A46ED00/4A4635CF $noname  S54 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT5 )
  (    2 /KEY_MATRIX/KEYIN7 )
 )
 ( /4A46ED00/4A4635CE $noname  S57 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT8 )
  (    2 /KEY_MATRIX/KEYIN7 )
 )
 ( /4A46ED00/4A4635CD $noname  S56 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT7 )
  (    2 /KEY_MATRIX/KEYIN7 )
 )
 ( /4A46ED00/4A4635CC $noname  S51 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT2 )
  (    2 /KEY_MATRIX/KEYIN7 )
 )
 ( /4A46ED00/4A4635CB $noname  S50 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT1 )
  (    2 /KEY_MATRIX/KEYIN7 )
 )
 ( /4A46ED00/4A4635CA $noname  S53 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT4 )
  (    2 /KEY_MATRIX/KEYIN7 )
 )
 ( /4A46ED00/4A4635C9 $noname  S52 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT3 )
  (    2 /KEY_MATRIX/KEYIN7 )
 )
 ( /4A46ED00/4A4635C8 $noname  S47 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT6 )
  (    2 /KEY_MATRIX/KEYIN6 )
 )
 ( /4A46ED00/4A4635C7 $noname  S46 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT5 )
  (    2 /KEY_MATRIX/KEYIN6 )
 )
 ( /4A46ED00/4A4635C6 $noname  S49 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT8 )
  (    2 /KEY_MATRIX/KEYIN6 )
 )
 ( /4A46ED00/4A4635C5 $noname  S48 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT7 )
  (    2 /KEY_MATRIX/KEYIN6 )
 )
 ( /4A46ED00/4A4635C4 $noname  S43 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT2 )
  (    2 /KEY_MATRIX/KEYIN6 )
 )
 ( /4A46ED00/4A4635C3 $noname  S42 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT1 )
  (    2 /KEY_MATRIX/KEYIN6 )
 )
 ( /4A46ED00/4A4635C2 $noname  S45 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT4 )
  (    2 /KEY_MATRIX/KEYIN6 )
 )
 ( /4A46ED00/4A4635C1 $noname  S44 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT3 )
  (    2 /KEY_MATRIX/KEYIN6 )
 )
 ( /4A46ED00/4A4635C0 $noname  S39 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT6 )
  (    2 /KEY_MATRIX/KEYIN5 )
 )
 ( /4A46ED00/4A4635BF $noname  S38 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT5 )
  (    2 /KEY_MATRIX/KEYIN5 )
 )
 ( /4A46ED00/4A4635BE $noname  S41 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT8 )
  (    2 /KEY_MATRIX/KEYIN5 )
 )
 ( /4A46ED00/4A4635BD $noname  S40 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT7 )
  (    2 /KEY_MATRIX/KEYIN5 )
 )
 ( /4A46ED00/4A4635BC $noname  S35 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT2 )
  (    2 /KEY_MATRIX/KEYIN5 )
 )
 ( /4A46ED00/4A4635BB $noname  S34 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT1 )
  (    2 /KEY_MATRIX/KEYIN5 )
 )
 ( /4A46ED00/4A4635BA $noname  S37 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT4 )
  (    2 /KEY_MATRIX/KEYIN5 )
 )
 ( /4A46ED00/4A4635B9 $noname  S36 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT3 )
  (    2 /KEY_MATRIX/KEYIN5 )
 )
 ( /4A46ED00/4A46358C $noname  S31 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT6 )
  (    2 /KEY_MATRIX/KEYIN4 )
 )
 ( /4A46ED00/4A46358B $noname  S30 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT5 )
  (    2 /KEY_MATRIX/KEYIN4 )
 )
 ( /4A46ED00/4A46358A $noname  S33 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT8 )
  (    2 /KEY_MATRIX/KEYIN4 )
 )
 ( /4A46ED00/4A463589 $noname  S32 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT7 )
  (    2 /KEY_MATRIX/KEYIN4 )
 )
 ( /4A46ED00/4A463588 $noname  S27 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT2 )
  (    2 /KEY_MATRIX/KEYIN4 )
 )
 ( /4A46ED00/4A463587 $noname  S26 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT1 )
  (    2 /KEY_MATRIX/KEYIN4 )
 )
 ( /4A46ED00/4A463586 $noname  S29 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT4 )
  (    2 /KEY_MATRIX/KEYIN4 )
 )
 ( /4A46ED00/4A463585 $noname  S28 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT3 )
  (    2 /KEY_MATRIX/KEYIN4 )
 )
 ( /4A46ED00/4A463584 $noname  S23 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT6 )
  (    2 /KEY_MATRIX/KEYIN3 )
 )
 ( /4A46ED00/4A463583 $noname  S22 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT5 )
  (    2 /KEY_MATRIX/KEYIN3 )
 )
 ( /4A46ED00/4A463582 $noname  S25 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT8 )
  (    2 /KEY_MATRIX/KEYIN3 )
 )
 ( /4A46ED00/4A463581 $noname  S24 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT7 )
  (    2 /KEY_MATRIX/KEYIN3 )
 )
 ( /4A46ED00/4A463580 $noname  S19 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT2 )
  (    2 /KEY_MATRIX/KEYIN3 )
 )
 ( /4A46ED00/4A46357F $noname  S18 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT1 )
  (    2 /KEY_MATRIX/KEYIN3 )
 )
 ( /4A46ED00/4A46357E $noname  S21 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT4 )
  (    2 /KEY_MATRIX/KEYIN3 )
 )
 ( /4A46ED00/4A46357D $noname  S20 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT3 )
  (    2 /KEY_MATRIX/KEYIN3 )
 )
 ( /4A46ED00/4A463552 $noname  S15 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT6 )
  (    2 /KEY_MATRIX/KEYIN2 )
 )
 ( /4A46ED00/4A463551 $noname  S14 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT5 )
  (    2 /KEY_MATRIX/KEYIN2 )
 )
 ( /4A46ED00/4A463550 $noname  S17 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT8 )
  (    2 /KEY_MATRIX/KEYIN2 )
 )
 ( /4A46ED00/4A46354F $noname  S16 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT7 )
  (    2 /KEY_MATRIX/KEYIN2 )
 )
 ( /4A46ED00/4A46354E $noname  S11 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT2 )
  (    2 /KEY_MATRIX/KEYIN2 )
 )
 ( /4A46ED00/4A46354D $noname  S10 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT1 )
  (    2 /KEY_MATRIX/KEYIN2 )
 )
 ( /4A46ED00/4A46354C $noname  S13 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT4 )
  (    2 /KEY_MATRIX/KEYIN2 )
 )
 ( /4A46ED00/4A46354B $noname  S12 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT3 )
  (    2 /KEY_MATRIX/KEYIN2 )
 )
 ( /4A46ED00/4A463529 $noname  S7 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT6 )
  (    2 /KEY_MATRIX/KEYIN1 )
 )
 ( /4A46ED00/4A463528 $noname  S6 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT5 )
  (    2 /KEY_MATRIX/KEYIN1 )
 )
 ( /4A46ED00/4A463526 $noname  S8 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT7 )
  (    2 /KEY_MATRIX/KEYIN1 )
 )
 ( /4A46ED00/4A463512 $noname  S3 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT2 )
  (    2 /KEY_MATRIX/KEYIN1 )
 )
 ( /4A46ED00/4A463511 $noname  S2 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT1 )
  (    2 /KEY_MATRIX/KEYIN1 )
 )
 ( /4A46ED00/4A46349C $noname  S5 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT4 )
  (    2 /KEY_MATRIX/KEYIN1 )
 )
 ( /4A46ED00/4A46347E $noname  S4 SW_METALDOMN {Lib=SW_METALDOMN}
  (    1 /KEY_MATRIX/KEYOUT3 )
  (    2 /KEY_MATRIX/KEYIN1 )
 )
 ( /4A46ED00/4A4632A6 $noname  TP69 TESTPOINT {Lib=TESTPOINT}
  (    1 /KEY_MATRIX/KEYIN3 )
 )
 ( /4A46ED00/4A46329C $noname  TP65 TESTPOINT {Lib=TESTPOINT}
  (    1 /KEY_MATRIX/KEYOUT7 )
 )
)
*
{ Allowed footprints by component:
$component SW1
 SWITCH
 SW
$endlist
$component C33
 SM*
 C?
 C1-1
$endlist
$component C32
 SM*
 C?
 C1-1
$endlist
$component C31
 SM*
 C?
 C1-1
$endlist
$component C30
 SM*
 C?
 C1-1
$endlist
$component C29
 SM*
 C?
 C1-1
$endlist
$component C28
 SM*
 C?
 C1-1
$endlist
$component C27
 SM*
 C?
 C1-1
$endlist
$component C26
 SM*
 C?
 C1-1
$endlist
$component C25
 SM*
 C?
 C1-1
$endlist
$component C24
 SM*
 C?
 C1-1
$endlist
$component C23
 SM*
 C?
 C1-1
$endlist
$component C22
 SM*
 C?
 C1-1
$endlist
$component C18
 SM*
 C?
 C1-1
$endlist
$component C17
 SM*
 C?
 C1-1
$endlist
$component C15
 SM*
 C?
 C1-1
$endlist
$component R7
 R?
 SM0603
 SM0805
$endlist
$component R9
 R?
 SM0603
 SM0805
$endlist
$component R5
 R?
 SM0603
 SM0805
$endlist
$component R4
 R?
 SM0603
 SM0805
$endlist
$component C21
 SM*
 C?
 C1-1
$endlist
$component C13
 SM*
 C?
 C1-1
$endlist
$component C14
 SM*
 C?
 C1-1
$endlist
$component C16
 SM*
 C?
 C1-1
$endlist
$component C4
 SM*
 C?
 C1-1
$endlist
$component C1
 SM*
 C?
 C1-1
$endlist
$component C8
 SM*
 C?
 C1-1
$endlist
$component C5
 SM*
 C?
 C1-1
$endlist
$component R8
 R?
 SM0603
 SM0805
$endlist
$component R2
 R?
 SM0603
 SM0805
$endlist
$component R1
 R?
 SM0603
 SM0805
$endlist
$component R16
 R?
 SM0603
 SM0805
$endlist
$component R18
 R?
 SM0603
 SM0805
$endlist
$component R17
 R?
 SM0603
 SM0805
$endlist
$component R13
 R?
 SM0603
 SM0805
$endlist
$component R19
 R?
 SM0603
 SM0805
$endlist
$component R6
 R?
 SM0603
 SM0805
$endlist
$component R3
 R?
 SM0603
 SM0805
$endlist
$component C3
 SM*
 C?
 C1-1
$endlist
$component C2
 SM*
 C?
 C1-1
$endlist
$component C7
 SM*
 C?
 C1-1
$endlist
$component C6
 SM*
 C?
 C1-1
$endlist
$component R11
 R?
 SM0603
 SM0805
$endlist
$component R10
 R?
 SM0603
 SM0805
$endlist
$component C12
 SM*
 C?
 C1-1
$endlist
$component C11
 SM*
 C?
 C1-1
$endlist
$component C10
 SM*
 C?
 C1-1
$endlist
$component R46
 R?
 SM0603
 SM0805
$endlist
$component C69
 SM*
 C?
 C1-1
$endlist
$component C9
 SM*
 C?
 C1-1
$endlist
$component C19
 SM*
 C?
 C1-1
$endlist
$component D1
 D?
 S*
$endlist
$component D2
 D?
 S*
$endlist
$component D4
 D?
 S*
$endlist
$component R12
 R?
 SM0603
 SM0805
$endlist
$component C35
 SM*
 C?
 C1-1
$endlist
$component R14
 R?
 SM0603
 SM0805
$endlist
$component R15
 R?
 SM0603
 SM0805
$endlist
$component C36
 SM*
 C?
 C1-1
$endlist
$component D6
 D?
 S*
$endlist
$component R48
 R?
 SM0603
 SM0805
$endlist
$component R49
 R?
 SM0603
 SM0805
$endlist
$component R50
 R?
 SM0603
 SM0805
$endlist
$component C73
 SM*
 C?
 C1-1
$endlist
$component C72
 SM*
 C?
 C1-1
$endlist
$component R45
 R?
 SM0603
 SM0805
$endlist
$component D5
 D?
 S*
$endlist
$component R43
 R?
 SM0603
 SM0805
$endlist
$component C71
 SM*
 C?
 C1-1
$endlist
$component C70
 SM*
 C?
 C1-1
$endlist
$component R47
 R?
 SM0603
 SM0805
$endlist
$component C50
 SM*
 C?
 C1-1
$endlist
$component R35
 R?
 SM0603
 SM0805
$endlist
$component R34
 R?
 SM0603
 SM0805
$endlist
$component R33
 R?
 SM0603
 SM0805
$endlist
$component C57
 SM*
 C?
 C1-1
$endlist
$component C58
 SM*
 C?
 C1-1
$endlist
$component C54
 SM*
 C?
 C1-1
$endlist
$component C55
 SM*
 C?
 C1-1
$endlist
$component R32
 R?
 SM0603
 SM0805
$endlist
$component R31
 R?
 SM0603
 SM0805
$endlist
$component C51
 SM*
 C?
 C1-1
$endlist
$component C53
 SM*
 C?
 C1-1
$endlist
$component C52
 SM*
 C?
 C1-1
$endlist
$component C49
 SM*
 C?
 C1-1
$endlist
$component C48
 SM*
 C?
 C1-1
$endlist
$component R22
 R?
 SM0603
 SM0805
$endlist
$component C47
 SM*
 C?
 C1-1
$endlist
$component R30
 R?
 SM0603
 SM0805
$endlist
$component R26
 R?
 SM0603
 SM0805
$endlist
$component R29
 R?
 SM0603
 SM0805
$endlist
$component R28
 R?
 SM0603
 SM0805
$endlist
$component R27
 R?
 SM0603
 SM0805
$endlist
$component R24
 R?
 SM0603
 SM0805
$endlist
$component R23
 R?
 SM0603
 SM0805
$endlist
$component C46
 SM*
 C?
 C1-1
$endlist
$component C45
 SM*
 C?
 C1-1
$endlist
$component C39
 SM*
 C?
 C1-1
$endlist
$component C44
 SM*
 C?
 C1-1
$endlist
$component C43
 SM*
 C?
 C1-1
$endlist
$component C42
 SM*
 C?
 C1-1
$endlist
$component C41
 SM*
 C?
 C1-1
$endlist
$component C40
 SM*
 C?
 C1-1
$endlist
$component C38
 SM*
 C?
 C1-1
$endlist
$component C37
 SM*
 C?
 C1-1
$endlist
$component R21
 R?
 SM0603
 SM0805
$endlist
$component R20
 R?
 SM0603
 SM0805
$endlist
$component R40
 R?
 SM0603
 SM0805
$endlist
$component R41
 R?
 SM0603
 SM0805
$endlist
$component R38
 R?
 SM0603
 SM0805
$endlist
$component R37
 R?
 SM0603
 SM0805
$endlist
$component R36
 R?
 SM0603
 SM0805
$endlist
$component C61
 SM*
 C?
 C1-1
$endlist
$component C63
 SM*
 C?
 C1-1
$endlist
$component R39
 R?
 SM0603
 SM0805
$endlist
$component R42
 R?
 SM0603
 SM0805
$endlist
$component C66
 SM*
 C?
 C1-1
$endlist
$component C67
 SM*
 C?
 C1-1
$endlist
$component R44
 R?
 SM0603
 SM0805
$endlist
$component C68
 SM*
 C?
 C1-1
$endlist
$endfootprintlist
}
{ Pin List by Nets
Net 2 ""
 TP7 1
 Q1 1
 D2 1
 R12 1
 C35 2
 U5 4
 R33 1
 C57 2
 BD6 2
Net 3 "GND"
 SW1 1
 CON3 GND
 CON3 1
 C33 2
 C32 2
 C31 2
 C30 2
 C29 2
 C28 2
 C27 2
 C26 2
 C25 2
 C24 2
 C23 2
 C22 2
 U1 142
 U1 138
 U1 94
 U1 187
 U1 181
 U1 171
 U1 77
 U1 45
 U1 29
 U1 22
 U1 9
 U1 184
 U1 67
 U1 48
 U1 34
 U1 8
 U1 119
 U1 101
 U1 102
 U1 104
 C18 2
 C17 2
 C15 2
 R9 2
 C21 2
 C13 2
 C14 2
 C16 2
 C4 2
 C1 2
 Y1 3
 C8 2
 C5 2
 Y2 3
 S1 1
 S9 1
 R18 2
 U6 1
 U7 2
 TP76 1
 R6 2
 C3 2
 C2 2
 C6 2
 U2 2
 R11 2
 C12 2
 C11 2
 C69 2
 C9 2
 U3 2
 C20 2
 C19 2
 U4 2
 C35 1
 R15 2
 Q3 2
 CON1 1
 U5 2
 C36 2
 R40 1
 R41 1
 BD8 1
 C61 1
 C60 2
 MIC-1 1
 R42 1
 C66 1
 C65 2
 C68 2
 U10 3
 C49 2
 C48 2
 C47 2
 U9 36
 U9 38
 U9 13
 J1 6
 J1 10
 J1 11
 J1 12
 J1 13
 C46 2
 C45 2
 C39 2
 C44 2
 C43 2
 C42 2
 C41 2
 C40 2
 C38 2
 C37 2
 U8 46
 U8 52
 U8 12
 U8 6
 U8 54
 U8 41
 U8 28
 BUZ-1 1
 U13 2
 R49 1
 C73 1
 C72 1
 U12 4
 U12 9
 U12 6
 U12 7
 R43 2
 C71 1
 BD10 2
 R47 1
 U11 4
 U11 1
 C50 2
 CON2 25
 CON2 26
 CON2 24
 CON2 23
 CON2 8
 CON2 3
 CON2 2
 CON2 1
 Q5 2
 R35 2
 C57 1
 BD7 2
 C58 1
 C54 2
 C55 2
 R32 1
 C51 2
 C53 2
 C52 2
 U1 118
 U1 117
 U1 108
 U1 131
 U1 130
 U1 133
 U1 132
/Net 4 "PW_ON_N"
 U1 125
 Q2 1
 R17 2
 Q3 1
Net 5 ""
 R14 2
 Q3 3
Net 6 ""
 R14 1
 R15 1
 U5 5
Net 7 ""
 D4 2
 D3 2
 U5 1
/Net 8 "TDI"
 U1 148
 TP4 1
/Net 9 "TCLK"
 U1 149
 TP2 1
/Net 10 "WAKEUP_N"
 U1 124
 R16 2
 S9 2
 TP77 1
/Net 11 "PWEN"
 Q2 3
 R18 1
 U2 1
 R46 2
/Net 12 "SHUTDOWN"
 R19 1
 U7 1
 TP78 1
 U1 152
Net 13 ""
 R6 1
 R3 2
 C7 2
 U2 5
/Net 14 "+V3.3"
 C33 1
 C32 1
 C31 1
 C30 1
 C29 1
 C28 1
 U1 185
 U1 91
 U1 66
 U1 49
 U1 33
 U1 7
 BD3 2
 BD2 2
 R7 1
 R5 1
 R4 1
 R19 2
 TP9 1
 R3 1
 C3 1
 C2 1
 C7 1
 L1 2
 R36 1
 C49 1
 C48 1
 R22 2
 C47 1
 R30 2
 U9 37
 U9 12
 R26 2
 Q4 2
 C39 1
 C44 1
 C43 1
 C42 1
 C41 1
 C40 1
 C38 1
 C37 1
 U8 43
 U8 49
 U8 9
 U8 3
 U8 1
 U8 27
 U8 14
 C70 2
 U11 8
 C50 1
 CON2 7
 CON2 6
 CON2 5
 CON2 4
 R34 1
 C55 1
 U1 112
 U1 111
 U1 105
Net 15 ""
 L1 1
 U2 3
Net 16 ""
 R11 1
 R10 2
 C10 2
 U3 5
Net 17 ""
 R46 1
 C69 1
 U3 1
Net 18 ""
 U7 3
 C6 1
 U2 4
 C9 1
 U3 4
 C19 1
 U4 3
 U4 1
 Q1 2
 D2 2
 BD9 1
 R50 2
 C73 2
 L4 1
 U12 8
Net 19 ""
 D1 1
 U4 4
 U4 5
Net 20 ""
 L2 1
 U3 3
/Net 21 "CHARGE_N"
 TP32 1
 D4 1
 U1 69
Net 22 ""
 C8 1
 Y2 1
 R8 2
 R2 2
/Net 23 "RESETP_N"
 U1 123
 S1 2
 R13 2
 U6 2
 TP6 1
/Net 24 "+V1.8"
 C27 1
 C26 1
 C25 1
 C24 1
 C23 1
 C22 1
 U1 103
 U1 100
 U1 172
 U1 76
 U1 44
 U1 30
 U1 21
 U1 10
 C13 1
 C14 1
 C16 1
 TP10 1
 R10 1
 C12 1
 C11 1
 C10 1
 L2 2
/Net 25 "TRST_N"
 U1 151
 TP1 1
/Net 26 "TDO"
 U1 147
 TP5 1
Net 27 ""
 U1 180
 R7 2
Net 28 ""
 D3 1
 R12 2
/Net 29 "TMS"
 U1 150
 TP3 1
/Net 30 "BOOT_SEL1_HIGH"
 SW1 2
 R9 1
 R5 2
/Net 31 "BOOT_SEL1"
 SW1 3
 U1 145
/Net 32 "+VBAT"
 TP8 1
 Q1 3
 CON1 3
 U5 3
 C36 1
 R48 2
 R31 1
/Net 33 "+VRTC"
 U1 122
 C21 1
 R16 1
 Q2 2
 R17 1
 R13 1
 U6 3
 C20 1
 D1 2
/Net 39 "RXD"
 CON3 3
 S59 2
 S58 2
 S60 2
 U1 72
/Net 40 "TXD"
 CON3 2
 U1 73
/Net 41 "VDDADC"
 U1 95
 BD2 1
 C15 1
/Net 42 "+VDDHP"
 U1 139
 U1 141
 C18 1
 BD3 1
 C17 1
 C51 1
 U1 127
 U1 126
 U1 137
 U1 136
/Net 43 "BOOT_SEL0"
 U1 146
 R4 2
/Net 44 "EXTAL"
 U1 90
 R8 1
/Net 45 "XTAL"
 U1 89
 C5 1
 Y2 2
 R2 1
/Net 46 "RCLKO"
 U1 121
 C4 1
 Y1 1
 R1 2
/Net 47 "RCLK"
 U1 120
 C1 1
 Y1 2
 R1 1
/KEY_MATRIX/Net 48 "KEYIN7"
 S55 2
 S54 2
 S57 2
 S56 2
 S51 2
 S50 2
 S53 2
 S52 2
 U1 74
/KEY_MATRIX/Net 49 "KEYIN6"
 S47 2
 S46 2
 S49 2
 S48 2
 S43 2
 S42 2
 S45 2
 S44 2
 U1 75
/KEY_MATRIX/Net 50 "KEYIN5"
 S39 2
 S38 2
 S41 2
 S40 2
 S35 2
 S34 2
 S37 2
 S36 2
 U1 86
/KEY_MATRIX/Net 51 "KEYIN4"
 S31 2
 S30 2
 S33 2
 S32 2
 S27 2
 S26 2
 S29 2
 S28 2
 U1 88
/KEY_MATRIX/Net 52 "KEYIN3"
 S23 2
 S22 2
 S25 2
 S24 2
 S19 2
 S18 2
 S21 2
 S20 2
 TP69 1
 U1 87
/KEY_MATRIX/Net 53 "KEYIN2"
 S15 2
 S14 2
 S17 2
 S16 2
 S11 2
 S10 2
 S13 2
 S12 2
 U1 85
/KEY_MATRIX/Net 54 "KEYIN1"
 S7 2
 S6 2
 S8 2
 S3 2
 S2 2
 S5 2
 S4 2
 U1 84
/KEY_MATRIX/Net 55 "KEYOUT8"
 S57 1
 S49 1
 S41 1
 S33 1
 S25 1
 S17 1
 U1 164
/KEY_MATRIX/Net 56 "KEYOUT7"
 S56 1
 S48 1
 S40 1
 S32 1
 S24 1
 S16 1
 S8 1
 TP65 1
 U1 165
/KEY_MATRIX/Net 57 "KEYOUT6"
 S55 1
 S47 1
 S39 1
 S31 1
 S23 1
 S15 1
 S7 1
 U1 166
/KEY_MATRIX/Net 58 "KEYOUT5"
 S54 1
 S46 1
 S38 1
 S30 1
 S22 1
 S14 1
 S6 1
 U1 167
/KEY_MATRIX/Net 59 "KEYOUT4"
 S53 1
 S45 1
 S37 1
 S29 1
 S21 1
 S13 1
 S5 1
 U1 168
/KEY_MATRIX/Net 60 "KEYOUT3"
 S60 1
 S52 1
 S44 1
 S36 1
 S28 1
 S20 1
 S12 1
 S4 1
 U1 169
/KEY_MATRIX/Net 61 "KEYOUT2"
 S59 1
 S51 1
 S43 1
 S35 1
 S27 1
 S19 1
 S11 1
 S3 1
 U1 170
/KEY_MATRIX/Net 62 "KEYOUT1"
 S58 1
 S50 1
 S42 1
 S34 1
 S26 1
 S18 1
 S10 1
 S2 1
 U1 173
Net 63 ""
 C59 1
 U1 135
 U1 134
Net 64 ""
 C62 2
 R41 2
 Q10 3
Net 65 ""
 Q9 2
 R37 2
/AUDIO/Net 66 "AMPIN"
 R36 2
 J3 4
 J3 5
 Q6 1
 C67 2
Net 67 ""
 C63 1
 R39 2
 MIC+1 1
Net 68 ""
 Q6 3
 R42 2
 U10 7
Net 69 ""
 BD9 2
 C66 2
 C65 1
 U10 8
Net 70 ""
 R44 1
 U10 5
Net 71 ""
 C68 1
 U10 4
 U10 6
Net 72 ""
 C67 1
 R44 2
Net 73 ""
 Q6 2
 U1 153
Net 74 ""
 Q10 2
 R38 2
/MEMORY/Net 75 "POP"
 Q10 1
 Q9 1
 U1 61
Net 76 ""
 C59 2
 R40 2
 Q9 3
Net 77 ""
 C62 1
 U1 129
 U1 128
/AUDIO/Net 78 "HPOR"
 R38 1
 J3 3
/AUDIO/Net 79 "HPOL"
 R37 1
 J3 2
/AUDIO/Net 80 "HPGND"
 BD8 2
 J3 1
/AUDIO/Net 81 "MICBIAS"
 C61 2
 C60 1
 R39 1
 U1 143
/AUDIO/Net 82 "MICIN"
 C63 2
 U1 144
/AUDIO/Net 83 "SP+"
 U10 2
 SP+1 1
/AUDIO/Net 84 "SP-"
 U10 1
 SP-1 1
Net 85 ""
 R26 1
 J1 9
 U1 155
Net 86 ""
 U1 62
 R45 1
 Q11 1
 J4 4
/MEMORY/Net 87 "CS2_N"
 U9 10
 U1 70
/MEMORY/Net 88 "CS1_N"
 U9 9
 U1 71
/MEMORY/Net 89 "FRE_N"
 U9 8
 U1 65
Net 90 ""
 R23 2
 J1 8
 U1 80
Net 91 ""
 R27 2
 J1 3
 U1 83
Net 92 ""
 R29 2
 J1 1
 U1 79
/MEMORY/Net 93 "D15"
 U8 53
 U1 5
/MEMORY/Net 94 "D14"
 U8 51
 U1 4
/MEMORY/Net 95 "D13"
 U8 50
 U1 3
/MEMORY/Net 96 "D12"
 U8 48
 U1 11
/MEMORY/Net 97 "D11"
 U8 47
 U1 6
/MEMORY/Net 98 "D10"
 U8 45
 U1 51
/MEMORY/Net 99 "D9"
 U8 44
 U1 50
/MEMORY/Net 100 "D8"
 U8 42
 U1 47
/MEMORY/Net 101 "MCKO"
 U8 38
 R20 1
/MEMORY/Net 102 "CKE"
 U8 37
 U1 26
/MEMORY/Net 103 "A14"
 U8 21
 U1 40
/MEMORY/Net 104 "A13"
 U8 20
 U1 39
/MEMORY/Net 105 "DCS0_N"
 U8 19
 U1 17
/MEMORY/Net 106 "RAS_N"
 U8 18
 U1 18
/MEMORY/Net 107 "CAS_N"
 U8 17
 U1 19
/MEMORY/Net 108 "MRDWR_N"
 U8 16
 R21 1
/MEMORY/Net 109 "WE0_N"
 U8 15
 U1 23
/MEMORY/Net 110 "WE1_N"
 U8 39
 U1 24
/MEMORY/Net 111 "A12"
 U8 36
 U1 27
/MEMORY/Net 112 "A11"
 U8 35
 U1 28
/MEMORY/Net 113 "A10"
 U8 22
 U1 16
/MEMORY/Net 114 "A9"
 U8 34
 U1 31
/MEMORY/Net 115 "A8"
 U8 33
 U1 32
/MEMORY/Net 116 "A7"
 U8 32
 U1 35
/MEMORY/Net 117 "A6"
 U8 31
 U1 36
/MEMORY/Net 118 "A5"
 U8 30
 U1 37
/MEMORY/Net 119 "A4"
 U8 29
 U1 38
/MEMORY/Net 120 "A3"
 U8 26
 U1 12
/MEMORY/Net 121 "A2"
 U8 25
 U1 13
/MEMORY/Net 122 "A1"
 U8 24
 U1 14
/MEMORY/Net 123 "A0"
 U8 23
 U1 15
/MEMORY/Net 124 "RDWR_N"
 R21 2
 U1 20
/MEMORY/Net 125 "GPB30"
 TP25 1
 U1 60
/MEMORY/Net 126 "GPB18"
 TP23 1
 U1 157
Net 127 ""
 U1 159
 CON2 21
Net 128 ""
 U1 160
 CON2 22
Net 129 ""
 U1 56
 Q5 3
 R34 2
/MEMORY/Net 130 "BUZPWM"
 BUZ+1 1
 U1 57
/MEMORY/Net 131 "CKO"
 R20 2
 U1 25
Net 132 ""
 Q4 1
 U1 154
Net 133 ""
 R29 1
 R28 1
 R27 1
 R24 1
 R23 1
 J1 4
 Q4 3
 C46 1
 C45 1
Net 134 ""
 J1 5
 U1 82
Net 135 ""
 R28 2
 J1 2
 U1 78
Net 136 ""
 R24 2
 J1 7
 U1 81
/MEMORY/Net 137 "FWE_N"
 U9 18
 U1 64
/MEMORY/Net 138 "FALE/GPB16"
 U9 17
 U1 58
/MEMORY/Net 139 "FCLE/GPB15"
 U9 16
 U1 59
/MEMORY/Net 140 "D7"
 U9 44
 U8 13
 U1 46
/MEMORY/Net 141 "D6"
 U9 43
 U8 11
 U1 43
/MEMORY/Net 142 "D5"
 U9 42
 U8 10
 U1 42
/MEMORY/Net 143 "D4"
 U9 41
 U8 8
 U1 41
/MEMORY/Net 144 "D3"
 U9 32
 U8 7
 U1 55
/MEMORY/Net 145 "D2"
 U9 31
 U8 5
 U1 54
/MEMORY/Net 146 "D1"
 U9 30
 U8 4
 U1 53
/MEMORY/Net 147 "D0"
 U9 29
 U8 2
 U1 52
Net 148 ""
 U1 158
 U12 3
/MEMORY/Net 153 "WP_N"
 R30 1
 U9 19
/MEMORY/Net 154 "FRB_N"
 R22 1
 U9 7
 U9 6
 U1 68
/LCD_USB/Net 179 "HOST_DP1"
 U13 1
 U1 106
/LCD_USB/Net 180 "HOST_DM1"
 U13 3
 U1 107
Net 181 ""
 U13 4
 J4 2
Net 182 ""
 Q5 1
 R35 1
 R33 2
Net 183 ""
 D6 1
 L4 2
 U12 2
Net 186 ""
 R48 1
 R49 2
 U1 93
Net 187 ""
 R50 1
 U12 5
Net 188 ""
 U13 5
 J4 3
Net 189 ""
 D5 2
 J4 1
Net 190 ""
 BD10 1
 J4 5
Net 191 ""
 R43 1
 C71 2
 J4 9
 J4 8
 J4 7
 J4 6
/LCD_USB/Net 192 "GPC8"
 U11 6
 TP35 1
 U1 175
/LCD_USB/Net 193 "LCDD0"
 BN2 5
 U1 1
/LCD_USB/Net 194 "LCDD1"
 BN2 6
 U1 186
/LCD_USB/Net 195 "LCDD2"
 BN2 7
 U1 183
/LCD_USB/Net 196 "LCDD3"
 BN2 8
 U1 182
/LCD_USB/Net 197 "LCDD4"
 BN1 5
 U1 179
/LCD_USB/Net 198 "LCDD5"
 BN1 6
 U1 178
/LCD_USB/Net 199 "LCDD6"
 BN1 7
 U1 177
/LCD_USB/Net 200 "LCDD7"
 BN1 8
 U1 176
/LCD_USB/Net 201 "VSYNC"
 CON2 18
 U1 161
/LCD_USB/Net 202 "DCLK"
 BD4 1
 U1 2
Net 203 ""
 BD6 1
 J2 1
Net 204 ""
 BD7 1
 J2 5
 J2 4
/LCD_USB/Net 205 "DN"
 L3 3
 U1 114
 U1 113
Net 206 ""
 L3 4
 J2 2
Net 207 ""
 C58 2
 J2 9
 J2 8
 J2 7
 J2 6
Net 208 ""
 C54 1
 U1 109
/LCD_USB/Net 209 "GPD15"
 TP38 1
 U1 156
Net 210 ""
 R32 2
 U1 110
Net 211 ""
 L3 1
 J2 3
/LCD_USB/Net 212 "DP"
 L3 2
 U1 116
 U1 115
/LCD_USB/Net 213 "LCDCS"
 CON2 20
 U1 163
/LCD_USB/Net 214 "HSYNC"
 CON2 19
 U1 162
Net 215 ""
 C70 1
 R47 2
 U11 2
/LCD_USB/Net 216 "GPC9"
 U11 5
 TP36 1
 U1 174
Net 217 ""
 Q11 3
 D5 1
/LCD_USB/Net 220 "VHOST"
 D6 2
 C72 2
 U12 1
 R45 2
 Q11 2
/LCD_USB/Net 223 "LCDDCLK"
 BD4 2
 CON2 17
/LCD_USB/Net 224 "LCD0"
 BN2 4
 CON2 16
/LCD_USB/Net 225 "LCD1"
 BN2 3
 CON2 15
/LCD_USB/Net 226 "LCD2"
 BN2 2
 CON2 14
/LCD_USB/Net 227 "LCD3"
 BN2 1
 CON2 13
/LCD_USB/Net 228 "LCD4"
 BN1 4
 CON2 12
/LCD_USB/Net 229 "LCD5"
 BN1 3
 CON2 11
/LCD_USB/Net 230 "LCD6"
 BN1 2
 CON2 10
/LCD_USB/Net 231 "LCD7"
 BN1 1
 CON2 9
/LCD_USB/Net 232 "BATIN"
 R31 2
 U1 92
/LCD_USB/Net 233 "VREF"
 C53 1
 C52 1
 U1 140
}
#End
