#
# $Id: f256 897 2007-12-29 13:02:32Z arniml $
#
# JTAG package script for EP2C8F256
#
# This program is free software; you can redistribute it and/or
# modify it under the terms of the GNU General Public License
# as published by the Free Software Foundation; either version 2
# of the License, or (at your option) any later version.
#
# This program is distributed in the hope that it will be useful,
# but WITHOUT ANY WARRANTY; without even the implied warranty of
# MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
# GNU General Public License for more details.
#
# You should have received a copy of the GNU General Public License
# along with this program; if not, write to the Free Software
# Foundation, Inc., 59 Temple Place - Suite 330, Boston, MA
# 02111-1307, USA.
#
# Written by H Hartley Sweeten <hsweeten@visionengravers.com>
#
# Note:
#   The signals defined in this file as unused pad are specified as
#   I/O pins in the main configuration file ep2c8.
#

salias	IOC3	BSC198	# Note: this pin is specified as I/O. If AS mode is specified by MSEL it is output only (ASDO)
salias	IOF4	BSC197	# Note: this pin is specified as I/O. If AS mode is specified by MSEL it is output only (nCSO)
salias	IOC1	BSC196
salias	IOC2	BSC195
salias	IOD5	BSC194
salias	IOE5	BSC193
salias	IOF5	BSC192
#		BSC191	# unused pad
salias	IOD3	BSC190
salias	IOD4	BSC189
salias	IOF3	BSC188
salias	IOD2	BSC187
salias	IOD1	BSC186
salias	IOE3	BSC185
salias	IOE4	BSC184
salias	IOG4	BSC183
salias	IOJ6	BSC182
salias	IOH6	BSC181
salias	IOE1	BSC180
salias	IOE2	BSC179
salias	DATA0	BSC178	# Family-specific input pin F1
salias	DCLK	BSC177	# Family-specific input pin H4
#	nCE	BSC176	# untestable Family-specific pin G5
salias	CLK0	BSC175	# Family-specific input pin H2
salias	CLK1	BSC174	# Family-specific input pin H1
#	nCONFIG	BSC173	# untestable Family-specific pin J5
salias	CLK2	BSC172	# Family-specific input pin J2
salias	CLK3	BSC171	# Family-specific input pin J1
salias	IOK2	BSC170
salias	IOK1	BSC169
salias	IOK4	BSC168
salias	IOK5	BSC167
#		BSC166	# unused pad
salias	IOL1	BSC165
salias	IOL2	BSC164
salias	IOJ4	BSC163
salias	IOM1	BSC162
salias	IOM2	BSC161
salias	IOM3	BSC160
salias	IOL3	BSC159
salias	ION1	BSC158
salias	ION2	BSC157
salias	IOP1	BSC156
salias	IOP2	BSC155
#		BSC154	# unused pad
salias	ION3	BSC153
salias	ION4	BSC152
salias	IOP3	BSC151
salias	IOL4	BSC150
salias	IOM4	BSC149
salias	IOR3	BSC148
salias	IOT3	BSC147
salias	IOP5	BSC146
salias	IOP4	BSC145
salias	IOT4	BSC144
salias	IOR4	BSC143
salias	IOT5	BSC142
salias	IOR5	BSC141
salias	ION7	BSC140
salias	IOK7	BSC139
salias	IOK6	BSC138
salias	IOT6	BSC137
salias	IOR6	BSC136
salias	IOP6	BSC135
salias	ION6	BSC134
salias	ION8	BSC133
salias	IOT7	BSC132
salias	IOR7	BSC131
salias	IOL7	BSC130
salias	IOL8	BSC129
salias	IOT8	BSC128
salias	IOR8	BSC127
salias	IOT9	BSC126
salias	IOR9	BSC125
salias	ION9	BSC124
salias	ION10	BSC123
salias	IOT11	BSC122
salias	IOR11	BSC121
salias	IOP11	BSC120
salias	IOL9	BSC119
salias	IOL10	BSC118
salias	IOR10	BSC117
salias	IOT10	BSC116
salias	IOK11	BSC115
salias	IOK10	BSC114
salias	ION11	BSC113
salias	IOP12	BSC112
salias	IOP13	BSC111
salias	IOT12	BSC110
salias	IOR12	BSC109
#		BSC108	# unused pad
salias	IOT13	BSC107
salias	IOR13	BSC106
salias	IOT14	BSC105
salias	IOR14	BSC104
salias	IOM11	BSC103
salias	IOL11	BSC102
salias	ION12	BSC101
salias	IOM12	BSC100
salias	IOL12	BSC099
salias	IOK13	BSC098
salias	ION13	BSC097
salias	ION14	BSC096
salias	IOP15	BSC095
salias	IOP16	BSC094
salias	ION15	BSC093
salias	ION16	BSC092
salias	IOP14	BSC091
#		BSC090	# unused pad
#		BSC089	# unused pad
salias	IOM14	BSC088
salias	IOM15	BSC087
salias	IOM16	BSC086
#		BSC085	# unused pad
salias	IOL14	BSC084
salias	IOL15	BSC083
salias	IOL16	BSC082
#	nSTATUS	BSC081	# untestable Family-specific pin M13
#	CONF_DONE	BSC080	# untestable Family-specific pin L13
salias	MSEL1	BSC079	# Family-specific input pin K12
salias	MSEL0	BSC078	# Family-specific input pin J13
salias	IOK16	BSC077
salias	IOK15	BSC076
salias	CLK7	BSC075	# Family-specific input pin J16
salias	CLK6	BSC074	# Family-specific input pin J15
salias	CLK5	BSC073	# Family-specific input pin H15
salias	CLK4	BSC072	# Family-specific input pin H16
salias	IOH12	BSC071
salias	IOJ12	BSC070
salias	IOG16	BSC069
salias	IOG15	BSC068
salias	IOF15	BSC067
salias	IOF16	BSC066
salias	IOJ11	BSC065
salias	IOH11	BSC064
salias	IOG12	BSC063
salias	IOG13	BSC062
salias	IOE13	BSC061
salias	IOF13	BSC060
salias	IOH13	BSC059
salias	IOD15	BSC058
salias	IOD16	BSC057
salias	IOE15	BSC056
salias	IOE16	BSC055
salias	IOF14	BSC054
salias	IOC15	BSC053
salias	IOC16	BSC052
salias	IOC14	BSC051
salias	IOD13	BSC050
salias	IOE14	BSC049
salias	IOD14	BSC048
salias	IOB14	BSC047
salias	IOA14	BSC046
salias	IOC13	BSC045
salias	IOC12	BSC044
salias	IOB13	BSC043
salias	IOA13	BSC042
salias	IOB12	BSC041
salias	IOA12	BSC040
salias	IOC11	BSC039
salias	IOB11	BSC038
salias	IOA11	BSC037
salias	IOG10	BSC036
salias	IOG11	BSC035
salias	IOB10	BSC034
salias	IOA10	BSC033
salias	IOF10	BSC032
salias	IOF9	BSC031
salias	IOD9	BSC030
salias	IOD11	BSC029
salias	IOD10	BSC028
salias	IOA9	BSC027
salias	IOB9	BSC026
salias	IOA8	BSC025
salias	IOB8	BSC024
salias	IOA7	BSC023
salias	IOB7	BSC022
salias	IOF7	BSC021
salias	IOF8	BSC020
#		BSC019	# unused pad
#		BSC018	# unused pad
salias	IOD8	BSC017
salias	IOB6	BSC016
salias	IOA6	BSC015
salias	IOG6	BSC014
salias	IOG7	BSC013
salias	IOD7	BSC012
salias	IOD6	BSC011
salias	IOC6	BSC010
salias	IOC5	BSC009
salias	IOC4	BSC008
salias	IOB5	BSC007
salias	IOA5	BSC006
salias	IOB4	BSC005
salias	IOA4	BSC004
salias	IOA3	BSC003
salias	IOB3	BSC002
salias	IOE6	BSC001
salias	IOF6	BSC000
