#
# $Id: t144 897 2007-12-29 13:02:32Z arniml $
#
# JTAG package script for EP2C8T144
#
# This program is free software; you can redistribute it and/or
# modify it under the terms of the GNU General Public License
# as published by the Free Software Foundation; either version 2
# of the License, or (at your option) any later version.
#
# This program is distributed in the hope that it will be useful,
# but WITHOUT ANY WARRANTY; without even the implied warranty of
# MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
# GNU General Public License for more details.
#
# You should have received a copy of the GNU General Public License
# along with this program; if not, write to the Free Software
# Foundation, Inc., 59 Temple Place - Suite 330, Boston, MA
# 02111-1307, USA.
#
# Written by H Hartley Sweeten <hsweeten@visionengravers.com>
#
# Note:
#   The signals defined in this file as unused pad are specified as
#   I/O pins in the main configuration file ep2c8.
#

salias	IO1	BSC198	# Note: this pin is specified as I/O. If AS mode is specified by MSEL it is output only (ASDO)
salias	IO2	BSC197	# Note: this pin is specified as I/O. If AS mode is specified by MSEL it is output only (nCSO)
salias	IO3	BSC196
salias	IO4	BSC195
#		BSC194	# unused pad
#		BSC193	# unused pad
#		BSC192	# unused pad
#		BSC191	# unused pad
#		BSC190	# unused pad
#		BSC189	# unused pad
salias	IO7	BSC188
#		BSC187	# unused pad
#		BSC186	# unused pad
#		BSC185	# unused pad
#		BSC184	# unused pad
#		BSC183	# unused pad
#		BSC182	# unused pad
#		BSC181	# unused pad
salias	IO8	BSC180
salias	IO9	BSC179
salias	DATA0	BSC178	# Family-specific input pin 14
salias	DCLK	BSC177	# Family-specific input pin 15
#	nCE	BSC176	# untestable Family-specific pin 16
salias	CLK0	BSC175	# Family-specific input pin 17
salias	CLK1	BSC174	# Family-specific input pin 18
#	nCONFIG	BSC173	# untestable Family-specific pin 20
salias	CLK2	BSC172	# Family-specific input pin 21
salias	CLK3	BSC171	# Family-specific input pin 22
salias	IO24	BSC170
salias	IO25	BSC169
#		BSC168	# unused pad
#		BSC167	# unused pad
#		BSC166	# unused pad
#		BSC165	# unused pad
#		BSC164	# unused pad
salias	IO28	BSC163
#		BSC162	# unused pad
#		BSC161	# unused pad
#		BSC160	# unused pad
#		BSC159	# unused pad
#		BSC158	# unused pad
#		BSC157	# unused pad
#		BSC156	# unused pad
#		BSC155	# unused pad
#		BSC154	# unused pad
#		BSC153	# unused pad
#		BSC152	# unused pad
salias	IO30	BSC151
salias	IO31	BSC150
salias	IO32	BSC149
salias	IO40	BSC148
salias	IO41	BSC147
salias	IO42	BSC146
salias	IO43	BSC145
salias	IO44	BSC144
salias	IO45	BSC143
salias	IO47	BSC142
salias	IO48	BSC141
#		BSC140	# unused pad
#		BSC139	# unused pad
#		BSC138	# unused pad
#		BSC137	# unused pad
#		BSC136	# unused pad
#		BSC135	# unused pad
#		BSC134	# unused pad
salias	IO51	BSC133
salias	IO52	BSC132
#		BSC131	# unused pad
#		BSC130	# unused pad
#		BSC129	# unused pad
salias	IO53	BSC128
salias	IO55	BSC127
salias	IO57	BSC126
salias	IO58	BSC125
salias	IO59	BSC124
salias	IO60	BSC123
#		BSC122	# unused pad
#		BSC121	# unused pad
#		BSC120	# unused pad
#		BSC119	# unused pad
#		BSC118	# unused pad
#		BSC117	# unused pad
#		BSC116	# unused pad
#		BSC115	# unused pad
#		BSC114	# unused pad
salias	IO63	BSC113
#		BSC112	# unused pad
#		BSC111	# unused pad
salias	IO64	BSC110
salias	IO65	BSC109
#		BSC108	# unused pad
#		BSC107	# unused pad
salias	IO67	BSC106
salias	IO69	BSC105
salias	IO70	BSC104
salias	IO71	BSC103
salias	IO72	BSC102
salias	IO73	BSC101
salias	IO74	BSC100
#		BSC099	# unused pad
#		BSC098	# unused pad
salias	IO75	BSC097
salias	IO76	BSC096
#		BSC095	# unused pad
#		BSC094	# unused pad
#		BSC093	# unused pad
#		BSC092	# unused pad
#		BSC091	# unused pad
#		BSC090	# unused pad
#		BSC089	# unused pad
salias	IO79	BSC088
#		BSC087	# unused pad
#		BSC086	# unused pad
#		BSC085	# unused pad
#		BSC084	# unused pad
#		BSC083	# unused pad
#		BSC082	# unused pad
#	nSTATUS	BSC081	# untestable Family-specific pin 82
#	CONF_DONE	BSC080	# untestable Family-specific pin 83
salias	MSEL1	BSC079	# Family-specific input pin 84
salias	MSEL0	BSC078	# Family-specific input pin 85
salias	IO86	BSC077
salias	IO87	BSC076
salias	CLK7	BSC075	# Family-specific input pin 88
salias	CLK6	BSC074	# Family-specific input pin 89
salias	CLK5	BSC073	# Family-specific input pin 90
salias	CLK4	BSC072	# Family-specific input pin 91
salias	IO92	BSC071
salias	IO93	BSC070
salias	IO94	BSC069
salias	IO96	BSC068
salias	IO97	BSC067
#		BSC066	# unused pad
#		BSC065	# unused pad
#		BSC064	# unused pad
#		BSC063	# unused pad
#		BSC062	# unused pad
#		BSC061	# unused pad
#		BSC060	# unused pad
salias	IO99	BSC059
#		BSC058	# unused pad
#		BSC057	# unused pad
#		BSC056	# unused pad
#		BSC055	# unused pad
#		BSC054	# unused pad
salias	IO100	BSC053
salias	IO101	BSC052
#		BSC051	# unused pad
#		BSC050	# unused pad
salias	IO103	BSC049
salias	IO104	BSC048
salias	IO112	BSC047
salias	IO113	BSC046
salias	IO114	BSC045
salias	IO115	BSC044
#		BSC043	# unused pad
#		BSC042	# unused pad
salias	IO118	BSC041
salias	IO119	BSC040
salias	IO120	BSC039
salias	IO121	BSC038
salias	IO122	BSC037
#		BSC036	# unused pad
#		BSC035	# unused pad
#		BSC034	# unused pad
#		BSC033	# unused pad
#		BSC032	# unused pad
#		BSC031	# unused pad
#		BSC030	# unused pad
salias	IO125	BSC029
salias	IO126	BSC028
#		BSC027	# unused pad
#		BSC026	# unused pad
#		BSC025	# unused pad
#		BSC024	# unused pad
#		BSC023	# unused pad
salias	IO129	BSC022
#		BSC021	# unused pad
#		BSC020	# unused pad
#		BSC019	# unused pad
#		BSC018	# unused pad
salias	IO132	BSC017
salias	IO133	BSC016
salias	IO134	BSC015
#		BSC014	# unused pad
#		BSC013	# unused pad
#		BSC012	# unused pad
#		BSC011	# unused pad
#		BSC010	# unused pad
#		BSC009	# unused pad
#		BSC008	# unused pad
salias	IO135	BSC007
salias	IO136	BSC006
salias	IO137	BSC005
salias	IO139	BSC004
salias	IO141	BSC003
salias	IO142	BSC002
salias	IO143	BSC001
salias	IO144	BSC000
