#!/bin/sh /etc/rc.common
START=90
# place your own startup commands here
#
# REMEMBER: You *MUST* place an '&' after launching programs you 
#   that are to continue running in the background.
#
#   i.e. 
#   BAD:  upnpd
#   GOOD: upnpd &
# 
# Failure to do this will result in the startup process halting
# on this file and the diagnostic light remaining on (at least
# for WRT54G(s) models).
#

# coldplug USB devices
udevtrigger &

# wait for coldplug and re-generate wireless config
#wifi detect > /etc/config/wireless &

