From 357761c423c0f9e4af4aafe85be7889dc36f3584 Mon Sep 17 00:00:00 2001
From: Florian Fainelli <florian@openwrt.org>
Date: Tue, 31 Jan 2012 15:12:23 +0100
Subject: [PATCH 4/6] MIPS: BCM63XX: add RNG peripheral definitions

Signed-off-by: Florian Fainelli <florian@openwrt.org>
Cc: linux-mips@linux-mips.org
Cc: mpm@selenic.com
Cc: herbert@gondor.apana.org.au
Patchwork: https://patchwork.linux-mips.org/patch/3326/
Signed-off-by: Ralf Baechle <ralf@linux-mips.org>
---
 arch/mips/include/asm/mach-bcm63xx/bcm63xx_cpu.h  |    9 +++++++++
 arch/mips/include/asm/mach-bcm63xx/bcm63xx_regs.h |   14 ++++++++++++++
 2 files changed, 23 insertions(+), 0 deletions(-)

--- a/arch/mips/include/asm/mach-bcm63xx/bcm63xx_cpu.h
+++ b/arch/mips/include/asm/mach-bcm63xx/bcm63xx_cpu.h
@@ -129,6 +129,7 @@ enum bcm63xx_regs_set {
 	RSET_PCMDMA,
 	RSET_PCMDMAC,
 	RSET_PCMDMAS,
+	RSET_RNG
 };
 
 #define RSET_DSL_LMEM_SIZE		(64 * 1024 * 4)
@@ -152,6 +153,7 @@ enum bcm63xx_regs_set {
 #define RSET_XTMDMA_SIZE		256
 #define RSET_XTMDMAC_SIZE(chans)	(16 * (chans))
 #define RSET_XTMDMAS_SIZE(chans)	(16 * (chans))
+#define RSET_RNG_SIZE			20
 
 /*
  * 6338 register sets base address
@@ -195,6 +197,7 @@ enum bcm63xx_regs_set {
 #define BCM_6338_PCMDMA_BASE		(0xdeadbeef)
 #define BCM_6338_PCMDMAC_BASE		(0xdeadbeef)
 #define BCM_6338_PCMDMAS_BASE		(0xdeadbeef)
+#define BCM_6338_RNG_BASE		(0xdeadbeef)
 
 /*
  * 6345 register sets base address
@@ -238,6 +241,7 @@ enum bcm63xx_regs_set {
 #define BCM_6345_PCMDMA_BASE		(0xdeadbeef)
 #define BCM_6345_PCMDMAC_BASE		(0xdeadbeef)
 #define BCM_6345_PCMDMAS_BASE		(0xdeadbeef)
+#define BCM_6345_RNG_BASE		(0xdeadbeef)
 
 /*
  * 6348 register sets base address
@@ -278,6 +282,7 @@ enum bcm63xx_regs_set {
 #define BCM_6348_PCMDMA_BASE		(0xdeadbeef)
 #define BCM_6348_PCMDMAC_BASE		(0xdeadbeef)
 #define BCM_6348_PCMDMAS_BASE		(0xdeadbeef)
+#define BCM_6348_RNG_BASE		(0xdeadbeef)
 
 /*
  * 6358 register sets base address
@@ -318,6 +323,7 @@ enum bcm63xx_regs_set {
 #define BCM_6358_PCMDMA_BASE		(0xfffe1800)
 #define BCM_6358_PCMDMAC_BASE		(0xfffe1900)
 #define BCM_6358_PCMDMAS_BASE		(0xfffe1a00)
+#define BCM_6358_RNG_BASE		(0xdeadbeef)
 
 
 /*
@@ -359,6 +365,7 @@ enum bcm63xx_regs_set {
 #define BCM_6368_PCMDMA_BASE		(0xb0005800)
 #define BCM_6368_PCMDMAC_BASE		(0xb0005a00)
 #define BCM_6368_PCMDMAS_BASE		(0xb0005c00)
+#define BCM_6368_RNG_BASE		(0xb0004180)
 
 
 extern const unsigned long *bcm63xx_regs_base;
@@ -404,6 +411,7 @@ extern const unsigned long *bcm63xx_regs
 	__GEN_RSET_BASE(__cpu, PCMDMA)					\
 	__GEN_RSET_BASE(__cpu, PCMDMAC)					\
 	__GEN_RSET_BASE(__cpu, PCMDMAS)					\
+	__GEN_RSET_BASE(__cpu, RNG)					\
 	}
 
 #define __GEN_CPU_REGS_TABLE(__cpu)					\
@@ -442,6 +450,7 @@ extern const unsigned long *bcm63xx_regs
 	[RSET_PCMDMA]		= BCM_## __cpu ##_PCMDMA_BASE,		\
 	[RSET_PCMDMAC]		= BCM_## __cpu ##_PCMDMAC_BASE,		\
 	[RSET_PCMDMAS]		= BCM_## __cpu ##_PCMDMAS_BASE,		\
+	[RSET_RNG]		= BCM_## __cpu ##_RNG_BASE,		\
 
 
 static inline unsigned long bcm63xx_regset_address(enum bcm63xx_regs_set set)
--- a/arch/mips/include/asm/mach-bcm63xx/bcm63xx_regs.h
+++ b/arch/mips/include/asm/mach-bcm63xx/bcm63xx_regs.h
@@ -974,6 +974,20 @@
 #define M2M_DSTID_REG(x)		((x) * 0x40 + 0x18)
 
 /*************************************************************************
+ * _REG relative to RSET_RNG
+ *************************************************************************/
+
+#define RNG_CTRL			0x00
+#define RNG_EN				(1 << 0)
+
+#define RNG_STAT			0x04
+#define RNG_AVAIL_MASK			(0xff000000)
+
+#define RNG_DATA			0x08
+#define RNG_THRES			0x0c
+#define RNG_MASK			0x10
+
+/*************************************************************************
  * _REG relative to RSET_SPI
  *************************************************************************/
 
