From b100a50c3bf7884a97d5008fc79d9b45f3b6e999 Mon Sep 17 00:00:00 2001
From: Kurt Mahan <kmahan@freescale.com>
Date: Fri, 30 Nov 2007 12:55:12 -0700
Subject: [PATCH] Fix bitfield definitions.

LTIBName: m5445x-ccm-bitdefs
Signed-off-by: Kurt Mahan <kmahan@freescale.com>
---
 include/asm-m68k/mcf5445x_ccm.h |   34 ++++++++++++++++++----------------
 1 files changed, 18 insertions(+), 16 deletions(-)

--- a/include/asm-m68k/mcf5445x_ccm.h
+++ b/include/asm-m68k/mcf5445x_ccm.h
@@ -118,22 +118,24 @@
 #define MCF_CCM_MISCCR_BMT(x)           (((x) & 0x0007) << 8)	/* Bus monitor timing field */
 #define MCF_CCM_MISCCR_BME              (0x0800)	/* Bus monitor external enable bit */
 #define MCF_CCM_MISCCR_LIMP             (0x1000)	/* Limp mode enable */
-#define MCF_CCM_MISCCR_BMT_65536        (0)
-#define MCF_CCM_MISCCR_BMT_32768        (1)
-#define MCF_CCM_MISCCR_BMT_16384        (2)
-#define MCF_CCM_MISCCR_BMT_8192         (3)
-#define MCF_CCM_MISCCR_BMT_4096         (4)
-#define MCF_CCM_MISCCR_BMT_2048         (5)
-#define MCF_CCM_MISCCR_BMT_1024         (6)
-#define MCF_CCM_MISCCR_BMT_512          (7)
-#define MCF_CCM_MISCCR_SSIPUS_UP        (1)
-#define MCF_CCM_MISCCR_SSIPUS_DOWN      (0)
-#define MCF_CCM_MISCCR_TIMDMA_TIM       (1)
-#define MCF_CCM_MISCCR_TIMDMA_SSI       (0)
-#define MCF_CCM_MISCCR_SSISRC_CLKIN     (0)
-#define MCF_CCM_MISCCR_SSISRC_PLL       (1)
-#define MCF_CCM_MISCCR_USBOC_ACTHI      (0)
-#define MCF_CCM_MISCCR_USBOV_ACTLO      (1)
+#define MCF_CCM_MISCCR_BMT_65536        (0 << 8)
+#define MCF_CCM_MISCCR_BMT_32768        (1 << 8)
+#define MCF_CCM_MISCCR_BMT_16384        (2 << 8)
+#define MCF_CCM_MISCCR_BMT_8192         (3 << 8)
+#define MCF_CCM_MISCCR_BMT_4096         (4 << 8)
+#define MCF_CCM_MISCCR_BMT_2048         (5 << 8)
+#define MCF_CCM_MISCCR_BMT_1024         (6 << 8)
+#define MCF_CCM_MISCCR_BMT_512          (7 << 8)
+#define MCF_CCM_MISCCR_SSIPUE_UP        (1 << 7)
+#define MCF_CCM_MISCCR_SSIPUE_DOWN      (0 << 7)
+#define MCF_CCM_MISCCR_SSIPUS_UP        (1 << 6)
+#define MCF_CCM_MISCCR_SSIPUS_DOWN      (0 << 6)
+#define MCF_CCM_MISCCR_TIMDMA_TIM       (1 << 5)
+#define MCF_CCM_MISCCR_TIMDMA_SSI       (0 << 5)
+#define MCF_CCM_MISCCR_SSISRC_CLKIN     (0 << 4)
+#define MCF_CCM_MISCCR_SSISRC_PLL       (1 << 4)
+#define MCF_CCM_MISCCR_USBOC_ACTHI      (0 << 1)
+#define MCF_CCM_MISCCR_USBOC_ACTLO      (1 << 1)
 #define MCF_CCM_MISCCR_USBSRC_CLKIN     (0)
 #define MCF_CCM_MISCCR_USBSRC_PLL       (1)
 
