This file is replaced by a cleaner version with the adding of a MFD driver for
the southbridge.

Signed-off-by: Florian Fainelli <florian@openwrt.org>
---
--- a/arch/x86/include/asm/rdc321x_defs.h
+++ /dev/null
@@ -1,12 +0,0 @@
-#define PFX	"rdc321x: "
-
-/* General purpose configuration and data registers */
-#define RDC3210_CFGREG_ADDR     0x0CF8
-#define RDC3210_CFGREG_DATA     0x0CFC
-
-#define RDC321X_GPIO_CTRL_REG1	0x48
-#define RDC321X_GPIO_CTRL_REG2	0x84
-#define RDC321X_GPIO_DATA_REG1	0x4c
-#define RDC321X_GPIO_DATA_REG2	0x88
-
-#define RDC321X_MAX_GPIO	58
