--- Fri 2011-12-16 ------------------------------------------------------------

reflash_m1.sh --release 2011-07-13
wget http://milkymist.org/updates/2011-07-13/for-rc3/boot.4e53273.bin
flterm --port /dev/ttyUSB0 --kernel boot.4e53273.bin

Check image CRCs: all but bios-rescue.bin pass. (bios-rescue has the
MAC issue.)

Configured to 1024x768, US keyboard, Ethernet off, performance mode,
only the "Tunnel" to patch.

10:29 test run starts (2/d9/, using 2/aloop)

--- Sat 2011-12-17 ------------------------------------------------------------

12:33 interrupted after completing cycle 5000
      dumplock: all locks read zero ("unlocked")
      CRC check: no anomalies

12:34 started test run (2/d10/)

--- Sun 2011-12-18 ------------------------------------------------------------

14:39 interrupted after completing cycle 5002
      dumplock: all locks read zero ("unlocked")
      CRC check: no anomalies
      standby partition bytewise comparison: only difference at the end

14:44 started test run (2/d11/)

--- Mon 2011-12-19 ------------------------------------------------------------

11:42 stopped after completing cycle 4019
      dumplock: all locks read zero ("unlocked")
      CRC check: no anomalies
      standby partition bytewise comparison: only difference at the end

If we assume that occurrence of NOR corruption follows an exponential
distribution with lambda = 1/700, then such corruption would have
been observed in the above 14002 cycles with a probability of
1-exp(-1/700*(5000+5002+4019)) = 99.9999998%.
